| FRDM-KW40Z Demo Software Reference Manual Rev 0.0 NXP Semiconductors |

API Reference
Here is a list of all modules:
[detail level 1 2 3]

Buzzer | Buzzer module implements functions to control a DC buzzer using PWM
▼e-Compass | E-Compass module combines accelerometer and magnetometer readings to determine the magnetic north position relative to the board orientation
e-Compass Driver | E-Compass Driver implements the functions to calculate the compass heading based on the accelerometer and magnetometer data
▼Accelerometer |
▼FXOS8700CQ | The FXOS8700CQ module implements the functions to initialize, configure, and read the FXOS8700CQ accelerometer + magnetometer sensor from NXP
FXOS8700CQ Registers | This module defines all the registers present in the FXOS8700CQ sensor
▼IR Controller |
IR Controller Parameters | This module includes the definition of time parameters and command codes for different TVs
IR Controller Driver | This module implements the APIs to initialize the IR controller driver and send IR commands
LED Control | This module provides the functions to control the FRDM-KW40Z board LED functionality
Potentiometer | Potentiometer module implements functions to obtain the relative position in a scale from 0% to 100%
Temperature Sensor | Temperature sensor module implements functions to obtain the internal chip temperature of the SoC by reading the temperature sensor ADC channel
▼Input Report | Input Report implements functions to acquire users input when a button is pressed (GPIO) or a capacitive sensor is touched (TSI)
TSI Sensor | TSI Sensor implements functions to detect touch events in capacitive pads