| FRDM-KW40Z Demo Software Reference Manual Rev 0.0 NXP Semiconductors |

Data Structures | Variables
IR Controller Parameters
IR Controller

## Overview

This module includes the definition of time parameters and command codes for different TVs.

## Data Structures
struct | controller_parameter_list_t

## Variables
controller_parameter_list_t | controllerParameterList [3]

## Data Structure Documentation

struct controller_parameter_list_t

TV Controller parameter structure.

Data Fields
ir_controller_parameters_t | controllerTimingParameters | Timing parameters (see ir_controller_parameters_t).
uint32_t | controllerCommands[6] | Controller command codes for these functions: On/Off Mute Volume + Volume - Channel + Channel - Note The command codes must be left-aligned
uint8_t | bitsPerCommand | Size of the command in bytes (see controller specification)
uint8_t | commandRepeatTimes | Number of times a command must be repeated to be valid (see controller specification)

## Variable Documentation

controller_parameter_list_t controllerParameterList[3]

List of controller parameters of type controller_parameter_list_t supported in this driver.