<?xml version="1.0" encoding="UTF-8"?>
<PE_PROJECT_SETTINGS_DOCUMENTATION>
  <PE_product_version v="version 5.3 for Freescale Microcontrollers" />
  <PE_core_version v="Processor Expert Version 0501" />
  <CPU_Bean name="Cpu" type="MC56F84789VLL">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="Cpu" />
      <CPU_type v="MC56F84789VLL" />
      <list name="Clock settings (included)" v="1">
        <group name="Clock settings">
          <group name="Internal oscillator">
            <boolgroup name="Internal 32kHz relaxation oscillator (ROSC_32K)" v="Disabled" />
            <boolgroup name="Internal 8MHz relaxation oscillator (ROSC_8M)" v="Enabled">
              <Fast_internal_reference_clock__MHz_ v="8" />
              <boolgroup name="Initialize frequency trim" v="yes">
                <Frequency_trim_value_address v="58412" />
              </boolgroup>
              <boolgroup name="Initialize temperature trim" v="no" />
            </boolgroup>
          </group>
          <boolgroup name="External reference clock" v="Disabled" />
          <group name="Clock protection">
            <Frequency v="Off" />
            <Oscillator v="Off" />
            <Phase_locked_loop v="Off" />
          </group>
        </group>
      </list>
      <list name="Common settings (included)" v="1">
        <group name="Common settings">
          <Initialization_priority v="minimal priority" />
          <Watchdog v="Disabled" />
          <Saturation_mode v="Disabled" />
        </group>
      </list>
      <list name="Initialize shadow registers (included)" v="1">
        <boolgroup name="Initialize shadow registers" v="yes">
          <R0 v="0" />
          <R1 v="0" />
          <R2 v="0" />
          <R3 v="0" />
          <R4 v="0" />
          <R5 v="0" />
          <N v="0" />
          <N3 v="65535" />
          <M01 v="65535" />
        </boolgroup>
      </list>
      <list name="Initialize unused I/O pins (included)" v="1">
        <enumgroup name="Initialize unused I/O pins" v="No initialization">
          <Pull_resistor v="No initialization" />
          <Open_drain v="No initialization" />
          <Output_value v="no initialization" />
          <Include_Reset_pin v="no" />
          <Include_JTAG_pins v="no" />
        </enumgroup>
      </list>
      <group name="Internal peripherals">
        <list name="Shared Reset settings" v="1">
          <boolgroup name="Reset pin" v="Enabled">
            <Reset_Pin v="GPIOD4/RESETB" />
            <Reset_Pin_signal v="" />
          </boolgroup>
        </list>
        <list name="Flash memory organization (included)" v="1">
          <group name="Flash memory organization">
            <list name="Shared FLASH settings" v="1">
              <group name="FlexNVM settings">
                <FlexNVM_size v="16 kW" />
                <D_flash_size v="16 kW" />
                <EEE_data_size v="0 words" />
                <boolgroup name="FlexRAM" v="Enabled">
                  <Start v="122880" />
                  <Size v="1024" />
                </boolgroup>
              </group>
            </list>
            <list name="Flash blocks" v="2">
              <group name="Flash block 0">
                <Address v="0" />
                <Size v="131072" />
                <Write_unit_size v="2" />
                <Erase_unit_size v="1024" />
                <Protection_unit_size v="4096" />
              </group>
              <group name="Flash block 1">
                <Address v="32768" />
                <Size v="16384" />
                <Write_unit_size v="2" />
                <Erase_unit_size v="512" />
                <Protection_unit_size v="2048" />
              </group>
            </list>
          </group>
        </list>
        <list name="Flash config settings (included)" v="1">
          <boolgroup name="Flash configuration field" v="Disabled" />
        </list>
        <list name="Memory resource protection (include)" v="1">
          <enumgroup name="Memory resource protection" v="Disabled">
            <EmptySection_DummyValue />
          </enumgroup>
        </list>
        <group name="Peripheral clock rates">
          <QSCI0_clock_rate v="Auto select" />
          <QSCI1_clock_rate v="Auto select" />
          <QSCI2_clock_rate v="Auto select" />
        </group>
        <list name="SIM module (included)" v="1">
          <group name="System integration module">
            <group name="Common CPU settings">
              <WAIT_disable_mode v="Enabled" />
              <STOP_disable_mode v="Enabled" />
              <DMA_disable_mode v="All modes" />
              <OnCE_clock_to_core v="Enabled when core TAP is enabled" />
              <Reset_filter v="Disabled" />
              <Select_Master_PIT v="Master 0 and slave 1" />
            </group>
            <group name="Power controls">
              <Regulator_1_2_V_standby v="normal mode" />
              <Regulator_2_7_V_powerdown v="normal mode" />
              <Regulator_2_7_V_standby v="normal mode" />
              <Large_regulator_standby v="normal mode" />
            </group>
            <group name="Clock output selectors">
              <CLKOUT_divide_factor v="Divide by 1" />
              <CLKOUT0_select v="System clock" />
              <boolgroup name="CLKOUT0" v="Disabled" />
              <CLKOUT1_select v="System clock" />
              <boolgroup name="CLKOUT1" v="Disabled" />
            </group>
            <group name="Clock gating control in stop mode">
              <GPIOA_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOB_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOC_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOD_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOE_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOF_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOG_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
              <CAN_peripheral_clock_in_stop_mode v="Disabled" />
              <I2C0_peripheral_clock_in_stop_mode v="Disabled" />
              <I2C1_peripheral_clock_in_stop_mode v="Disabled" />
              <QSPI0_peripheral_clock_in_stop_mode v="Disabled" />
              <QSPI1_peripheral_clock_in_stop_mode v="Disabled" />
              <QSPI2_peripheral_clock_in_stop_mode v="Disabled" />
              <QSCI0_peripheral_clock_in_stop_mode v="Disabled" />
              <QSCI1_peripheral_clock_in_stop_mode v="Disabled" />
              <QSCI2_peripheral_clock_in_stop_mode v="Disabled" />
              <DAC_peripheral_clock_in_stop_mode v="Disabled" />
              <PDB0_peripheral_clock_in_stop_mode v="Disabled" />
              <PDB1_peripheral_clock_in_stop_mode v="Disabled" />
              <PIT0_peripheral_clock_in_stop_mode v="Disabled" />
              <PIT1_peripheral_clock_in_stop_mode v="Disabled" />
              <ENC_peripheral_clock_in_stop_mode v="Disabled" />
              <CRC_peripheral_clock_in_stop_mode v="Disabled" />
              <ADC16_peripheral_clock_in_stop_mode v="Disabled" />
              <ADC12_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPA_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPB_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPC_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPD_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
            </group>
            <group name="Clock gating control">
              <GPIOA_peripheral_clock v="Enabled" />
              <GPIOB_peripheral_clock v="Enabled" />
              <GPIOC_peripheral_clock v="Enabled" />
              <GPIOD_peripheral_clock v="Enabled" />
              <GPIOE_peripheral_clock v="Enabled" />
              <GPIOF_peripheral_clock v="Enabled" />
              <GPIOG_peripheral_clock v="Enabled" />
              <Timer_A_Channel_0_peripheral_clock v="Disabled" />
              <Timer_A_Channel_1_peripheral_clock v="Disabled" />
              <Timer_A_Channel_2_peripheral_clock v="Disabled" />
              <Timer_A_Channel_3_peripheral_clock v="Disabled" />
              <Timer_B_Channel_0_peripheral_clock v="Disabled" />
              <Timer_B_Channel_1_peripheral_clock v="Disabled" />
              <Timer_B_Channel_2_peripheral_clock v="Disabled" />
              <Timer_B_Channel_3_peripheral_clock v="Disabled" />
              <CAN_peripheral_clock v="Disabled" />
              <I2C0_peripheral_clock v="Disabled" />
              <I2C1_peripheral_clock v="Disabled" />
              <QSPI0_peripheral_clock v="Disabled" />
              <QSPI1_peripheral_clock v="Disabled" />
              <QSPI2_peripheral_clock v="Disabled" />
              <QSCI0_peripheral_clock v="Disabled" />
              <QSCI1_peripheral_clock v="Enabled" />
              <QSCI2_peripheral_clock v="Disabled" />
              <DAC_peripheral_clock v="Disabled" />
              <PDB0_peripheral_clock v="Disabled" />
              <PDB1_peripheral_clock v="Disabled" />
              <PIT0_peripheral_clock v="Disabled" />
              <PIT1_peripheral_clock v="Disabled" />
              <ENC_peripheral_clock v="Disabled" />
              <CRC_peripheral_clock v="Disabled" />
              <ADC16_peripheral_clock v="Disabled" />
              <ADC12_peripheral_clock v="Disabled" />
              <CMPA_peripheral_clock v="Disabled" />
              <CMPB_peripheral_clock v="Disabled" />
              <CMPC_peripheral_clock v="Disabled" />
              <CMPD_peripheral_clock v="Disabled" />
              <PWM_A_Channel_0_peripheral_clock v="Disabled" />
              <PWM_A_Channel_1_peripheral_clock v="Disabled" />
              <PWM_A_Channel_2_peripheral_clock v="Disabled" />
              <PWM_A_Channel_3_peripheral_clock v="Disabled" />
              <PWM_B_Channel_0_peripheral_clock v="Disabled" />
              <PWM_B_Channel_1_peripheral_clock v="Disabled" />
              <PWM_B_Channel_2_peripheral_clock v="Disabled" />
              <PWM_B_Channel_3_peripheral_clock v="Disabled" />
            </group>
            <group name="Peripheral protection">
              <Power_Mode_Control_Write v="Off" />
              <GPIO_Port_D v="Off" />
              <Peripheral_Clock_Enable v="Off" />
              <GPIO_and_Internal_Peripheral_Select v="Off" />
            </group>
          </group>
        </list>
        <list name="MCM module (included)" v="1">
          <group name="Miscellaneous control module">
            <Program_RAM_Base_Address v="0" />
            <Flash_Base_Address v="0" />
            <Register_lock v="Disabled" />
            <AXBS_crossbar_switch_arbitration_scheme v="Fixed priority" />
            <Core_instruction_buffer v="Enabled" />
            <Core_new_shadow_region v="Enabled" />
            <Core_reverse_carry v="Enabled" />
            <_56800EX_instructions v="Enabled" />
            <group name="SoC control fields">
              <SoC_output_0_signal v="Disabled" />
              <SoC_output_1_signal v="Disabled" />
              <SoC_output_2_signal v="Disabled" />
              <SoC_output_3_signal v="Disabled" />
              <SoC_output_4_signal v="Disabled" />
              <SoC_output_5_signal v="Disabled" />
              <SoC_output_6_signal v="Disabled" />
              <SoC_output_7_signal v="Disabled" />
              <SoC_output_8_signal v="Disabled" />
              <SoC_output_9_signal v="Disabled" />
              <SoC_output_10_signal v="Disabled" />
              <SoC_output_11_signal v="Disabled" />
              <SoC_output_12_signal v="Disabled" />
              <SoC_output_13_signal v="Disabled" />
              <SoC_output_14_signal v="Disabled" />
              <SoC_output_15_signal v="Disabled" />
            </group>
          </group>
        </list>
        <list name="PMC module (included)" v="1">
          <boolgroup name="Power management controller" v="Disabled" />
        </list>
        <list name="FMC module (included)" v="1">
          <boolgroup name="Flexible memory controller" v="Disabled" />
        </list>
        <list name="GPIOA module (included)" v="1">
          <group name="GPIOA">
            <group name="GPIOA_Low">
              <Drive_strength_for_GPIOA0 v="Low" />
              <Slew_rate_for_GPIOA0 v="Fast" />
              <Drive_strength_for_GPIOA1 v="Low" />
              <Slew_rate_for_GPIOA1 v="Fast" />
              <Drive_strength_for_GPIOA2 v="Low" />
              <Slew_rate_for_GPIOA2 v="Fast" />
              <Drive_strength_for_GPIOA3 v="Low" />
              <Slew_rate_for_GPIOA3 v="Fast" />
              <Drive_strength_for_GPIOA4 v="Low" />
              <Slew_rate_for_GPIOA4 v="Fast" />
              <Drive_strength_for_GPIOA5 v="Low" />
              <Slew_rate_for_GPIOA5 v="Fast" />
              <Drive_strength_for_GPIOA6 v="Low" />
              <Slew_rate_for_GPIOA6 v="Fast" />
              <Drive_strength_for_GPIOA7 v="Low" />
              <Slew_rate_for_GPIOA7 v="Fast" />
            </group>
            <group name="GPIOA_High">
              <Drive_strength_for_GPIOA8 v="Low" />
              <Slew_rate_for_GPIOA8 v="Fast" />
              <Drive_strength_for_GPIOA9 v="Low" />
              <Slew_rate_for_GPIOA9 v="Fast" />
              <Drive_strength_for_GPIOA10 v="Low" />
              <Slew_rate_for_GPIOA10 v="Fast" />
              <Drive_strength_for_GPIOA11 v="Low" />
              <Slew_rate_for_GPIOA11 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOB module (included)" v="1">
          <group name="GPIOB">
            <group name="GPIOB_Low">
              <Drive_strength_for_GPIOB0 v="Low" />
              <Slew_rate_for_GPIOB0 v="Fast" />
              <Drive_strength_for_GPIOB1 v="Low" />
              <Slew_rate_for_GPIOB1 v="Fast" />
              <Drive_strength_for_GPIOB2 v="Low" />
              <Slew_rate_for_GPIOB2 v="Fast" />
              <Drive_strength_for_GPIOB3 v="Low" />
              <Slew_rate_for_GPIOB3 v="Fast" />
              <Drive_strength_for_GPIOB4 v="Low" />
              <Slew_rate_for_GPIOB4 v="Fast" />
              <Drive_strength_for_GPIOB5 v="Low" />
              <Slew_rate_for_GPIOB5 v="Fast" />
              <Drive_strength_for_GPIOB6 v="Low" />
              <Slew_rate_for_GPIOB6 v="Fast" />
              <Drive_strength_for_GPIOB7 v="Low" />
              <Slew_rate_for_GPIOB7 v="Fast" />
            </group>
            <group name="GPIOB_High">
              <Drive_strength_for_GPIOB8 v="Low" />
              <Slew_rate_for_GPIOB8 v="Fast" />
              <Drive_strength_for_GPIOB9 v="Low" />
              <Slew_rate_for_GPIOB9 v="Fast" />
              <Drive_strength_for_GPIOB10 v="Low" />
              <Slew_rate_for_GPIOB10 v="Fast" />
              <Drive_strength_for_GPIOB11 v="Low" />
              <Slew_rate_for_GPIOB11 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOC module (included)" v="1">
          <group name="GPIOC">
            <group name="GPIOC_Low">
              <Drive_strength_for_GPIOC0 v="Low" />
              <Slew_rate_for_GPIOC0 v="Fast" />
              <Drive_strength_for_GPIOC1 v="Low" />
              <Slew_rate_for_GPIOC1 v="Fast" />
              <Drive_strength_for_GPIOC2 v="Low" />
              <Slew_rate_for_GPIOC2 v="Fast" />
              <Drive_strength_for_GPIOC3 v="Low" />
              <Slew_rate_for_GPIOC3 v="Fast" />
              <Drive_strength_for_GPIOC4 v="Low" />
              <Slew_rate_for_GPIOC4 v="Fast" />
              <Drive_strength_for_GPIOC5 v="Low" />
              <Slew_rate_for_GPIOC5 v="Fast" />
              <Drive_strength_for_GPIOC6 v="Low" />
              <Slew_rate_for_GPIOC6 v="Fast" />
              <Drive_strength_for_GPIOC7 v="Low" />
              <Slew_rate_for_GPIOC7 v="Fast" />
            </group>
            <group name="GPIOC_High">
              <Drive_strength_for_GPIOC8 v="Low" />
              <Slew_rate_for_GPIOC8 v="Fast" />
              <Drive_strength_for_GPIOC9 v="Low" />
              <Slew_rate_for_GPIOC9 v="Fast" />
              <Drive_strength_for_GPIOC10 v="Low" />
              <Slew_rate_for_GPIOC10 v="Fast" />
              <Drive_strength_for_GPIOC11 v="Low" />
              <Slew_rate_for_GPIOC11 v="Fast" />
              <Drive_strength_for_GPIOC12 v="Low" />
              <Slew_rate_for_GPIOC12 v="Fast" />
              <Drive_strength_for_GPIOC13 v="Low" />
              <Slew_rate_for_GPIOC13 v="Fast" />
              <Drive_strength_for_GPIOC14 v="Low" />
              <Slew_rate_for_GPIOC14 v="Fast" />
              <Drive_strength_for_GPIOC15 v="Low" />
              <Slew_rate_for_GPIOC15 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOD module (included)" v="1">
          <group name="GPIOD">
            <Drive_strength_for_GPIOD0 v="Low" />
            <Slew_rate_for_GPIOD0 v="Fast" />
            <Drive_strength_for_GPIOD1 v="Low" />
            <Slew_rate_for_GPIOD1 v="Fast" />
            <Drive_strength_for_GPIOD2 v="Low" />
            <Slew_rate_for_GPIOD2 v="Fast" />
            <Drive_strength_for_GPIOD3 v="Low" />
            <Slew_rate_for_GPIOD3 v="Fast" />
            <Drive_strength_for_GPIOD4 v="Low" />
            <Slew_rate_for_GPIOD4 v="Fast" />
            <Drive_strength_for_GPIOD5 v="Low" />
            <Slew_rate_for_GPIOD5 v="Fast" />
            <Drive_strength_for_GPIOD6 v="Low" />
            <Slew_rate_for_GPIOD6 v="Fast" />
            <Drive_strength_for_GPIOD7 v="Low" />
            <Slew_rate_for_GPIOD7 v="Fast" />
          </group>
        </list>
        <list name="GPIOE module (included)" v="1">
          <group name="GPIOE">
            <group name="GPIOE_Low">
              <Drive_strength_for_GPIOE0 v="Low" />
              <Slew_rate_for_GPIOE0 v="Fast" />
              <Drive_strength_for_GPIOE1 v="Low" />
              <Slew_rate_for_GPIOE1 v="Fast" />
              <Drive_strength_for_GPIOE2 v="Low" />
              <Slew_rate_for_GPIOE2 v="Fast" />
              <Drive_strength_for_GPIOE3 v="Low" />
              <Slew_rate_for_GPIOE3 v="Fast" />
              <Drive_strength_for_GPIOE4 v="Low" />
              <Slew_rate_for_GPIOE4 v="Fast" />
              <Drive_strength_for_GPIOE5 v="Low" />
              <Slew_rate_for_GPIOE5 v="Fast" />
              <Drive_strength_for_GPIOE6 v="Low" />
              <Slew_rate_for_GPIOE6 v="Fast" />
              <Drive_strength_for_GPIOE7 v="Low" />
              <Slew_rate_for_GPIOE7 v="Fast" />
            </group>
            <group name="GPIOE_High">
              <Drive_strength_for_GPIOE8 v="Low" />
              <Slew_rate_for_GPIOE8 v="Fast" />
              <Drive_strength_for_GPIOE9 v="Low" />
              <Slew_rate_for_GPIOE9 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOF module (included)" v="1">
          <group name="GPIOF">
            <group name="GPIOF_Low">
              <Drive_strength_for_GPIOF0 v="Low" />
              <Slew_rate_for_GPIOF0 v="Fast" />
              <Drive_strength_for_GPIOF1 v="Low" />
              <Slew_rate_for_GPIOF1 v="Fast" />
              <Drive_strength_for_GPIOF2 v="Low" />
              <Slew_rate_for_GPIOF2 v="Fast" />
              <Drive_strength_for_GPIOF3 v="Low" />
              <Slew_rate_for_GPIOF3 v="Fast" />
              <Drive_strength_for_GPIOF4 v="Low" />
              <Slew_rate_for_GPIOF4 v="Fast" />
              <Drive_strength_for_GPIOF5 v="Low" />
              <Slew_rate_for_GPIOF5 v="Fast" />
              <Drive_strength_for_GPIOF6 v="Low" />
              <Slew_rate_for_GPIOF6 v="Fast" />
              <Drive_strength_for_GPIOF7 v="Low" />
              <Slew_rate_for_GPIOF7 v="Fast" />
            </group>
            <group name="GPIOF_High">
              <Drive_strength_for_GPIOF8 v="Low" />
              <Slew_rate_for_GPIOF8 v="Fast" />
              <Drive_strength_for_GPIOF9 v="Low" />
              <Slew_rate_for_GPIOF9 v="Fast" />
              <Drive_strength_for_GPIOF10 v="Low" />
              <Slew_rate_for_GPIOF10 v="Fast" />
              <Drive_strength_for_GPIOF11 v="Low" />
              <Slew_rate_for_GPIOF11 v="Fast" />
              <Drive_strength_for_GPIOF12 v="Low" />
              <Slew_rate_for_GPIOF12 v="Fast" />
              <Drive_strength_for_GPIOF13 v="Low" />
              <Slew_rate_for_GPIOF13 v="Fast" />
              <Drive_strength_for_GPIOF14 v="Low" />
              <Slew_rate_for_GPIOF14 v="Fast" />
              <Drive_strength_for_GPIOF15 v="Low" />
              <Slew_rate_for_GPIOF15 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOG module (included)" v="1">
          <group name="GPIOG">
            <group name="GPIOG_Low">
              <Drive_strength_for_GPIOG0 v="Low" />
              <Slew_rate_for_GPIOG0 v="Fast" />
              <Drive_strength_for_GPIOG1 v="Low" />
              <Slew_rate_for_GPIOG1 v="Fast" />
              <Drive_strength_for_GPIOG2 v="Low" />
              <Slew_rate_for_GPIOG2 v="Fast" />
              <Drive_strength_for_GPIOG3 v="Low" />
              <Slew_rate_for_GPIOG3 v="Fast" />
              <Drive_strength_for_GPIOG4 v="Low" />
              <Slew_rate_for_GPIOG4 v="Fast" />
              <Drive_strength_for_GPIOG5 v="Low" />
              <Slew_rate_for_GPIOG5 v="Fast" />
              <Drive_strength_for_GPIOG6 v="Low" />
              <Slew_rate_for_GPIOG6 v="Fast" />
              <Drive_strength_for_GPIOG7 v="Low" />
              <Slew_rate_for_GPIOG7 v="Fast" />
            </group>
            <group name="GPIOG_High">
              <Drive_strength_for_GPIOG8 v="Low" />
              <Slew_rate_for_GPIOG8 v="Fast" />
              <Drive_strength_for_GPIOG9 v="Low" />
              <Slew_rate_for_GPIOG9 v="Fast" />
              <Drive_strength_for_GPIOG10 v="Low" />
              <Slew_rate_for_GPIOG10 v="Fast" />
              <Drive_strength_for_GPIOG11 v="Low" />
              <Slew_rate_for_GPIOG11 v="Fast" />
            </group>
          </group>
        </list>
      </group>
      <group name="CPU interrupts">
        <boolgroup name="Interrupt SW0" v="Disabled" />
        <boolgroup name="Interrupt SW1" v="Disabled" />
        <boolgroup name="Interrupt SW2" v="Disabled" />
        <boolgroup name="Interrupt SW3" v="Disabled" />
        <boolgroup name="Interrupt LP" v="Disabled" />
        <boolgroup name="Interrupt PLL" v="Disabled" />
        <boolgroup name="Interrupt LVI" v="Disabled" />
        <boolgroup name="Interrupt Illegal Instruction" v="Disabled" />
        <boolgroup name="Interrupt Misalign Access" v="Disabled" />
        <boolgroup name="Interrupt HW Stack Overflow" v="Disabled" />
        <list name="MCM module (included)" v="1">
          <boolgroup name="Interrupt Core Fault" v="Disabled" />
        </list>
      </group>
      <list name="Enabled speed modes (included)" v="1">
        <group name="Enabled speed modes">
          <boolgroup name="High speed mode" v="Enabled">
            <Input_clock_source_ v="Internal oscillator 8MHz" />
            <Clock_output_divider__Postscaler_ v="Auto select" />
            <System_clock__IP_Bus___MHz_ v="100" />
            <boolgroup name="PLL clock" v="Enabled">
              <PLL_multiplier v="Auto select" />
              <PLL_clock_frequency v="400" />
              <Enable_PLL_after_reset v="yes" />
            </boolgroup>
          </boolgroup>
          <boolgroup name="Low speed mode" v="Disabled" />
          <boolgroup name="Slow speed mode" v="Disabled" />
        </group>
      </list>
    </Properties>
    <Methods>
      <list name="CPUCond0" v="1">
        <SetHighSpeed v="don&amp;apos;t generate code" />
        <SetLowSpeed v="don&amp;apos;t generate code" />
        <SetSlowSpeed v="don&amp;apos;t generate code" />
        <GetSpeedMode v="don&amp;apos;t generate code" />
        <EnableInt v="generate code" />
        <DisableInt v="generate code" />
        <GetResetSource v="don&amp;apos;t generate code" />
        <SetWaitMode v="generate code" />
        <SetStopMode v="generate code" />
        <GetBusFreqHz v="don&amp;apos;t generate code" />
        <OpenBackDoor v="don&amp;apos;t generate code" />
        <SetFlexRAMFunction v="don&amp;apos;t generate code" />
        <SetFlexNVMPartition v="don&amp;apos;t generate code" />
        <InitShadowRegs v="don&amp;apos;t generate code" />
        <Delay100US v="don&amp;apos;t generate code" />
        <EnablePLL v="don&amp;apos;t generate code" />
      </list>
    </Methods>
    <Events>
      <Event_module_name v="Events" />
      <list name="CPUCond" v="1">
        <event name="OnReset" v="don&amp;apos;t generate code" />
        <event name="OnSwINT0" v="don&amp;apos;t generate code" />
        <event name="OnSwINT1" v="don&amp;apos;t generate code" />
        <event name="OnSwINT2" v="don&amp;apos;t generate code" />
        <event name="OnSwINT3" v="don&amp;apos;t generate code" />
        <event name="OnSwINTLP" v="don&amp;apos;t generate code" />
        <event name="OnPLLError" v="don&amp;apos;t generate code" />
        <event name="OnIllegalOpcode" v="don&amp;apos;t generate code" />
        <event name="OnMisalignData" v="don&amp;apos;t generate code" />
        <event name="OnHWStackError" v="don&amp;apos;t generate code" />
        <event name="OnLVI22" v="don&amp;apos;t generate code" />
        <event name="OnLVI27" v="don&amp;apos;t generate code" />
        <event name="OnCoreFault" v="don&amp;apos;t generate code" />
      </list>
    </Events>
    <Compiler v="CodeWarrior DSP C Compiler" />
    <CompilerProperties>
      <Compiler v="CodeWarrior DSP C Compiler" />
      <PESL_support v="yes" />
      <Unhandled_interrupts v="One handler for all" />
      <group name="User initialization">
        <User_data_declarations>
          <StrgList></StrgList>
        </User_data_declarations>
        <User_code_before_PE_initialization>
          <StrgList></StrgList>
        </User_code_before_PE_initialization>
        <User_code_after_PE_initialization>
          <StrgList></StrgList>
        </User_code_after_PE_initialization>
      </group>
      <boolgroup name="Generate debugger files" v="yes">
        <Generate_mem_file v="yes" />
      </boolgroup>
      <boolgroup name="Generate linker file" v="yes">
        <Constants_in_xROM v="no" />
        <xROM_xRAM_mode v="no" />
        <pROM_xRAM_mode v="no" />
        <Stack_size v="512" />
        <Heap_size v="256" />
        <Set_memory_segments_to_default v="Click to set default &amp;gt;" />
        <Default_memory_for_interrupts v="INTERNAL FLASH" />
        <Default_memory_for_code v="INTERNAL FLASH" />
        <Default_memory_for_data v="INTERNAL RAM" />
        <list name="ROM/RAM Areas" v="4">
          <group name="MemoryArea0">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_Interrupts" />
              <Address v="0" />
              <Size v="222" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea1">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_Code" />
              <Address v="520" />
              <Size v="130552" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea2">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".x_Data" />
              <Address v="1" />
              <Size v="16383" />
              <Qualifier v="RW" />
            </boolgroup>
          </group>
          <group name="MemoryArea3">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_reserved_FCF" />
              <Address v="512" />
              <Size v="8" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
        </list>
      </boolgroup>
      <list name="System paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="Libraries" v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User directories" v="0">
        <EmptySection_DummyValue />
      </list>
    </CompilerProperties>
  </CPU_Bean>
  <CPU_Bean name="Cpu" type="MC56F84789VLL">
    <Enabled v="N" />
    <Properties>
      <Component_name v="Cpu" />
      <CPU_type v="MC56F84789VLL" />
      <list name="Clock settings (included)" v="1">
        <group name="Clock settings">
          <group name="Internal oscillator">
            <boolgroup name="Internal 32kHz relaxation oscillator (ROSC_32K)" v="Disabled" />
            <boolgroup name="Internal 8MHz relaxation oscillator (ROSC_8M)" v="Enabled">
              <Fast_internal_reference_clock__MHz_ v="8" />
              <boolgroup name="Initialize frequency trim" v="no" />
              <boolgroup name="Initialize temperature trim" v="no" />
            </boolgroup>
          </group>
          <boolgroup name="External reference clock" v="Disabled" />
          <group name="Clock protection">
            <Frequency v="Off" />
            <Oscillator v="Off" />
            <Phase_locked_loop v="Off" />
          </group>
        </group>
      </list>
      <list name="Common settings (included)" v="1">
        <group name="Common settings">
          <Initialization_priority v="minimal priority" />
          <Watchdog v="Disabled" />
          <Saturation_mode v="Disabled" />
        </group>
      </list>
      <list name="Initialize shadow registers (included)" v="1">
        <boolgroup name="Initialize shadow registers" v="no" />
      </list>
      <list name="Initialize unused I/O pins (included)" v="1">
        <enumgroup name="Initialize unused I/O pins" v="No initialization">
          <Pull_resistor v="No initialization" />
          <Open_drain v="No initialization" />
          <Output_value v="no initialization" />
          <Include_Reset_pin v="no" />
          <Include_JTAG_pins v="no" />
        </enumgroup>
      </list>
      <group name="Internal peripherals">
        <list name="Shared Reset settings" v="1">
          <boolgroup name="Reset pin" v="Enabled">
            <Reset_Pin v="GPIOD4/RESETB" />
            <Reset_Pin_signal v="" />
          </boolgroup>
        </list>
        <list name="Flash memory organization (included)" v="1">
          <group name="Flash memory organization">
            <list name="Shared FLASH settings" v="1">
              <group name="FlexNVM settings">
                <FlexNVM_size v="16 kW" />
                <D_flash_size v="16 kW" />
                <EEE_data_size v="0 words" />
                <boolgroup name="FlexRAM" v="Enabled">
                  <Start v="122880" />
                  <Size v="1024" />
                </boolgroup>
              </group>
            </list>
            <list name="Flash blocks" v="2">
              <group name="Flash block 0">
                <Address v="0" />
                <Size v="131072" />
                <Write_unit_size v="2" />
                <Erase_unit_size v="1024" />
                <Protection_unit_size v="4096" />
              </group>
              <group name="Flash block 1">
                <Address v="32768" />
                <Size v="16384" />
                <Write_unit_size v="2" />
                <Erase_unit_size v="512" />
                <Protection_unit_size v="2048" />
              </group>
            </list>
          </group>
        </list>
        <list name="Flash config settings (included)" v="1">
          <boolgroup name="Flash configuration field" v="Disabled" />
        </list>
        <list name="Memory resource protection (include)" v="1">
          <enumgroup name="Memory resource protection" v="Disabled">
            <EmptySection_DummyValue />
          </enumgroup>
        </list>
        <group name="Peripheral clock rates">
          <QSCI0_clock_rate v="Auto select" />
          <QSCI1_clock_rate v="Auto select" />
          <QSCI2_clock_rate v="Auto select" />
        </group>
        <list name="SIM module (included)" v="1">
          <group name="System integration module">
            <group name="Common CPU settings">
              <WAIT_disable_mode v="Enabled" />
              <STOP_disable_mode v="Enabled" />
              <DMA_disable_mode v="All modes" />
              <OnCE_clock_to_core v="Enabled when core TAP is enabled" />
              <Reset_filter v="Disabled" />
              <Select_Master_PIT v="Master 0 and slave 1" />
            </group>
            <group name="Power controls">
              <Regulator_1_2_V_standby v="normal mode" />
              <Regulator_2_7_V_powerdown v="normal mode" />
              <Regulator_2_7_V_standby v="normal mode" />
              <Large_regulator_standby v="normal mode" />
            </group>
            <group name="Clock output selectors">
              <CLKOUT_divide_factor v="Divide by 1" />
              <CLKOUT0_select v="System clock" />
              <boolgroup name="CLKOUT0" v="Disabled" />
              <CLKOUT1_select v="System clock" />
              <boolgroup name="CLKOUT1" v="Disabled" />
            </group>
            <group name="Clock gating control in stop mode">
              <GPIOA_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOB_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOC_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOD_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOE_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOF_peripheral_clock_in_stop_mode v="Disabled" />
              <GPIOG_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_A_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <Timer_B_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
              <CAN_peripheral_clock_in_stop_mode v="Disabled" />
              <I2C0_peripheral_clock_in_stop_mode v="Disabled" />
              <I2C1_peripheral_clock_in_stop_mode v="Disabled" />
              <QSPI0_peripheral_clock_in_stop_mode v="Disabled" />
              <QSPI1_peripheral_clock_in_stop_mode v="Disabled" />
              <QSPI2_peripheral_clock_in_stop_mode v="Disabled" />
              <QSCI0_peripheral_clock_in_stop_mode v="Disabled" />
              <QSCI1_peripheral_clock_in_stop_mode v="Disabled" />
              <QSCI2_peripheral_clock_in_stop_mode v="Disabled" />
              <DAC_peripheral_clock_in_stop_mode v="Disabled" />
              <PDB0_peripheral_clock_in_stop_mode v="Disabled" />
              <PDB1_peripheral_clock_in_stop_mode v="Disabled" />
              <PIT0_peripheral_clock_in_stop_mode v="Disabled" />
              <PIT1_peripheral_clock_in_stop_mode v="Disabled" />
              <ENC_peripheral_clock_in_stop_mode v="Disabled" />
              <CRC_peripheral_clock_in_stop_mode v="Disabled" />
              <ADC16_peripheral_clock_in_stop_mode v="Disabled" />
              <ADC12_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPA_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPB_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPC_peripheral_clock_in_stop_mode v="Disabled" />
              <CMPD_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_A_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_0_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_1_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_2_peripheral_clock_in_stop_mode v="Disabled" />
              <PWM_B_Channel_3_peripheral_clock_in_stop_mode v="Disabled" />
            </group>
            <group name="Clock gating control">
              <GPIOA_peripheral_clock v="Enabled" />
              <GPIOB_peripheral_clock v="Enabled" />
              <GPIOC_peripheral_clock v="Enabled" />
              <GPIOD_peripheral_clock v="Enabled" />
              <GPIOE_peripheral_clock v="Enabled" />
              <GPIOF_peripheral_clock v="Enabled" />
              <GPIOG_peripheral_clock v="Enabled" />
              <Timer_A_Channel_0_peripheral_clock v="Disabled" />
              <Timer_A_Channel_1_peripheral_clock v="Disabled" />
              <Timer_A_Channel_2_peripheral_clock v="Disabled" />
              <Timer_A_Channel_3_peripheral_clock v="Disabled" />
              <Timer_B_Channel_0_peripheral_clock v="Disabled" />
              <Timer_B_Channel_1_peripheral_clock v="Disabled" />
              <Timer_B_Channel_2_peripheral_clock v="Disabled" />
              <Timer_B_Channel_3_peripheral_clock v="Disabled" />
              <CAN_peripheral_clock v="Disabled" />
              <I2C0_peripheral_clock v="Disabled" />
              <I2C1_peripheral_clock v="Disabled" />
              <QSPI0_peripheral_clock v="Disabled" />
              <QSPI1_peripheral_clock v="Disabled" />
              <QSPI2_peripheral_clock v="Disabled" />
              <QSCI0_peripheral_clock v="Disabled" />
              <QSCI1_peripheral_clock v="Enabled" />
              <QSCI2_peripheral_clock v="Disabled" />
              <DAC_peripheral_clock v="Disabled" />
              <PDB0_peripheral_clock v="Disabled" />
              <PDB1_peripheral_clock v="Disabled" />
              <PIT0_peripheral_clock v="Disabled" />
              <PIT1_peripheral_clock v="Disabled" />
              <ENC_peripheral_clock v="Disabled" />
              <CRC_peripheral_clock v="Disabled" />
              <ADC16_peripheral_clock v="Disabled" />
              <ADC12_peripheral_clock v="Disabled" />
              <CMPA_peripheral_clock v="Disabled" />
              <CMPB_peripheral_clock v="Disabled" />
              <CMPC_peripheral_clock v="Disabled" />
              <CMPD_peripheral_clock v="Disabled" />
              <PWM_A_Channel_0_peripheral_clock v="Disabled" />
              <PWM_A_Channel_1_peripheral_clock v="Disabled" />
              <PWM_A_Channel_2_peripheral_clock v="Disabled" />
              <PWM_A_Channel_3_peripheral_clock v="Disabled" />
              <PWM_B_Channel_0_peripheral_clock v="Disabled" />
              <PWM_B_Channel_1_peripheral_clock v="Disabled" />
              <PWM_B_Channel_2_peripheral_clock v="Disabled" />
              <PWM_B_Channel_3_peripheral_clock v="Disabled" />
            </group>
            <group name="Peripheral protection">
              <Power_Mode_Control_Write v="Off" />
              <GPIO_Port_D v="Off" />
              <Peripheral_Clock_Enable v="Off" />
              <GPIO_and_Internal_Peripheral_Select v="Off" />
            </group>
          </group>
        </list>
        <list name="MCM module (included)" v="1">
          <group name="Miscellaneous control module">
            <Program_RAM_Base_Address v="0" />
            <Flash_Base_Address v="0" />
            <Register_lock v="Disabled" />
            <AXBS_crossbar_switch_arbitration_scheme v="Fixed priority" />
            <Core_instruction_buffer v="Enabled" />
            <Core_new_shadow_region v="Enabled" />
            <Core_reverse_carry v="Enabled" />
            <_56800EX_instructions v="Enabled" />
            <group name="SoC control fields">
              <SoC_output_0_signal v="Disabled" />
              <SoC_output_1_signal v="Disabled" />
              <SoC_output_2_signal v="Disabled" />
              <SoC_output_3_signal v="Disabled" />
              <SoC_output_4_signal v="Disabled" />
              <SoC_output_5_signal v="Disabled" />
              <SoC_output_6_signal v="Disabled" />
              <SoC_output_7_signal v="Disabled" />
              <SoC_output_8_signal v="Disabled" />
              <SoC_output_9_signal v="Disabled" />
              <SoC_output_10_signal v="Disabled" />
              <SoC_output_11_signal v="Disabled" />
              <SoC_output_12_signal v="Disabled" />
              <SoC_output_13_signal v="Disabled" />
              <SoC_output_14_signal v="Disabled" />
              <SoC_output_15_signal v="Disabled" />
            </group>
          </group>
        </list>
        <list name="PMC module (included)" v="1">
          <boolgroup name="Power management controller" v="Disabled" />
        </list>
        <list name="FMC module (included)" v="1">
          <boolgroup name="Flexible memory controller" v="Disabled" />
        </list>
        <list name="GPIOA module (included)" v="1">
          <group name="GPIOA">
            <group name="GPIOA_Low">
              <Drive_strength_for_GPIOA0 v="Low" />
              <Slew_rate_for_GPIOA0 v="Fast" />
              <Drive_strength_for_GPIOA1 v="Low" />
              <Slew_rate_for_GPIOA1 v="Fast" />
              <Drive_strength_for_GPIOA2 v="Low" />
              <Slew_rate_for_GPIOA2 v="Fast" />
              <Drive_strength_for_GPIOA3 v="Low" />
              <Slew_rate_for_GPIOA3 v="Fast" />
              <Drive_strength_for_GPIOA4 v="Low" />
              <Slew_rate_for_GPIOA4 v="Fast" />
              <Drive_strength_for_GPIOA5 v="Low" />
              <Slew_rate_for_GPIOA5 v="Fast" />
              <Drive_strength_for_GPIOA6 v="Low" />
              <Slew_rate_for_GPIOA6 v="Fast" />
              <Drive_strength_for_GPIOA7 v="Low" />
              <Slew_rate_for_GPIOA7 v="Fast" />
            </group>
            <group name="GPIOA_High">
              <Drive_strength_for_GPIOA8 v="Low" />
              <Slew_rate_for_GPIOA8 v="Fast" />
              <Drive_strength_for_GPIOA9 v="Low" />
              <Slew_rate_for_GPIOA9 v="Fast" />
              <Drive_strength_for_GPIOA10 v="Low" />
              <Slew_rate_for_GPIOA10 v="Fast" />
              <Drive_strength_for_GPIOA11 v="Low" />
              <Slew_rate_for_GPIOA11 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOB module (included)" v="1">
          <group name="GPIOB">
            <group name="GPIOB_Low">
              <Drive_strength_for_GPIOB0 v="Low" />
              <Slew_rate_for_GPIOB0 v="Fast" />
              <Drive_strength_for_GPIOB1 v="Low" />
              <Slew_rate_for_GPIOB1 v="Fast" />
              <Drive_strength_for_GPIOB2 v="Low" />
              <Slew_rate_for_GPIOB2 v="Fast" />
              <Drive_strength_for_GPIOB3 v="Low" />
              <Slew_rate_for_GPIOB3 v="Fast" />
              <Drive_strength_for_GPIOB4 v="Low" />
              <Slew_rate_for_GPIOB4 v="Fast" />
              <Drive_strength_for_GPIOB5 v="Low" />
              <Slew_rate_for_GPIOB5 v="Fast" />
              <Drive_strength_for_GPIOB6 v="Low" />
              <Slew_rate_for_GPIOB6 v="Fast" />
              <Drive_strength_for_GPIOB7 v="Low" />
              <Slew_rate_for_GPIOB7 v="Fast" />
            </group>
            <group name="GPIOB_High">
              <Drive_strength_for_GPIOB8 v="Low" />
              <Slew_rate_for_GPIOB8 v="Fast" />
              <Drive_strength_for_GPIOB9 v="Low" />
              <Slew_rate_for_GPIOB9 v="Fast" />
              <Drive_strength_for_GPIOB10 v="Low" />
              <Slew_rate_for_GPIOB10 v="Fast" />
              <Drive_strength_for_GPIOB11 v="Low" />
              <Slew_rate_for_GPIOB11 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOC module (included)" v="1">
          <group name="GPIOC">
            <group name="GPIOC_Low">
              <Drive_strength_for_GPIOC0 v="Low" />
              <Slew_rate_for_GPIOC0 v="Fast" />
              <Drive_strength_for_GPIOC1 v="Low" />
              <Slew_rate_for_GPIOC1 v="Fast" />
              <Drive_strength_for_GPIOC2 v="Low" />
              <Slew_rate_for_GPIOC2 v="Fast" />
              <Drive_strength_for_GPIOC3 v="Low" />
              <Slew_rate_for_GPIOC3 v="Fast" />
              <Drive_strength_for_GPIOC4 v="Low" />
              <Slew_rate_for_GPIOC4 v="Fast" />
              <Drive_strength_for_GPIOC5 v="Low" />
              <Slew_rate_for_GPIOC5 v="Fast" />
              <Drive_strength_for_GPIOC6 v="Low" />
              <Slew_rate_for_GPIOC6 v="Fast" />
              <Drive_strength_for_GPIOC7 v="Low" />
              <Slew_rate_for_GPIOC7 v="Fast" />
            </group>
            <group name="GPIOC_High">
              <Drive_strength_for_GPIOC8 v="Low" />
              <Slew_rate_for_GPIOC8 v="Fast" />
              <Drive_strength_for_GPIOC9 v="Low" />
              <Slew_rate_for_GPIOC9 v="Fast" />
              <Drive_strength_for_GPIOC10 v="Low" />
              <Slew_rate_for_GPIOC10 v="Fast" />
              <Drive_strength_for_GPIOC11 v="Low" />
              <Slew_rate_for_GPIOC11 v="Fast" />
              <Drive_strength_for_GPIOC12 v="Low" />
              <Slew_rate_for_GPIOC12 v="Fast" />
              <Drive_strength_for_GPIOC13 v="Low" />
              <Slew_rate_for_GPIOC13 v="Fast" />
              <Drive_strength_for_GPIOC14 v="Low" />
              <Slew_rate_for_GPIOC14 v="Fast" />
              <Drive_strength_for_GPIOC15 v="Low" />
              <Slew_rate_for_GPIOC15 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOD module (included)" v="1">
          <group name="GPIOD">
            <Drive_strength_for_GPIOD0 v="Low" />
            <Slew_rate_for_GPIOD0 v="Fast" />
            <Drive_strength_for_GPIOD1 v="Low" />
            <Slew_rate_for_GPIOD1 v="Fast" />
            <Drive_strength_for_GPIOD2 v="Low" />
            <Slew_rate_for_GPIOD2 v="Fast" />
            <Drive_strength_for_GPIOD3 v="Low" />
            <Slew_rate_for_GPIOD3 v="Fast" />
            <Drive_strength_for_GPIOD4 v="Low" />
            <Slew_rate_for_GPIOD4 v="Fast" />
            <Drive_strength_for_GPIOD5 v="Low" />
            <Slew_rate_for_GPIOD5 v="Fast" />
            <Drive_strength_for_GPIOD6 v="Low" />
            <Slew_rate_for_GPIOD6 v="Fast" />
            <Drive_strength_for_GPIOD7 v="Low" />
            <Slew_rate_for_GPIOD7 v="Fast" />
          </group>
        </list>
        <list name="GPIOE module (included)" v="1">
          <group name="GPIOE">
            <group name="GPIOE_Low">
              <Drive_strength_for_GPIOE0 v="Low" />
              <Slew_rate_for_GPIOE0 v="Fast" />
              <Drive_strength_for_GPIOE1 v="Low" />
              <Slew_rate_for_GPIOE1 v="Fast" />
              <Drive_strength_for_GPIOE2 v="Low" />
              <Slew_rate_for_GPIOE2 v="Fast" />
              <Drive_strength_for_GPIOE3 v="Low" />
              <Slew_rate_for_GPIOE3 v="Fast" />
              <Drive_strength_for_GPIOE4 v="Low" />
              <Slew_rate_for_GPIOE4 v="Fast" />
              <Drive_strength_for_GPIOE5 v="Low" />
              <Slew_rate_for_GPIOE5 v="Fast" />
              <Drive_strength_for_GPIOE6 v="Low" />
              <Slew_rate_for_GPIOE6 v="Fast" />
              <Drive_strength_for_GPIOE7 v="Low" />
              <Slew_rate_for_GPIOE7 v="Fast" />
            </group>
            <group name="GPIOE_High">
              <Drive_strength_for_GPIOE8 v="Low" />
              <Slew_rate_for_GPIOE8 v="Fast" />
              <Drive_strength_for_GPIOE9 v="Low" />
              <Slew_rate_for_GPIOE9 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOF module (included)" v="1">
          <group name="GPIOF">
            <group name="GPIOF_Low">
              <Drive_strength_for_GPIOF0 v="Low" />
              <Slew_rate_for_GPIOF0 v="Fast" />
              <Drive_strength_for_GPIOF1 v="Low" />
              <Slew_rate_for_GPIOF1 v="Fast" />
              <Drive_strength_for_GPIOF2 v="Low" />
              <Slew_rate_for_GPIOF2 v="Fast" />
              <Drive_strength_for_GPIOF3 v="Low" />
              <Slew_rate_for_GPIOF3 v="Fast" />
              <Drive_strength_for_GPIOF4 v="Low" />
              <Slew_rate_for_GPIOF4 v="Fast" />
              <Drive_strength_for_GPIOF5 v="Low" />
              <Slew_rate_for_GPIOF5 v="Fast" />
              <Drive_strength_for_GPIOF6 v="Low" />
              <Slew_rate_for_GPIOF6 v="Fast" />
              <Drive_strength_for_GPIOF7 v="Low" />
              <Slew_rate_for_GPIOF7 v="Fast" />
            </group>
            <group name="GPIOF_High">
              <Drive_strength_for_GPIOF8 v="Low" />
              <Slew_rate_for_GPIOF8 v="Fast" />
              <Drive_strength_for_GPIOF9 v="Low" />
              <Slew_rate_for_GPIOF9 v="Fast" />
              <Drive_strength_for_GPIOF10 v="Low" />
              <Slew_rate_for_GPIOF10 v="Fast" />
              <Drive_strength_for_GPIOF11 v="Low" />
              <Slew_rate_for_GPIOF11 v="Fast" />
              <Drive_strength_for_GPIOF12 v="Low" />
              <Slew_rate_for_GPIOF12 v="Fast" />
              <Drive_strength_for_GPIOF13 v="Low" />
              <Slew_rate_for_GPIOF13 v="Fast" />
              <Drive_strength_for_GPIOF14 v="Low" />
              <Slew_rate_for_GPIOF14 v="Fast" />
              <Drive_strength_for_GPIOF15 v="Low" />
              <Slew_rate_for_GPIOF15 v="Fast" />
            </group>
          </group>
        </list>
        <list name="GPIOG module (included)" v="1">
          <group name="GPIOG">
            <group name="GPIOG_Low">
              <Drive_strength_for_GPIOG0 v="Low" />
              <Slew_rate_for_GPIOG0 v="Fast" />
              <Drive_strength_for_GPIOG1 v="Low" />
              <Slew_rate_for_GPIOG1 v="Fast" />
              <Drive_strength_for_GPIOG2 v="Low" />
              <Slew_rate_for_GPIOG2 v="Fast" />
              <Drive_strength_for_GPIOG3 v="Low" />
              <Slew_rate_for_GPIOG3 v="Fast" />
              <Drive_strength_for_GPIOG4 v="Low" />
              <Slew_rate_for_GPIOG4 v="Fast" />
              <Drive_strength_for_GPIOG5 v="Low" />
              <Slew_rate_for_GPIOG5 v="Fast" />
              <Drive_strength_for_GPIOG6 v="Low" />
              <Slew_rate_for_GPIOG6 v="Fast" />
              <Drive_strength_for_GPIOG7 v="Low" />
              <Slew_rate_for_GPIOG7 v="Fast" />
            </group>
            <group name="GPIOG_High">
              <Drive_strength_for_GPIOG8 v="Low" />
              <Slew_rate_for_GPIOG8 v="Fast" />
              <Drive_strength_for_GPIOG9 v="Low" />
              <Slew_rate_for_GPIOG9 v="Fast" />
              <Drive_strength_for_GPIOG10 v="Low" />
              <Slew_rate_for_GPIOG10 v="Fast" />
              <Drive_strength_for_GPIOG11 v="Low" />
              <Slew_rate_for_GPIOG11 v="Fast" />
            </group>
          </group>
        </list>
      </group>
      <group name="CPU interrupts">
        <boolgroup name="Interrupt SW0" v="Disabled" />
        <boolgroup name="Interrupt SW1" v="Disabled" />
        <boolgroup name="Interrupt SW2" v="Disabled" />
        <boolgroup name="Interrupt SW3" v="Disabled" />
        <boolgroup name="Interrupt LP" v="Disabled" />
        <boolgroup name="Interrupt PLL" v="Disabled" />
        <boolgroup name="Interrupt LVI" v="Disabled" />
        <boolgroup name="Interrupt Illegal Instruction" v="Disabled" />
        <boolgroup name="Interrupt Misalign Access" v="Disabled" />
        <boolgroup name="Interrupt HW Stack Overflow" v="Disabled" />
        <list name="MCM module (included)" v="1">
          <boolgroup name="Interrupt Core Fault" v="Disabled" />
        </list>
      </group>
      <list name="Enabled speed modes (included)" v="1">
        <group name="Enabled speed modes">
          <boolgroup name="High speed mode" v="Enabled">
            <Input_clock_source_ v="Internal oscillator 8MHz" />
            <Clock_output_divider__Postscaler_ v="Auto select" />
            <System_clock__IP_Bus___MHz_ v="20" />
            <boolgroup name="PLL clock" v="Enabled">
              <PLL_multiplier v="Auto select" />
              <PLL_clock_frequency v="160" />
              <Enable_PLL_after_reset v="yes" />
            </boolgroup>
          </boolgroup>
          <boolgroup name="Low speed mode" v="Disabled" />
          <boolgroup name="Slow speed mode" v="Disabled" />
        </group>
      </list>
    </Properties>
    <Methods>
      <list name="CPUCond0" v="1">
        <SetHighSpeed v="don&amp;apos;t generate code" />
        <SetLowSpeed v="don&amp;apos;t generate code" />
        <SetSlowSpeed v="don&amp;apos;t generate code" />
        <GetSpeedMode v="don&amp;apos;t generate code" />
        <EnableInt v="generate code" />
        <DisableInt v="generate code" />
        <GetResetSource v="don&amp;apos;t generate code" />
        <SetWaitMode v="generate code" />
        <SetStopMode v="generate code" />
        <GetBusFreqHz v="don&amp;apos;t generate code" />
        <OpenBackDoor v="don&amp;apos;t generate code" />
        <SetFlexRAMFunction v="don&amp;apos;t generate code" />
        <SetFlexNVMPartition v="don&amp;apos;t generate code" />
        <InitShadowRegs v="don&amp;apos;t generate code" />
        <Delay100US v="don&amp;apos;t generate code" />
        <EnablePLL v="don&amp;apos;t generate code" />
      </list>
    </Methods>
    <Events>
      <Event_module_name v="Events" />
      <list name="CPUCond" v="1">
        <event name="OnReset" v="don&amp;apos;t generate code" />
        <event name="OnSwINT0" v="don&amp;apos;t generate code" />
        <event name="OnSwINT1" v="don&amp;apos;t generate code" />
        <event name="OnSwINT2" v="don&amp;apos;t generate code" />
        <event name="OnSwINT3" v="don&amp;apos;t generate code" />
        <event name="OnSwINTLP" v="don&amp;apos;t generate code" />
        <event name="OnPLLError" v="don&amp;apos;t generate code" />
        <event name="OnIllegalOpcode" v="don&amp;apos;t generate code" />
        <event name="OnMisalignData" v="don&amp;apos;t generate code" />
        <event name="OnHWStackError" v="don&amp;apos;t generate code" />
        <event name="OnLVI22" v="don&amp;apos;t generate code" />
        <event name="OnLVI27" v="don&amp;apos;t generate code" />
        <event name="OnCoreFault" v="don&amp;apos;t generate code" />
      </list>
    </Events>
    <Compiler v="CodeWarrior DSP C Compiler" />
    <CompilerProperties>
      <Compiler v="CodeWarrior DSP C Compiler" />
      <PESL_support v="yes" />
      <Unhandled_interrupts v="One handler for all" />
      <group name="User initialization">
        <User_data_declarations>
          <StrgList></StrgList>
        </User_data_declarations>
        <User_code_before_PE_initialization>
          <StrgList></StrgList>
        </User_code_before_PE_initialization>
        <User_code_after_PE_initialization>
          <StrgList></StrgList>
        </User_code_after_PE_initialization>
      </group>
      <boolgroup name="Generate debugger files" v="yes">
        <Generate_mem_file v="yes" />
      </boolgroup>
      <boolgroup name="Generate linker file" v="yes">
        <Constants_in_xROM v="no" />
        <xROM_xRAM_mode v="no" />
        <pROM_xRAM_mode v="no" />
        <Stack_size v="512" />
        <Heap_size v="256" />
        <Set_memory_segments_to_default v="Click to set default &amp;gt;" />
        <Default_memory_for_interrupts v="INTERNAL FLASH" />
        <Default_memory_for_code v="INTERNAL FLASH" />
        <Default_memory_for_data v="INTERNAL RAM" />
        <list name="ROM/RAM Areas" v="4">
          <group name="MemoryArea0">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_Interrupts" />
              <Address v="0" />
              <Size v="222" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea1">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_Code" />
              <Address v="520" />
              <Size v="130552" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
          <group name="MemoryArea2">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".x_Data" />
              <Address v="1" />
              <Size v="16383" />
              <Qualifier v="RW" />
            </boolgroup>
          </group>
          <group name="MemoryArea3">
            <boolgroup name="ROM/RAM Area" v="Enabled">
              <Name v=".p_reserved_FCF" />
              <Address v="512" />
              <Size v="8" />
              <Qualifier v="RWX" />
            </boolgroup>
          </group>
        </list>
      </boolgroup>
      <list name="System paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User paths " v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="Libraries" v="0">
        <EmptySection_DummyValue />
      </list>
      <list name="User directories" v="0">
        <EmptySection_DummyValue />
      </list>
    </CompilerProperties>
  </CPU_Bean>
  <Bean name="ASl1" type="AsynchroSlave">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="ASl1" />
      <Channel v="QSCI1" />
      <boolgroup name="Interrupt service/event" v="Enabled">
        <Interrupt_RxD v="INT_QSCI1_RCV" />
        <Interrupt_RxD_priority v="medium priority" />
        <Interrupt_RxD_preserve_registers v="yes" />
        <Interrupt_TxD v="INT_QSCI1_TDRE" />
        <Interrupt_TxD_priority v="medium priority" />
        <Interrupt_TxD_preserve_registers v="yes" />
        <Interrupt_Error v="INT_QSCI1_RERR" />
        <Interrupt_Error_priority v="medium priority" />
        <Interrupt_Error_preserve_registers v="yes" />
        <Interrupt_Idle v="INT_QSCI1_TIDLE" />
        <Interrupt_Idle_priority v="medium priority" />
        <Interrupt_Idle_preserve_registers v="yes" />
        <Input_buffer_size v="120" />
        <Output_buffer_size v="12" />
      </boolgroup>
      <group name="Settings">
        <Parity sel_value="hardware wake-up">
          
wake-up (hw or sw)

          <EmptySection_DummyValue />
        </Parity>
        <Width v="9 bits" />
        <Stop_bit v="1" />
        <enumgroup name="SCI output mode" v="Loop">
          <EmptySection_DummyValue />
        </enumgroup>
        <boolgroup name="Receiver" v="Enabled">
          <RxD v="GPIOC12/CANRX/SDA1/RXD1" />
          <RxD_pin_signal v="" />
        </boolgroup>
        <boolgroup name="Transmitter" v="Enabled">
          <TxD v="GPIOC11/CANTX/SCL1/TXD1" />
          <TxD_pin_signal v="" />
        </boolgroup>
        <Baud_rate v="9600 baud" />
        <Break_signal v="Enabled" />
        <Slave_id v="1" />
        <Wakeup_condition v="Idle line wakeup" />
        <Transmitter_output v="Not Inverted" />
        <Stop_in_wait_mode v="no" />
      </group>
      <group name="Initialization">
        <Enabled_in_init_code v="yes" />
        <Events_enabled_in_init_ v="yes" />
      </group>
      <group name="CPU clock/speed selection">
        <High_speed_mode v="This component enabled" />
        <Low_speed_mode v="This component disabled" />
        <Slow_speed_mode v="This component disabled" />
      </group>
    </Properties>
    <Methods>
      <Enable v="don&amp;apos;t generate code" />
      <Disable v="don&amp;apos;t generate code" />
      <EnableEvent v="don&amp;apos;t generate code" />
      <DisableEvent v="don&amp;apos;t generate code" />
      <RecvChar v="generate code" />
      <SendChar v="generate code" />
      <RecvBlock v="generate code" />
      <SendBlock v="generate code" />
      <ClearRxBuf v="generate code" />
      <ClearTxBuf v="generate code" />
      <CharsInRxBuf v="don&amp;apos;t generate code" />
      <GetCharsInRxBuf v="generate code" />
      <CharsInTxBuf v="don&amp;apos;t generate code" />
      <GetCharsInTxBuf v="generate code" />
      <GetError v="don&amp;apos;t generate code" />
      <GetBreak v="generate code" />
      <SetBreak v="generate code" />
      <Selected v="generate code" />
      <TurnTxOn v="don&amp;apos;t generate code" />
      <TurnTxOff v="don&amp;apos;t generate code" />
      <TurnRxOn v="don&amp;apos;t generate code" />
      <TurnRxOff v="don&amp;apos;t generate code" />
      <LoopMode v="don&amp;apos;t generate code" />
      <SetIdle v="don&amp;apos;t generate code" />
      <ConnectPin v="don&amp;apos;t generate code" />
      <GetRxIdle v="don&amp;apos;t generate code" />
      <GetTxComplete v="don&amp;apos;t generate code" />
    </Methods>
    <Events>
      <Event_module_name v="Events" />
      <event name="BeforeNewSpeed" v="don&amp;apos;t generate code" />
      <event name="AfterNewSpeed" v="don&amp;apos;t generate code" />
      <event name="OnError" v="don&amp;apos;t generate code" />
      <event name="OnRxChar" v="generate code">
        <Event_procedure_name v="ASl1_OnRxChar" />
        <Priority v="same as interrupt" />
      </event>
      <event name="OnRxCharExt" v="don&amp;apos;t generate code" />
      <event name="OnTxChar" v="generate code">
        <Event_procedure_name v="ASl1_OnTxChar" />
        <Priority v="same as interrupt" />
      </event>
      <event name="OnFullRxBuf" v="don&amp;apos;t generate code" />
      <event name="OnFreeTxBuf" v="generate code">
        <Event_procedure_name v="ASl1_OnFreeTxBuf" />
        <Priority v="same as interrupt" />
      </event>
      <event name="OnBreak" v="generate code">
        <Event_procedure_name v="ASl1_OnBreak" />
        <Priority v="same as interrupt" />
      </event>
      <event name="OnSelect" v="don&amp;apos;t generate code" />
      <event name="OnUnselect" v="don&amp;apos;t generate code" />
      <event name="OnTxComplete" v="don&amp;apos;t generate code" />
    </Events>
  </Bean>
  <Bean name="TEST1" type="DSP_Test">
    <Enabled v="Y" />
    <Properties>
      <Component_name v="TEST1" />
      <Max__len__of_Test_Name v="60" />
    </Properties>
    <Methods>
      <testStart v="generate code" />
      <testFailed v="generate code" />
      <testComment v="generate code" />
      <testEnd v="generate code" />
    </Methods>
    <Events>
      <EmptySection_DummyValue />
    </Events>
  </Bean>
</PE_PROJECT_SETTINGS_DOCUMENTATION>

