=============================================================================
List of generated methods in project: ProcessorExpert

THIS TEXT DESCRIPTION IS GENERATED BY THE TOOL. DO NOT MODIFY IT.
=============================================================================

Module "IFsh1"     (component IntFLASH)
   - IFsh1_DisableEvent -This method disables all the events except <OnSaveBuffer>, <OnRestoreBuffer> and <OnEraseError>. The 
                method is available only if any event is enabled.
   - IFsh1_EnableEvent -This method enables all the events except <OnSaveBuffer>, <OnRestoreBuffer> and <OnEraseError>. The 
                method is available only if any event is enabled.
   - IFsh1_Busy -This method returns the status of the FLASH device. The method may be required and called from another 
                component methods - in this case it cannot be disabled.
   - IFsh1_EraseSector -Erases the sector to which address Addr belongs.
   - IFsh1_SetByteFlash -Writes a byte to an address in FLASH. The operation of this method depends on the "Write method" 
                property and state of the flash. Please see more details on general info page of the help.
   - IFsh1_SetWordFlash -Writes a word to an address in FLASH. The operation of this method depends on the "Write method" 
                property and state of the flash. Please see more details on general info page of the help.
   - IFsh1_GetWordFlash -Gets a word from an address in FLASH.
   - IFsh1_DataPtr2Addr -This method converts data pointer to format of a component's method address parameter. Generally a 
                data pointer format is different from format of a method Addr parameter.
   - IFsh1_FuncPtr2Addr -This method converts function pointer to format of a component's method address parameter. Generally a 
                function pointer format is different from format of a method Addr parameter.

Module "TEST1"     (component DSP_Test)
   - TEST1_testStart -The testStart function initializes the test_sRec data structure
   - TEST1_testFailed -The testFailed function indicates that one step of the test case has failed. The string pointed to by 
                pMsg denotes the cause of the failure.
   - TEST1_testComment -The testComment function records information about the current test. The testComment is independent on 
                the test result (if it fails or not).
   - TEST1_testEnd -The testEnd function declares the end of the test and determines whether the test case has passed or failed.
                If no call had been made to testFailed since testStart was called, the test case passes. If any call to 
                testFailed had been made, the test case fails.

Module "Cpu"       (component MC56F84789VLL)
   - Cpu_EnableInt -Enables all maskable interrupts
   - Cpu_DisableInt -Disables all maskable interrupts
   - Cpu_SetWaitMode -Sets low power mode - Wait mode.   For more information about the wait mode see this CPU documentation.   
                Release from wait mode: Reset or interrupt
   - Cpu_SetStopMode -Sets low power mode - Stop mode.   For more information about the stop mode see this CPU documentation.

===================================================================================
