# Static Call Graph for image .\obj\bootloader.axf

#<CALLGRAPH># ARM Linker, 5.02 [Build 28]: Last Updated: Thu Feb 07 10:34:53 2013

### Maximum Stack Usage = 88 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

USB_EndPoint2 ⇒ MSC_BulkOut ⇒ MSC_GetCBW ⇒ MSC_Inquiry ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BOD_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BusFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CANActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CAN_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DMA_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DebugMon_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - ENET_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - HardFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2S_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MemManage_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - NMI_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PWM1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PendSV_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - QEI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RIT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RTC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - Reset_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SPI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SVC_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SysTick_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USBActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USB_EndPoint0 from usbcore.o(.text) referenced from usbuser.o(.constdata)
  - USB_EndPoint2 from usbuser.o(.text) referenced from usbuser.o(.constdata)
  - USB_IRQHandler from usbhw.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UsageFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - WDT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_lpc17xx.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ enter_usb_isp ⇒ USB_Init ⇒ USB_SetAddress
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  boot_jump (Thumb, 8 bytes, Stack size 0 bytes, sbl_iap.o(.emb_text))
  [Called By]

  - >> execute_user_code

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_lpc17xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  USB_Reset_Event (Thumb, 4 bytes, Stack size 0 bytes, usbuser.o(.text))
  [Calls]

  - >> USB_ResetCore
  [Called By]
  - >> USB_IRQHandler

  USB_Suspend_Event (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text))
  [Called By]

  - >> USB_IRQHandler

  USB_Resume_Event (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text))
  [Called By]

  - >> USB_IRQHandler

  USB_Configure_Event (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text))
  [Called By]

  - >> USB_EndPoint0

  USB_EndPoint1 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint2 (Thumb, 18 bytes, Stack size 0 bytes, usbuser.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = USB_EndPoint2 ⇒ MSC_BulkOut ⇒ MSC_GetCBW ⇒ MSC_Inquiry ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> MSC_BulkOut
  - >> MSC_BulkIn
  [Address Reference Count : 1]
  - usbuser.o(.constdata)

  USB_EndPoint3 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint4 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint5 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint6 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint7 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint8 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint9 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint10 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint11 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint12 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint13 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint14 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  USB_EndPoint15 (Thumb, 2 bytes, Stack size 0 bytes, usbuser.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  USB_GetDescriptor (Thumb, 104 bytes, Stack size 8 bytes, usbcore.o(i.USB_GetDescriptor))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_GetDescriptor ⇒ USB_DataInStage ⇒ USB_WriteEP
  [Calls]
  - >> USB_DataInStage
  [Called By]
  - >> USB_EndPoint0

  SystemInit (Thumb, 336 bytes, Stack size 16 bytes, system_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit
  [Called By]
  - >> enter_usb_isp

  MSC_Reset (Thumb, 10 bytes, Stack size 0 bytes, mscuser.o(.text), UNUSED)

  MSC_GetMaxLUN (Thumb, 10 bytes, Stack size 0 bytes, mscuser.o(.text), UNUSED)

  translate_rd (Thumb, 142 bytes, Stack size 20 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = translate_rd
  [Called By]
  - >> MSC_MemoryRead

  MSC_MemoryRead (Thumb, 106 bytes, Stack size 16 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = MSC_MemoryRead ⇒ translate_rd
  [Calls]
  - >> USB_WriteEP
  - >> translate_rd
  [Called By]
  - >> MSC_BulkIn
  - >> MSC_GetCBW

  MSC_SetCSW (Thumb, 26 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_WriteEP
  [Called By]
  - >> MSC_BulkOut
  - >> MSC_BulkIn
  - >> MSC_GetCBW
  - >> MSC_TestUnitReady
  - >> DataInFormat
  - >> MSC_RWSetup
  - >> MSC_MemoryVerify
  - >> MSC_MemoryWrite

  translate_wr (Thumb, 130 bytes, Stack size 40 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = translate_wr ⇒ write_flash ⇒ find_erase_prepare_sector
  [Calls]
  - >> write_flash
  - >> erase_user_flash
  [Called By]
  - >> MSC_MemoryWrite

  MSC_MemoryWrite (Thumb, 100 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = MSC_MemoryWrite ⇒ translate_wr ⇒ write_flash ⇒ find_erase_prepare_sector
  [Calls]
  - >> USB_SetStallEP
  - >> translate_wr
  - >> MSC_SetCSW
  [Called By]
  - >> MSC_BulkOut

  MSC_MemoryVerify (Thumb, 136 bytes, Stack size 24 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MSC_MemoryVerify ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_SetStallEP
  - >> MSC_SetCSW
  [Called By]
  - >> MSC_BulkOut

  MSC_RWSetup (Thumb, 72 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MSC_RWSetup ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_SetStallEP
  - >> MSC_SetCSW
  [Called By]
  - >> MSC_GetCBW

  DataInFormat (Thumb, 42 bytes, Stack size 16 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_SetStallEP
  - >> MSC_SetCSW
  [Called By]
  - >> MSC_ReadFormatCapacity
  - >> MSC_ReadCapacity
  - >> MSC_ModeSense10
  - >> MSC_ModeSense6
  - >> MSC_Inquiry
  - >> MSC_RequestSense

  DataInTransfer (Thumb, 52 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DataInTransfer ⇒ USB_WriteEP
  [Calls]
  - >> USB_WriteEP
  [Called By]
  - >> MSC_ReadFormatCapacity
  - >> MSC_ReadCapacity
  - >> MSC_ModeSense10
  - >> MSC_ModeSense6
  - >> MSC_Inquiry
  - >> MSC_RequestSense

  MSC_TestUnitReady (Thumb, 40 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MSC_TestUnitReady ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_SetStallEP
  - >> MSC_SetCSW
  [Called By]
  - >> MSC_GetCBW

  MSC_RequestSense (Thumb, 76 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MSC_RequestSense ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> DataInTransfer
  - >> DataInFormat
  [Called By]
  - >> MSC_GetCBW

  MSC_Inquiry (Thumb, 190 bytes, Stack size 16 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = MSC_Inquiry ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> DataInTransfer
  - >> DataInFormat
  [Called By]
  - >> MSC_GetCBW

  MSC_ModeSense6 (Thumb, 38 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MSC_ModeSense6 ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> DataInTransfer
  - >> DataInFormat
  [Called By]
  - >> MSC_GetCBW

  MSC_ModeSense10 (Thumb, 46 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MSC_ModeSense10 ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> DataInTransfer
  - >> DataInFormat
  [Called By]
  - >> MSC_GetCBW

  MSC_ReadCapacity (Thumb, 74 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MSC_ReadCapacity ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> DataInTransfer
  - >> DataInFormat
  [Called By]
  - >> MSC_GetCBW

  MSC_ReadFormatCapacity (Thumb, 80 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MSC_ReadFormatCapacity ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> DataInTransfer
  - >> DataInFormat
  [Called By]
  - >> MSC_GetCBW

  MSC_GetCBW (Thumb, 282 bytes, Stack size 24 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = MSC_GetCBW ⇒ MSC_Inquiry ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_SetStallEP
  - >> MSC_ReadFormatCapacity
  - >> MSC_ReadCapacity
  - >> MSC_ModeSense10
  - >> MSC_ModeSense6
  - >> MSC_Inquiry
  - >> MSC_RequestSense
  - >> MSC_TestUnitReady
  - >> MSC_RWSetup
  - >> MSC_SetCSW
  - >> MSC_MemoryRead
  [Called By]
  - >> MSC_BulkOut

  MSC_BulkIn (Thumb, 58 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = MSC_BulkIn ⇒ MSC_MemoryRead ⇒ translate_rd
  [Calls]
  - >> USB_SetStallEP
  - >> MSC_SetCSW
  - >> MSC_MemoryRead
  [Called By]
  - >> USB_EndPoint2

  MSC_BulkOut (Thumb, 76 bytes, Stack size 8 bytes, mscuser.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = MSC_BulkOut ⇒ MSC_GetCBW ⇒ MSC_Inquiry ⇒ DataInFormat ⇒ MSC_SetCSW ⇒ USB_WriteEP
  [Calls]
  - >> USB_SetStallEP
  - >> USB_ReadEP
  - >> MSC_GetCBW
  - >> MSC_MemoryVerify
  - >> MSC_MemoryWrite
  - >> MSC_SetCSW
  [Called By]
  - >> USB_EndPoint2

  USB_ResetCore (Thumb, 20 bytes, Stack size 0 bytes, usbcore.o(.text))
  [Called By]

  - >> USB_Reset_Event

  USB_SetupStage (Thumb, 10 bytes, Stack size 0 bytes, usbcore.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_SetupStage ⇒ USB_ReadEP
  [Calls]
  - >> USB_ReadEP
  [Called By]
  - >> USB_EndPoint0

  USB_DataInStage (Thumb, 36 bytes, Stack size 8 bytes, usbcore.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DataInStage ⇒ USB_WriteEP
  [Calls]
  - >> USB_WriteEP
  [Called By]
  - >> USB_GetStatus
  - >> USB_GetDescriptor
  - >> USB_EndPoint0

  USB_DataOutStage (Thumb, 28 bytes, Stack size 8 bytes, usbcore.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DataOutStage ⇒ USB_ReadEP
  [Calls]
  - >> USB_ReadEP
  [Called By]
  - >> USB_EndPoint0

  USB_StatusInStage (Thumb, 10 bytes, Stack size 0 bytes, usbcore.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_StatusInStage ⇒ USB_WriteEP
  [Calls]
  - >> USB_WriteEP
  [Called By]
  - >> USB_EndPoint0

  USB_StatusOutStage (Thumb, 8 bytes, Stack size 0 bytes, usbcore.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_StatusOutStage ⇒ USB_ReadEP
  [Calls]
  - >> USB_ReadEP
  [Called By]
  - >> USB_EndPoint0

  USB_EndPoint0 (Thumb, 298 bytes, Stack size 24 bytes, usbcore.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USB_EndPoint0 ⇒ USB_SetInterface ⇒ USB_ConfigEP
  [Calls]
  - >> USB_SetAddress
  - >> USB_DirCtrlEP
  - >> USB_Configure_Event
  - >> USB_ClrStallEP
  - >> USB_SetInterface
  - >> USB_SetConfiguration
  - >> USB_SetClrFeature
  - >> USB_GetStatus
  - >> USB_GetDescriptor
  - >> USB_StatusOutStage
  - >> USB_StatusInStage
  - >> USB_DataOutStage
  - >> USB_DataInStage
  - >> USB_SetupStage
  - >> USB_SetStallEP
  [Address Reference Count : 1]
  - usbuser.o(.constdata)

  EPAdr (Thumb, 18 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_ResetEP
  - >> USB_EnableEP
  - >> USB_DisableEP
  - >> USB_ConfigEP
  - >> USB_ClrStallEP
  - >> USB_WriteEP
  - >> USB_SetStallEP
  - >> USB_ReadEP

  WrCmd (Thumb, 24 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_IRQHandler
  - >> USB_GetFrame
  - >> USB_WriteEP
  - >> USB_ReadEP

  WrCmdDat (Thumb, 40 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_WakeUp
  - >> USB_Connect
  - >> USB_SetAddress
  - >> USB_ResetEP
  - >> USB_EnableEP
  - >> USB_DisableEP
  - >> USB_Configure
  - >> USB_ClrStallEP
  - >> USB_SetStallEP

  RdCmdDat (Thumb, 28 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_IRQHandler
  - >> USB_GetFrame

  USB_SetAddress (Thumb, 28 bytes, Stack size 12 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_SetAddress
  [Calls]
  - >> WrCmdDat
  [Called By]
  - >> USB_Init
  - >> USB_EndPoint0

  USB_Reset (Thumb, 50 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_IRQHandler
  - >> USB_Init

  USB_Init (Thumb, 88 bytes, Stack size 4 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_Init ⇒ USB_SetAddress
  [Calls]
  - >> USB_Reset
  - >> USB_SetAddress
  [Called By]
  - >> enter_usb_isp

  USB_Connect (Thumb, 16 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Calls]

  - >> WrCmdDat
  [Called By]
  - >> enter_usb_isp

  USB_Suspend (Thumb, 2 bytes, Stack size 0 bytes, usbhw.o(.text), UNUSED)

  USB_Resume (Thumb, 2 bytes, Stack size 0 bytes, usbhw.o(.text), UNUSED)

  USB_WakeUp (Thumb, 16 bytes, Stack size 0 bytes, usbhw.o(.text), UNUSED)
  [Calls]

  - >> WrCmdDat

  USB_WakeUpCfg (Thumb, 2 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_SetClrFeature

  USB_Configure (Thumb, 44 bytes, Stack size 8 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_Configure
  [Calls]
  - >> WrCmdDat
  [Called By]
  - >> USB_SetConfiguration

  USB_ConfigEP (Thumb, 56 bytes, Stack size 8 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_ConfigEP
  [Calls]
  - >> EPAdr
  [Called By]
  - >> USB_SetInterface
  - >> USB_SetConfiguration

  USB_DirCtrlEP (Thumb, 2 bytes, Stack size 0 bytes, usbhw.o(.text))
  [Called By]

  - >> USB_EndPoint0

  USB_EnableEP (Thumb, 20 bytes, Stack size 4 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = USB_EnableEP
  [Calls]
  - >> WrCmdDat
  - >> EPAdr
  [Called By]
  - >> USB_SetInterface
  - >> USB_SetConfiguration

  USB_DisableEP (Thumb, 20 bytes, Stack size 4 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = USB_DisableEP
  [Calls]
  - >> WrCmdDat
  - >> EPAdr
  [Called By]
  - >> USB_SetInterface
  - >> USB_SetConfiguration

  USB_ResetEP (Thumb, 20 bytes, Stack size 4 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = USB_ResetEP
  [Calls]
  - >> WrCmdDat
  - >> EPAdr
  [Called By]
  - >> USB_SetInterface
  - >> USB_SetConfiguration

  USB_SetStallEP (Thumb, 20 bytes, Stack size 4 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = USB_SetStallEP
  [Calls]
  - >> WrCmdDat
  - >> EPAdr
  [Called By]
  - >> USB_SetClrFeature
  - >> USB_EndPoint0
  - >> MSC_BulkOut
  - >> MSC_BulkIn
  - >> MSC_GetCBW
  - >> MSC_TestUnitReady
  - >> DataInFormat
  - >> MSC_RWSetup
  - >> MSC_MemoryVerify
  - >> MSC_MemoryWrite

  USB_ClrStallEP (Thumb, 20 bytes, Stack size 4 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = USB_ClrStallEP
  [Calls]
  - >> WrCmdDat
  - >> EPAdr
  [Called By]
  - >> USB_SetClrFeature
  - >> USB_EndPoint0

  USB_ReadEP (Thumb, 98 bytes, Stack size 16 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_ReadEP
  [Calls]
  - >> WrCmd
  - >> EPAdr
  [Called By]
  - >> USB_StatusOutStage
  - >> USB_DataOutStage
  - >> USB_SetupStage
  - >> MSC_BulkOut

  USB_WriteEP (Thumb, 84 bytes, Stack size 16 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_WriteEP
  [Calls]
  - >> WrCmd
  - >> EPAdr
  [Called By]
  - >> USB_StatusInStage
  - >> USB_DataInStage
  - >> DataInTransfer
  - >> MSC_SetCSW
  - >> MSC_MemoryRead

  USB_GetFrame (Thumb, 30 bytes, Stack size 8 bytes, usbhw.o(.text), UNUSED)
  [Calls]

  - >> RdCmdDat
  - >> WrCmd

  USB_IRQHandler (Thumb, 186 bytes, Stack size 24 bytes, usbhw.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_IRQHandler
  [Calls]
  - >> USB_Suspend_Event
  - >> USB_Resume_Event
  - >> USB_Reset_Event
  - >> USB_Reset
  - >> RdCmdDat
  - >> WrCmd
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  enable_interrupts (Thumb, 4 bytes, Stack size 0 bytes, sbl_iap.o(.text), UNUSED)

  iap_entry (Thumb, 4 bytes, Stack size 0 bytes, sbl_iap.o(.text))
  [Called By]

  - >> user_code_present
  - >> erase_sector
  - >> prepare_sector
  - >> write_data

  disable_interrupts (Thumb, 4 bytes, Stack size 0 bytes, sbl_iap.o(.text), UNUSED)

  write_data (Thumb, 46 bytes, Stack size 8 bytes, sbl_iap.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = write_data
  [Calls]
  - >> iap_entry
  [Called By]
  - >> write_flash

  prepare_sector (Thumb, 32 bytes, Stack size 0 bytes, sbl_iap.o(.text))
  [Calls]

  - >> iap_entry
  [Called By]
  - >> find_erase_prepare_sector
  - >> erase_user_flash

  erase_sector (Thumb, 32 bytes, Stack size 0 bytes, sbl_iap.o(.text))
  [Calls]

  - >> iap_entry
  [Called By]
  - >> find_erase_prepare_sector
  - >> erase_user_flash

  find_erase_prepare_sector (Thumb, 66 bytes, Stack size 8 bytes, sbl_iap.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = find_erase_prepare_sector
  [Calls]
  - >> erase_sector
  - >> prepare_sector
  [Called By]
  - >> write_flash

  write_flash (Thumb, 92 bytes, Stack size 24 bytes, sbl_iap.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = write_flash ⇒ find_erase_prepare_sector
  [Calls]
  - >> find_erase_prepare_sector
  - >> write_data
  [Called By]
  - >> translate_wr

  execute_user_code (Thumb, 12 bytes, Stack size 0 bytes, sbl_iap.o(.text))
  [Calls]

  - >> boot_jump
  [Called By]
  - >> main
  - >> check_isp_entry_pin

  user_code_present (Thumb, 36 bytes, Stack size 8 bytes, sbl_iap.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = user_code_present
  [Calls]
  - >> iap_entry
  [Called By]
  - >> main

  check_isp_entry_pin (Thumb, 12 bytes, Stack size 0 bytes, sbl_iap.o(.text))
  [Calls]

  - >> execute_user_code
  [Called By]
  - >> main

  erase_user_flash (Thumb, 32 bytes, Stack size 8 bytes, sbl_iap.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = erase_user_flash
  [Calls]
  - >> erase_sector
  - >> prepare_sector
  [Called By]
  - >> translate_wr

  Prepare_Zero (Thumb, 14 bytes, Stack size 0 bytes, memory.o(.text), UNUSED)

  Prepare_Copy (Thumb, 18 bytes, Stack size 0 bytes, memory.o(.text), UNUSED)

  enter_usb_isp (Thumb, 254 bytes, Stack size 0 bytes, memory.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = enter_usb_isp ⇒ USB_Init ⇒ USB_SetAddress
  [Calls]
  - >> USB_Connect
  - >> USB_Init
  - >> SystemInit
  [Called By]
  - >> main

  main (Thumb, 34 bytes, Stack size 0 bytes, memory.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = main ⇒ enter_usb_isp ⇒ USB_Init ⇒ USB_SetAddress
  [Calls]
  - >> enter_usb_isp
  - >> check_isp_entry_pin
  - >> user_code_present
  - >> execute_user_code
  [Called By]
  - >> __rt_entry_main

  USB_GetStatus (Thumb, 120 bytes, Stack size 16 bytes, usbcore.o(i.USB_GetStatus))
  [Stack]

  - Max Depth = 40
  - Call Chain = USB_GetStatus ⇒ USB_DataInStage ⇒ USB_WriteEP
  [Calls]
  - >> USB_DataInStage
  [Called By]
  - >> USB_EndPoint0

  USB_SetClrFeature (Thumb, 140 bytes, Stack size 16 bytes, usbcore.o(i.USB_SetClrFeature))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_SetClrFeature ⇒ USB_ClrStallEP
  [Calls]
  - >> USB_WakeUpCfg
  - >> USB_ClrStallEP
  - >> USB_SetStallEP
  [Called By]
  - >> USB_EndPoint0

  USB_SetConfiguration (Thumb, 324 bytes, Stack size 40 bytes, usbcore.o(i.USB_SetConfiguration))
  [Stack]

  - Max Depth = 48
  - Call Chain = USB_SetConfiguration ⇒ USB_Configure
  [Calls]
  - >> USB_ResetEP
  - >> USB_EnableEP
  - >> USB_DisableEP
  - >> USB_Configure
  - >> USB_ConfigEP
  [Called By]
  - >> USB_EndPoint0

  USB_SetInterface (Thumb, 226 bytes, Stack size 48 bytes, usbcore.o(i.USB_SetInterface))
  [Stack]

  - Max Depth = 56
  - Call Chain = USB_SetInterface ⇒ USB_ConfigEP
  [Calls]
  - >> USB_ResetEP
  - >> USB_EnableEP
  - >> USB_DisableEP
  - >> USB_ConfigEP
  [Called By]
  - >> USB_EndPoint0

  ### Local Symbols

  ### Undefined Global Symbols