The project is a demo program for the Keil MCB11U10 Board 
using a NXP LPC11Uxx Microcontroller.

Example functionality: 
 - Clock Settings:
   - XTAL                   = 12 MHz
   - processor clock = CCLK = 48 MHz
   - USB clock              = 48 MHz
   
It demonstrates an USB Composite Device(DFU+HID).

The USB HID is recognized by the host PC running Windows
which will load generic HID driver. 
The board LEDs and Push Buttons(S3 and S4) can then be accessed 
from the PC through a custom HID Client Program(HIDClient.exe).
For DFU, install the driver in \USBClass\DFU\Driver

Note: J1-ON, J2-ON, J4-23


