# Static Call Graph for image .\RAM\Demo.axf

#<CALLGRAPH># ARM Linker, 5.02 [Build 28]: Last Updated: Mon May 20 14:17:58 2013

### Maximum Stack Usage = 128 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemInit ⇒ SystemInit_ExtMemCtl ⇒ WaitUs ⇒ __aeabi_uldivmod

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC0_IRQHandler ⇒ ADC0_IRQHandler

  ### Function Pointers

  - ADC0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - ADC1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - ATIMER_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - BusFault_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - CAN0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - CAN1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - DAC_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - DMA_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - DebugMon_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - ETH_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - EVRT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - EZH_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - FLASH_EEPROM_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GINT0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GINT1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO2_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO3_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO4_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO5_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO6_IRQHandler from sgpcamdemo.o(SECT_RAMCODE) referenced from startup_lpc43xx.o(RESET)
  - GPIO7_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - HardFault_Handler from sgpcamdemo.o(i.HardFault_Handler) referenced from startup_lpc43xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2S0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2S1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - LCD_IRQHandler from sgpcamdemo.o(i.LCD_IRQHandler) referenced from startup_lpc43xx.o(RESET)
  - M0CORE_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - M0s_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - MemManage_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - NMI_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - PendSV_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - QEI_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - RIT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - RTC_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - Reset_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SCT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SDIO_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SGPIO_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SPIFI_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SPI_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SVC_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SysTick_Handler from sgpcamdemo.o(i.SysTick_Handler) referenced from startup_lpc43xx.o(RESET)
  - TIMER0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART2_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART3_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - USB0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - USB1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UsageFault_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - VADC_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - WDT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc43xx.o(.text)
  - main from sgpcamdemo.o(i.main) referenced from entry8.o(.ARM.Collect$$$$00000009)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry8.o(.ARM.Collect$$$$00000009))

  __asm___18_LCDRfrsh_MCB4300_c_dee28309____REV16 (Thumb, 4 bytes, Stack size 0 bytes, lcdrfrsh_mcb4300.o(.emb_text), UNUSED)

  __asm___18_LCDRfrsh_MCB4300_c_dee28309____REVSH (Thumb, 4 bytes, Stack size 0 bytes, lcdrfrsh_mcb4300.o(.emb_text), UNUSED)

  __asm___18_LCDRfrsh_MCB4300_c_dee28309__SwapBytePairSIDD (Thumb, 4 bytes, Stack size 0 bytes, lcdrfrsh_mcb4300.o(.emb_text))
  [Called By]

  - >> OV7670RefreshGray
  - >> OV7670RefreshColor

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> ADC0_IRQHandler
  [Called By]
  - >> ADC0_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  ATIMER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  CAN0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  CAN1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  EVRT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  EZH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  FLASH_EEPROM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2S0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2S1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  M0CORE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  M0s_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SGPIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SPIFI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  USB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  USB1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  VADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  getPC (Thumb, 4 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Called By]

  - >> SystemInit

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> SystemInit_ExtMemCtl
  - >> WaitUs

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> IPC_DownloadM0Image

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> CamInit

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  GPIO6_IRQHandler (Thumb, 160 bytes, Stack size 8 bytes, sgpcamdemo.o(SECT_RAMCODE))
  [Stack]

  - Max Depth = 16
  - Call Chain = GPIO6_IRQHandler ⇒ SGPStop
  [Calls]
  - >> __set_PRIMASK
  - >> SGPStop
  - >> SGPGetRdyToGo
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  OV7670RefreshColor (Thumb, 208 bytes, Stack size 48 bytes, lcdrfrsh_mcb4300.o(SECT_RAMCODE))
  [Stack]

  - Max Depth = 64
  - Call Chain = OV7670RefreshColor ⇒ FBQ_GetProduceIndex
  [Calls]
  - >> FBQ_ProduceDone
  - >> FBQ_GetProduceIndex
  - >> __asm___18_LCDRfrsh_MCB4300_c_dee28309__SwapBytePairSIDD
  [Called By]
  - >> VideoRefresh

  OV7670RefreshGray (Thumb, 142 bytes, Stack size 40 bytes, lcdrfrsh_mcb4300.o(SECT_RAMCODE), UNUSED)
  [Calls]

  - >> FBQ_GetProduceIndex
  - >> __asm___18_LCDRfrsh_MCB4300_c_dee28309__SwapBytePairSIDD

  CGUOutMCLKInit (Thumb, 40 bytes, Stack size 0 bytes, cam_ov7670.o(i.CGUOutMCLKInit))
  [Called By]

  - >> CamInit

  CamInit (Thumb, 158 bytes, Stack size 16 bytes, cam_ov7670.o(i.CamInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = CamInit ⇒ SetupSGPIO ⇒ NVIC_SetPriority
  [Calls]
  - >> __aeabi_memclr4
  - >> ov7670_read_reg
  - >> VSyncIrqInit
  - >> SetupSGPIO
  - >> OV7670RegInit
  - >> DelayTicks
  - >> CGUOutMCLKInit
  - >> NVIC_SetPriority
  - >> NVIC_DisableIRQ
  - >> I2CForOv7670_Init
  - >> PinInit
  [Called By]
  - >> main

  DelayTicks (Thumb, 18 bytes, Stack size 0 bytes, cam_ov7670.o(i.DelayTicks))
  [Called By]

  - >> CamInit

  FBQ_ConsumeDone (Thumb, 70 bytes, Stack size 8 bytes, frabufq.o(i.FBQ_ConsumeDone))
  [Stack]

  - Max Depth = 8
  - Call Chain = FBQ_ConsumeDone
  [Calls]
  - >> __set_PRIMASK
  [Called By]
  - >> LCD_IRQHandler

  FBQ_GetConsumeIndex (Thumb, 60 bytes, Stack size 16 bytes, frabufq.o(i.FBQ_GetConsumeIndex))
  [Stack]

  - Max Depth = 16
  - Call Chain = FBQ_GetConsumeIndex
  [Calls]
  - >> __set_PRIMASK
  [Called By]
  - >> LCD_IRQHandler

  FBQ_GetProduceIndex (Thumb, 66 bytes, Stack size 16 bytes, frabufq.o(i.FBQ_GetProduceIndex))
  [Stack]

  - Max Depth = 16
  - Call Chain = FBQ_GetProduceIndex
  [Calls]
  - >> __set_PRIMASK
  [Called By]
  - >> OV7670RefreshGray
  - >> OV7670RefreshColor

  FBQ_Init (Thumb, 78 bytes, Stack size 0 bytes, frabufq.o(i.FBQ_Init))
  [Called By]

  - >> main

  FBQ_IsFull (Thumb, 20 bytes, Stack size 0 bytes, frabufq.o(i.FBQ_IsFull))
  [Called By]

  - >> main

  FBQ_ProduceDone (Thumb, 76 bytes, Stack size 8 bytes, frabufq.o(i.FBQ_ProduceDone))
  [Stack]

  - Max Depth = 8
  - Call Chain = FBQ_ProduceDone
  [Calls]
  - >> __set_PRIMASK
  [Called By]
  - >> OV7670RefreshColor

  GLCD_Clear (Thumb, 24 bytes, Stack size 0 bytes, glcd_lpc43xx.o(i.GLCD_Clear))
  [Called By]

  - >> main

  GLCD_DisplayChar (Thumb, 84 bytes, Stack size 24 bytes, glcd_lpc43xx.o(i.GLCD_DisplayChar))
  [Stack]

  - Max Depth = 56
  - Call Chain = GLCD_DisplayChar ⇒ GLCD_DrawChar
  [Calls]
  - >> GLCD_DrawChar
  [Called By]
  - >> GLCD_DisplayString

  GLCD_DisplayString (Thumb, 36 bytes, Stack size 20 bytes, glcd_lpc43xx.o(i.GLCD_DisplayString))
  [Stack]

  - Max Depth = 76
  - Call Chain = GLCD_DisplayString ⇒ GLCD_DisplayChar ⇒ GLCD_DrawChar
  [Calls]
  - >> GLCD_DisplayChar
  [Called By]
  - >> main

  GLCD_DrawChar (Thumb, 174 bytes, Stack size 32 bytes, glcd_lpc43xx.o(i.GLCD_DrawChar))
  [Stack]

  - Max Depth = 32
  - Call Chain = GLCD_DrawChar
  [Called By]
  - >> GLCD_DisplayChar

  GLCD_Init (Thumb, 902 bytes, Stack size 8 bytes, glcd_lpc43xx.o(i.GLCD_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = GLCD_Init ⇒ wr_reg ⇒ wr_cmd
  [Calls]
  - >> wr_reg
  - >> delay
  [Called By]
  - >> main

  GLCD_SetBackColor (Thumb, 6 bytes, Stack size 0 bytes, glcd_lpc43xx.o(i.GLCD_SetBackColor))
  [Called By]

  - >> main

  GLCD_SetTextColor (Thumb, 6 bytes, Stack size 0 bytes, glcd_lpc43xx.o(i.GLCD_SetTextColor))
  [Called By]

  - >> main

  GetClkSel (Thumb, 170 bytes, Stack size 8 bytes, system_lpc43xx.o(i.GetClkSel))
  [Stack]

  - Max Depth = 8
  - Call Chain = GetClkSel
  [Called By]
  - >> GetClockFreq

  GetClockFreq (Thumb, 196 bytes, Stack size 32 bytes, system_lpc43xx.o(i.GetClockFreq))
  [Stack]

  - Max Depth = 44
  - Call Chain = GetClockFreq ⇒ GetPLL1Param
  [Calls]
  - >> GetPLL1Param
  - >> GetClkSel
  [Called By]
  - >> SystemCoreClockUpdate

  GetPLL1Param (Thumb, 68 bytes, Stack size 12 bytes, system_lpc43xx.o(i.GetPLL1Param))
  [Stack]

  - Max Depth = 12
  - Call Chain = GetPLL1Param
  [Called By]
  - >> GetClockFreq

  HardFault_Handler (Thumb, 50 bytes, Stack size 0 bytes, sgpcamdemo.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2CForOv7670_Start (Thumb, 18 bytes, Stack size 8 bytes, cam_ov7670.o(i.I2CForOv7670_Start))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2CForOv7670_Start
  [Calls]
  - >> WaitStart
  [Called By]
  - >> ov7670_write_reg
  - >> ov7670_read_reg

  IPC_DownloadM0Image (Thumb, 24 bytes, Stack size 16 bytes, sgpcamdemo.o(i.IPC_DownloadM0Image))
  [Stack]

  - Max Depth = 16
  - Call Chain = IPC_DownloadM0Image
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> main

  IPC_HoldM0 (Thumb, 30 bytes, Stack size 0 bytes, sgpcamdemo.o(i.IPC_HoldM0))
  [Called By]

  - >> main

  IPC_ReleaseM0 (Thumb, 32 bytes, Stack size 0 bytes, sgpcamdemo.o(i.IPC_ReleaseM0))
  [Called By]

  - >> main

  LCD_IRQHandler (Thumb, 66 bytes, Stack size 16 bytes, sgpcamdemo.o(i.LCD_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_IRQHandler ⇒ FBQ_GetConsumeIndex
  [Calls]
  - >> FBQ_GetConsumeIndex
  - >> FBQ_ConsumeDone
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  OV7670RegInit (Thumb, 1372 bytes, Stack size 8 bytes, cam_ov7670.o(i.OV7670RegInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = OV7670RegInit ⇒ ov7670_write_reg ⇒ I2CForOv7670_Start
  [Calls]
  - >> ov7670_write_reg
  [Called By]
  - >> CamInit

  PinInit (Thumb, 158 bytes, Stack size 0 bytes, sgpcamdemo.o(i.PinInit))
  [Called By]

  - >> CamInit

  SGPGetRdyToGo (Thumb, 62 bytes, Stack size 8 bytes, sgpcamdemo.o(i.SGPGetRdyToGo))
  [Stack]

  - Max Depth = 8
  - Call Chain = SGPGetRdyToGo
  [Called By]
  - >> GPIO6_IRQHandler

  SGPStop (Thumb, 46 bytes, Stack size 8 bytes, sgpcamdemo.o(i.SGPStop))
  [Stack]

  - Max Depth = 8
  - Call Chain = SGPStop
  [Called By]
  - >> GPIO6_IRQHandler

  SetClock (Thumb, 372 bytes, Stack size 12 bytes, system_lpc43xx.o(i.SetClock))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetClock
  [Called By]
  - >> SystemInit

  SetupSGPIO (Thumb, 196 bytes, Stack size 32 bytes, cam_ov7670.o(i.SetupSGPIO))
  [Stack]

  - Max Depth = 40
  - Call Chain = SetupSGPIO ⇒ NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  - >> NVIC_DisableIRQ
  [Called By]
  - >> CamInit

  SysTick_Handler (Thumb, 130 bytes, Stack size 0 bytes, sgpcamdemo.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SystemCoreClockUpdate (Thumb, 22 bytes, Stack size 8 bytes, system_lpc43xx.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 52
  - Call Chain = SystemCoreClockUpdate ⇒ GetClockFreq ⇒ GetPLL1Param
  [Calls]
  - >> GetClockFreq
  [Called By]
  - >> SystemInit

  SystemInit (Thumb, 44 bytes, Stack size 8 bytes, system_lpc43xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 128
  - Call Chain = SystemInit ⇒ SystemInit_ExtMemCtl ⇒ WaitUs ⇒ __aeabi_uldivmod
  [Calls]
  - >> SystemInit_ExtMemCtl
  - >> SystemCoreClockUpdate
  - >> SetClock
  - >> getPC
  [Called By]
  - >> main

  SystemInit_ExtMemCtl (Thumb, 1420 bytes, Stack size 48 bytes, system_lpc43xx.o(i.SystemInit_ExtMemCtl))
  [Stack]

  - Max Depth = 120
  - Call Chain = SystemInit_ExtMemCtl ⇒ WaitUs ⇒ __aeabi_uldivmod
  [Calls]
  - >> WaitUs
  - >> __aeabi_uldivmod
  [Called By]
  - >> SystemInit

  VSyncIrqInit (Thumb, 76 bytes, Stack size 16 bytes, cam_ov7670.o(i.VSyncIrqInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = VSyncIrqInit ⇒ NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> CamInit

  VideoRefresh (Thumb, 8 bytes, Stack size 8 bytes, cam_ov7670.o(i.VideoRefresh))
  [Stack]

  - Max Depth = 72
  - Call Chain = VideoRefresh ⇒ OV7670RefreshColor ⇒ FBQ_GetProduceIndex
  [Calls]
  - >> OV7670RefreshColor
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 298 bytes, Stack size 0 bytes, sgpcamdemo.o(i.main))
  [Stack]

  - Max Depth = 128
  - Call Chain = main ⇒ SystemInit ⇒ SystemInit_ExtMemCtl ⇒ WaitUs ⇒ __aeabi_uldivmod
  [Calls]
  - >> __set_PRIMASK
  - >> __set_FAULTMASK
  - >> FBQ_IsFull
  - >> FBQ_Init
  - >> GLCD_SetTextColor
  - >> GLCD_SetBackColor
  - >> GLCD_Init
  - >> GLCD_DisplayString
  - >> GLCD_Clear
  - >> SystemInit
  - >> VideoRefresh
  - >> CamInit
  - >> IPC_ReleaseM0
  - >> IPC_HoldM0
  - >> IPC_DownloadM0Image
  [Address Reference Count : 1]
  - entry8.o(.ARM.Collect$$$$00000009)

  ov7670_read_reg (Thumb, 52 bytes, Stack size 16 bytes, cam_ov7670.o(i.ov7670_read_reg))
  [Stack]

  - Max Depth = 32
  - Call Chain = ov7670_read_reg ⇒ I2CForOv7670_Read
  [Calls]
  - >> I2CForOv7670_Start
  - >> I2CForOv7670_Write
  - >> I2CForOv7670_Stop
  - >> I2CForOv7670_Read
  [Called By]
  - >> CamInit

  ov7670_write_reg (Thumb, 36 bytes, Stack size 16 bytes, cam_ov7670.o(i.ov7670_write_reg))
  [Stack]

  - Max Depth = 24
  - Call Chain = ov7670_write_reg ⇒ I2CForOv7670_Start
  [Calls]
  - >> I2CForOv7670_Start
  - >> I2CForOv7670_Write
  - >> I2CForOv7670_Stop
  [Called By]
  - >> OV7670RegInit

  ### Local Symbols

  WaitUs (Thumb, 72 bytes, Stack size 32 bytes, system_lpc43xx.o(i.WaitUs))
  [Stack]

  - Max Depth = 72
  - Call Chain = WaitUs ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> SystemInit_ExtMemCtl

  delay (Thumb, 14 bytes, Stack size 0 bytes, glcd_lpc43xx.o(i.delay))
  [Called By]

  - >> GLCD_Init

  spi_tran (Thumb, 26 bytes, Stack size 0 bytes, glcd_lpc43xx.o(i.spi_tran))
  [Called By]

  - >> wr_reg
  - >> wr_cmd

  wr_cmd (Thumb, 42 bytes, Stack size 8 bytes, glcd_lpc43xx.o(i.wr_cmd))
  [Stack]

  - Max Depth = 8
  - Call Chain = wr_cmd
  [Calls]
  - >> spi_tran
  [Called By]
  - >> wr_reg

  wr_reg (Thumb, 54 bytes, Stack size 16 bytes, glcd_lpc43xx.o(i.wr_reg))
  [Stack]

  - Max Depth = 24
  - Call Chain = wr_reg ⇒ wr_cmd
  [Calls]
  - >> wr_cmd
  - >> spi_tran
  [Called By]
  - >> GLCD_Init

  __set_PRIMASK (Thumb, 6 bytes, Stack size 0 bytes, frabufq.o(i.__set_PRIMASK))
  [Called By]

  - >> FBQ_ProduceDone
  - >> FBQ_GetProduceIndex
  - >> FBQ_GetConsumeIndex
  - >> FBQ_ConsumeDone

  __set_FAULTMASK (Thumb, 10 bytes, Stack size 0 bytes, sgpcamdemo.o(i.__set_FAULTMASK))
  [Called By]

  - >> main

  __set_PRIMASK (Thumb, 6 bytes, Stack size 0 bytes, sgpcamdemo.o(i.__set_PRIMASK))
  [Called By]

  - >> main
  - >> GPIO6_IRQHandler

  I2CForOv7670_Init (Thumb, 84 bytes, Stack size 0 bytes, cam_ov7670.o(i.I2CForOv7670_Init))
  [Called By]

  - >> CamInit

  I2CForOv7670_Read (Thumb, 60 bytes, Stack size 16 bytes, cam_ov7670.o(i.I2CForOv7670_Read))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2CForOv7670_Read
  [Calls]
  - >> WaitStatus
  [Called By]
  - >> ov7670_read_reg

  I2CForOv7670_Stop (Thumb, 14 bytes, Stack size 0 bytes, cam_ov7670.o(i.I2CForOv7670_Stop))
  [Called By]

  - >> ov7670_write_reg
  - >> ov7670_read_reg

  I2CForOv7670_Write (Thumb, 20 bytes, Stack size 8 bytes, cam_ov7670.o(i.I2CForOv7670_Write))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2CForOv7670_Write
  [Calls]
  - >> WaitStatus
  [Called By]
  - >> ov7670_write_reg
  - >> ov7670_read_reg

  NVIC_DisableIRQ (Thumb, 18 bytes, Stack size 0 bytes, cam_ov7670.o(i.NVIC_DisableIRQ))
  [Called By]

  - >> SetupSGPIO
  - >> CamInit

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, cam_ov7670.o(i.NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_SetPriority
  [Called By]
  - >> VSyncIrqInit
  - >> SetupSGPIO
  - >> CamInit

  WaitStart (Thumb, 30 bytes, Stack size 0 bytes, cam_ov7670.o(i.WaitStart))
  [Called By]

  - >> I2CForOv7670_Start

  WaitStatus (Thumb, 28 bytes, Stack size 0 bytes, cam_ov7670.o(i.WaitStatus))
  [Called By]

  - >> I2CForOv7670_Write
  - >> I2CForOv7670_Read

  ### Undefined Global Symbols