# Static Call Graph for image .\InFlash\example.axf

#<CALLGRAPH># ARM Linker, 5.02 [Build 28]: Last Updated: Thu Mar 21 16:50:08 2013

### Maximum Stack Usage = 212 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ c_entry ⇒ SGPIO_UART_Receive ⇒ SGPIO_UART_ReceiveByte

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC0_IRQHandler ⇒ ADC0_IRQHandler

  ### Function Pointers

  - ADC0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - ADC1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - ATIMER_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - BusFault_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - CAN0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - CAN1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - DAC_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - DMA_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - DebugMon_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - ETH_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - EVRT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - EZH_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - FLASH_EEPROM_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GINT0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GINT1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO2_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO3_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO4_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO5_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO6_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - GPIO7_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - HardFault_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2S0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - I2S1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - LCD_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - M0CORE_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - M0s_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - MemManage_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - NMI_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - PendSV_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - QEI_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - RIT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - RTC_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - Reset_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SCT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SDIO_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SGPIO_IRQHandler from sgpio_uart.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SPIFI_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SPI_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SVC_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - SysTick_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART2_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UART3_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - USB0_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - USB1_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - UsageFault_Handler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - VADC_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - WDT_IRQHandler from startup_lpc43xx.o(.text) referenced from startup_lpc43xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc43xx.o(.text)
  - main from sgpio_uart_demo.o(.text) referenced from entry8.o(.ARM.Collect$$$$00000009)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry8.o(.ARM.Collect$$$$00000009))

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Calls]

  - >> ADC0_IRQHandler
  [Called By]
  - >> ADC0_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  ATIMER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  CAN0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  CAN1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  EVRT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  EZH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  FLASH_EEPROM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  GPIO7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2S0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  I2S1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  M0CORE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  M0s_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SPIFI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  USB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  USB1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  VADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc43xx.o(RESET)

  getPC (Thumb, 4 bytes, Stack size 0 bytes, startup_lpc43xx.o(.text), UNUSED)

  SystemInit (Thumb, 36 bytes, Stack size 0 bytes, system_lpc43xx.o(.text))
  [Called By]

  - >> c_entry

  CGU_UpdateClock (Thumb, 180 bytes, Stack size 12 bytes, lpc43xx_cgu.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CGU_UpdateClock
  [Called By]
  - >> CGU_Init

  CGU_EntityConnect (Thumb, 116 bytes, Stack size 12 bytes, lpc43xx_cgu.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CGU_EntityConnect
  [Called By]
  - >> SGPIO_UART_setclk
  - >> CGU_Init

  CGU_EnableEntity (Thumb, 272 bytes, Stack size 24 bytes, lpc43xx_cgu.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = CGU_EnableEntity ⇒ scu_pinmux
  [Calls]
  - >> scu_pinmux
  [Called By]
  - >> CGU_ConfigPWR
  - >> CGU_Init

  CGU_SetPLL1 (Thumb, 160 bytes, Stack size 20 bytes, lpc43xx_cgu.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = CGU_SetPLL1
  [Called By]
  - >> CGU_Init

  CGU_SetXTALOSC (Thumb, 54 bytes, Stack size 0 bytes, lpc43xx_cgu.o(.text))
  [Called By]

  - >> CGU_Init

  CGU_Init (Thumb, 54 bytes, Stack size 8 bytes, lpc43xx_cgu.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = CGU_Init ⇒ CGU_EnableEntity ⇒ scu_pinmux
  [Calls]
  - >> CGU_SetXTALOSC
  - >> CGU_SetPLL1
  - >> CGU_EnableEntity
  - >> CGU_EntityConnect
  - >> CGU_UpdateClock
  [Called By]
  - >> c_entry

  CGU_GetBaseStatus (Thumb, 232 bytes, Stack size 0 bytes, lpc43xx_cgu.o(.text), UNUSED)
  [Called By]

  - >> CGU_ConfigPWR

  CGU_ConfigPWR (Thumb, 672 bytes, Stack size 16 bytes, lpc43xx_cgu.o(.text), UNUSED)
  [Calls]

  - >> CGU_ConfigPWR
  - >> CGU_GetBaseStatus
  - >> CGU_EnableEntity
  [Called By]
  - >> CGU_ConfigPWR

  CGU_GetPCLKFrequency (Thumb, 230 bytes, Stack size 0 bytes, lpc43xx_cgu.o(.text))
  [Called By]

  - >> SGPIO_UART_setclk

  CGU_SetDIV (Thumb, 56 bytes, Stack size 8 bytes, lpc43xx_cgu.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CGU_SetDIV
  [Called By]
  - >> SGPIO_UART_setclk

  CGU_SetPLL0 (Thumb, 62 bytes, Stack size 0 bytes, lpc43xx_cgu.o(.text), UNUSED)

  CGU_SetPLL0audio (Thumb, 34 bytes, Stack size 0 bytes, lpc43xx_cgu.o(.text), UNUSED)

  CGU_FrequencyMonitor (Thumb, 166 bytes, Stack size 20 bytes, lpc43xx_cgu.o(.text), UNUSED)
  [Called By]

  - >> CGU_RealFrequencyCompare

  CGU_RealFrequencyCompare (Thumb, 64 bytes, Stack size 36 bytes, lpc43xx_cgu.o(.text), UNUSED)
  [Calls]

  - >> CGU_FrequencyMonitor

  scu_pinmux (Thumb, 30 bytes, Stack size 20 bytes, lpc43xx_scu.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = scu_pinmux
  [Called By]
  - >> SGPIO_Borad_config
  - >> CGU_EnableEntity

  SGPIO_UART_ConfigStructInit (Thumb, 36 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> c_entry

  SGPIO_UART_setclk (Thumb, 256 bytes, Stack size 32 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = SGPIO_UART_setclk ⇒ CGU_EntityConnect
  [Calls]
  - >> CGU_SetDIV
  - >> CGU_GetPCLKFrequency
  - >> CGU_EntityConnect
  [Called By]
  - >> c_entry

  SGPIO_UART_EnTxIRQ (Thumb, 10 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> SGPIO_UART_Tx_Init

  SGPIO_UART_DisTxIRQ (Thumb, 12 bytes, Stack size 0 bytes, sgpio_uart.o(.text), UNUSED)

  SGPIO_UART_Tx_Init (Thumb, 72 bytes, Stack size 16 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SGPIO_UART_Tx_Init
  [Calls]
  - >> SGPIO_UART_EnTxIRQ
  - >> NVIC_EnableIRQ
  [Called By]
  - >> c_entry

  SGPIO_UART_Rx_Init (Thumb, 66 bytes, Stack size 16 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SGPIO_UART_Rx_Init
  [Calls]
  - >> NVIC_EnableIRQ
  - >> SGPIO_UART_Rx_Match
  [Called By]
  - >> c_entry

  SGPIO_UART_Setmode (Thumb, 50 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> c_entry
  - >> SGPIO_UART_SendFull
  - >> SGPIO_UART_Send

  SGPIO_UART_Enter_SendIdle (Thumb, 28 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> SGPIO_UART_SendFull
  - >> SGPIO_UART_Send

  SGPIO_UART_SendByte (Thumb, 18 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> SGPIO_UART_SendFull
  - >> SGPIO_UART_Send

  SGPIO_UART_ReceiveByte (Thumb, 130 bytes, Stack size 28 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SGPIO_UART_ReceiveByte
  [Called By]
  - >> SGPIO_UART_RxFull
  - >> SGPIO_UART_Receive

  SGPIO_UART_Send (Thumb, 80 bytes, Stack size 28 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SGPIO_UART_Send
  [Calls]
  - >> SGPIO_UART_SendByte
  - >> SGPIO_UART_Enter_SendIdle
  - >> SGPIO_UART_Setmode
  [Called By]
  - >> c_entry
  - >> print_menu

  SGPIO_UART_Receive (Thumb, 68 bytes, Stack size 32 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = SGPIO_UART_Receive ⇒ SGPIO_UART_ReceiveByte
  [Calls]
  - >> SGPIO_UART_ReceiveByte
  - >> SGPIO_UART_Rx_Match
  [Called By]
  - >> c_entry

  SGPIO_UART_SendFull (Thumb, 132 bytes, Stack size 32 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SGPIO_UART_SendFull
  [Calls]
  - >> SGPIO_UART_SendByte
  - >> SGPIO_UART_Enter_SendIdle
  - >> SGPIO_UART_Setmode
  [Called By]
  - >> c_entry

  SGPIO_UART_RxFull (Thumb, 54 bytes, Stack size 24 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = SGPIO_UART_RxFull ⇒ SGPIO_UART_ReceiveByte
  [Calls]
  - >> SGPIO_UART_ReceiveByte
  - >> SGPIO_UART_Rx_Match
  [Called By]
  - >> c_entry

  SGPIO_IRQHandler (Thumb, 208 bytes, Stack size 8 bytes, sgpio_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SGPIO_IRQHandler
  [Calls]
  - >> SGPIO_UART_Rx_Capture
  [Address Reference Count : 1]
  - startup_lpc43xx.o(RESET)

  print_menu (Thumb, 36 bytes, Stack size 8 bytes, sgpio_uart_demo.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = print_menu ⇒ SGPIO_UART_Send
  [Calls]
  - >> SGPIO_UART_Send
  [Called By]
  - >> c_entry

  SGPIO_Borad_config (Thumb, 46 bytes, Stack size 8 bytes, sgpio_uart_demo.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SGPIO_Borad_config ⇒ scu_pinmux
  [Calls]
  - >> scu_pinmux
  [Called By]
  - >> c_entry

  c_entry (Thumb, 426 bytes, Stack size 144 bytes, sgpio_uart_demo.o(.text))
  [Stack]

  - Max Depth = 204
  - Call Chain = c_entry ⇒ SGPIO_UART_Receive ⇒ SGPIO_UART_ReceiveByte
  [Calls]
  - >> strcpy
  - >> SGPIO_Borad_config
  - >> print_menu
  - >> SGPIO_UART_RxFull
  - >> SGPIO_UART_SendFull
  - >> SGPIO_UART_Receive
  - >> SGPIO_UART_Send
  - >> SGPIO_UART_Setmode
  - >> SGPIO_UART_Rx_Init
  - >> SGPIO_UART_Tx_Init
  - >> SGPIO_UART_setclk
  - >> SGPIO_UART_ConfigStructInit
  - >> CGU_Init
  - >> SystemInit
  [Called By]
  - >> main

  main (Thumb, 8 bytes, Stack size 8 bytes, sgpio_uart_demo.o(.text))
  [Stack]

  - Max Depth = 212
  - Call Chain = main ⇒ c_entry ⇒ SGPIO_UART_Receive ⇒ SGPIO_UART_ReceiveByte
  [Calls]
  - >> c_entry
  [Address Reference Count : 1]
  - entry8.o(.ARM.Collect$$$$00000009)

  strcpy (Thumb, 18 bytes, Stack size 0 bytes, strcpy.o(.text))
  [Called By]

  - >> c_entry

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 92 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SGPIO_UART_Rx_Match (Thumb, 52 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> SGPIO_UART_RxFull
  - >> SGPIO_UART_Receive
  - >> SGPIO_UART_Rx_Init

  SGPIO_UART_Rx_Capture (Thumb, 90 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> SGPIO_IRQHandler

  NVIC_EnableIRQ (Thumb, 24 bytes, Stack size 0 bytes, sgpio_uart.o(.text))
  [Called By]

  - >> SGPIO_UART_Rx_Init
  - >> SGPIO_UART_Tx_Init

  ### Undefined Global Symbols