NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Functions
Component : Linux User Spi
Bus Abstraction Layer

Component without functionality to ease implementation of additional busses. More...

Collaboration diagram for Component : Linux User Spi:

## Data Structures
struct | phbalReg_LinuxUserSpi_DataParams_t
| BAL Linux User Spi parameter structure. More...

## Macros
#define | PHBAL_REG_LINUX_USER_SPI_ID 0x12U
| ID for Linux User Spi BAL component.

## Functions
phStatus_t | phbalReg_LinuxUserSpi_Init (phbalReg_LinuxUserSpi_DataParams_t *pDataParams, uint16_t wSizeOfDataParams)
| Initialise the BAL Linux User Spi layer. More...

## Detailed Description

Component without functionality to ease implementation of additional busses.

## Function Documentation

## § phbalReg_LinuxUserSpi_Init()

phStatus_t phbalReg_LinuxUserSpi_Init | ( | phbalReg_LinuxUserSpi_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams
| ) |  |

Initialise the BAL Linux User Spi layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.
  PH_ERR_INVALID_DATA_PARAMS | Parameter structure size is invalid.