NXP NFC Reader Library v4.040.05.011646

Data Fields
phalTop_T5T Struct Reference
Application Layer » Tag Operation Layer » Component : Software

T5T parameter structure. More...

## Data Fields
void * | pAlI15693DataParams
| Pointer to T5T data parameters.
uint8_t | bRwa
| Tag read/write size.
uint8_t | bTerminatorTlvPresence
| Terminator TLV presence; 1 -present, 0 - not present.
uint8_t | bMbRead
| Flag Bit for Multiple Read support.
uint8_t | bLockBlock
| Flag Bit for Lock Command support.
uint8_t | bSplFrm
| Flag Bit for special frame support.
uint8_t | bExtendedCommandSupport
| Flag Bit for Extended Command Support support.
uint8_t | bOptionFlag
| Option Flag PH_ON = Enable, PH_OFF = Disable.
uint16_t | wMlen
| Tag Memory size.
uint16_t | wNdefHeaderAddr
| Header offset of first NDEF message.
uint16_t | wNdefMsgAddr
| NDEF message start address.
uint16_t | bBlockSize
| T5T Block Size supported by card.
uint16_t | bMaxBlockNum
| Maximum Block number supported by Card.

## Detailed Description

T5T parameter structure.

The documentation for this struct was generated from the following file:

- phalTop.h