NXP NFC Reader Library v4.040.05.011646

Data Structures | Data Fields
phacDiscLoop_Sw_TypeA_Info Struct Reference
Activity Layer » Discovery Loop » Component : Software

Type A parameter structure. More...

## Data Structures
struct | phacDiscLoop_Type_P2P_TAGS
| Structure holding information on Type A P2P activation/communication. More...
struct | phacDiscLoop_TypeA_I3P3
| Structure info required for ISO/IEC 14443 communication. More...
struct | phascDiscLoop_TypeA_I3P4
| Structure info required for ISO/IEC 14443-4 communication. More...

## Data Fields
uint8_t | bTotalTagsFound
| Number of type A tags found. More...
uint8_t | bT1TFlag
| Flag to indicate detected tag is T1T Tag in NFC profile, could be any jewel tag in other profile.

## Detailed Description

Type A parameter structure.

## Field Documentation

## § bTotalTagsFound

uint8_t phacDiscLoop_Sw_TypeA_Info::bTotalTagsFound

Number of type A tags found.

The documentation for this struct was generated from the following file:

- phacDiscLoop.h