NXP NFC Reader Library v4.040.05.011646

Data Fields
phpalI18000p3m3_Sw_DataParams_t Struct Reference
Protocol Abstraction Layer » ISO/IEC 18000-3 Mode3 » Component : Software

Software PAL-I18000P3M3 parameter structure. More...

## Data Fields
uint16_t | wId
| Layer ID for this component, NEVER MODIFY!
void * | pHalDataParams
| Pointer to the parameter structure of the underlying HAL layer. More...
uint8_t | bSession
| Active session of inventory round. More...
uint8_t | abStoredCRC [2]
| Stored CRC returned by the tag. More...
uint8_t | bStoredCRCValid
| Whether StoredCRC is valid or not. More...

## Detailed Description

Software PAL-I18000P3M3 parameter structure.

## Field Documentation

## § pHalDataParams

void* phpalI18000p3m3_Sw_DataParams_t::pHalDataParams

Pointer to the parameter structure of the underlying HAL layer.

## § bSession

uint8_t phpalI18000p3m3_Sw_DataParams_t::bSession

Active session of inventory round.

## § abStoredCRC

uint8_t phpalI18000p3m3_Sw_DataParams_t::abStoredCRC[2]

Stored CRC returned by the tag.

## § bStoredCRCValid

uint8_t phpalI18000p3m3_Sw_DataParams_t::bStoredCRCValid

Whether StoredCRC is valid or not.

The documentation for this struct was generated from the following file:

- phpalI18000p3m3.h