NXP NFC Reader Library v4.040.05.011646

Data Fields
phalTop_TIT_Segment Struct Reference
Application Layer » Tag Operation Layer » Component : Software

T1T Segment parameters. More...

## Data Fields
uint8_t | bAddress
| Current active segment address.
uint8_t * | pData
| Segment data (points to HAL RX buffer)
uint8_t | bLockReservedOtp [16]
| Lock/reserved/OTP bytes in current segment.

## Detailed Description

T1T Segment parameters.

The documentation for this struct was generated from the following file:

- phalTop.h