NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Functions
Component : Software
Protocol Abstraction Layer » MIFARE(R)
Collaboration diagram for Component : Software:

## Data Structures
struct | phpalMifare_Sw_DataParams_t
| Software PAL-MIFARE parameter structure. More...

## Macros
#define | PHPAL_MIFARE_SW_ID 0x02
| ID for Software MIFARE layer. More...

## Functions
phStatus_t | phpalMifare_Sw_Init (phpalMifare_Sw_DataParams_t *pDataParams, uint16_t wSizeOfDataParams, void *pHalDataParams, void *pPalI14443p4DataParams)
| Initialize this layer. More...

## Detailed Description

## Macro Definition Documentation

## § PHPAL_MIFARE_SW_ID

#define PHPAL_MIFARE_SW_ID 0x02

ID for Software MIFARE layer.

## Function Documentation

## § phpalMifare_Sw_Init()

phStatus_t phpalMifare_Sw_Init | ( | phpalMifare_Sw_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams,
|  | void * | pHalDataParams,
|  | void * | pPalI14443p4DataParams
| ) |  |

Initialize this layer.

Remark: `pPalI14443p4DataParams` can be NULL in case phpalMifare_ExchangeL4 and phpalMifare_ExchangePc are not needed.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.

Parameters

  [in] | pDataParams | Pointer to this layer's parameter structure.
  [in] | wSizeOfDataParams | Specifies the size of the data parameter structure.
  [in] | pHalDataParams | Pointer to the parameter structure of the underlying HAL layer.
  [in] | pPalI14443p4DataParams | Pointer to the parameter structure of the underlying ISO14443-4 layer.