NXP NFC Reader Library v4.040.05.011646

Data Fields
phalTop_T4T Struct Reference
Application Layer » Tag Operation Layer » Component : Software

T4T parameter structure. More...

## Data Fields
void * | pAlT4TDataParams
| Pointer to T4T data parameters.
uint8_t | aNdefFileID [2]
| NDEF File ID to Create.
uint8_t | bRa
| NDEF file read access condition size.
uint8_t | bWa
| NDEF file write access condition size.
uint8_t | bCurrentSelectedFile
| Current selected file.
uint16_t | wMLe
| MLe supported by card (obtained from CC)
uint16_t | wMLc
| MLc supported by card (obtained from CC)
uint16_t | wCCLEN
| Size of CCr,Valid CCLEN range 000Fh-FFFEh. More...
uint16_t | wMaxFileSize
| Maximum NDEF file size in bytes.

## Detailed Description

T4T parameter structure.

## Field Documentation

## § wCCLEN

uint16_t phalTop_T4T::wCCLEN

Size of CCr,Valid CCLEN range 000Fh-FFFEh.

The documentation for this struct was generated from the following file:

- phalTop.h