NXP NFC Reader Library v4.040.05.011646

Data Fields
phNfcLib_MFC Struct Reference

Defines parameters that needs be provided by User to communicate with MIFare Classic card. More...

## Data Fields
phNfcLib_MFC_Commands_t | bCommand
| [In] Mifare Classic command needs to be provided. More...
uint8_t | bBlockNumber
| [In] Block number on which Mifare Classic command to be executed. More...
uint8_t | bKeyType
| [In] Key Type used to Authenticate Mifare Classic. More...
uint8_t | bKeyNumber
| [In] Key Number from Sw KeyStore to be fetched to Authenticate Mifare Classic. More...
uint8_t | bKeyVersion
| [In] Key version from Sw KeyStore to be retrieved to Authenticate Mifare Classic. More...
uint8_t | bUidType
| [In] UID Type used to Personalize the MFC card. More...

## Detailed Description

Defines parameters that needs be provided by User to communicate with MIFare Classic card.

## Field Documentation

## § bCommand

phNfcLib_MFC_Commands_t phNfcLib_MFC::bCommand

[In] Mifare Classic command needs to be provided.

## § bBlockNumber

uint8_t phNfcLib_MFC::bBlockNumber

[In] Block number on which Mifare Classic command to be executed.

## § bKeyType

uint8_t phNfcLib_MFC::bKeyType

[In] Key Type used to Authenticate Mifare Classic.

Takes either PHHAL_HW_MFC_KEYA or PHHAL_HW_MFC_KEYB.

## § bKeyNumber

uint8_t phNfcLib_MFC::bKeyNumber

[In] Key Number from Sw KeyStore to be fetched to Authenticate Mifare Classic.

## § bKeyVersion

uint8_t phNfcLib_MFC::bKeyVersion

[In] Key version from Sw KeyStore to be retrieved to Authenticate Mifare Classic.

## § bUidType

uint8_t phNfcLib_MFC::bUidType

[In] UID Type used to Personalize the MFC card.

Refer nfc_lib_mfc_uid_type

The documentation for this struct was generated from the following file:

- phNfcLib.h