NXP NFC Reader Library v4.040.05.011646

Data Fields
phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4 Struct Reference

Structure info required for ISO/IEC 14443-4 communication. More...

## Data Fields
uint8_t | bFsdi
| Frame size integer. More...
uint8_t | bCid
| Card identifier. More...
uint8_t | bNad
| Node ADdress. More...
uint8_t | bDri
| Data Rate received by Initiator. More...
uint8_t | bDsi
| Data Rate send by Initiator. More...
uint8_t * | pAts
| Holds the answer to select response. More...

## Detailed Description

Structure info required for ISO/IEC 14443-4 communication.

## Field Documentation

## § bFsdi

uint8_t phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4::bFsdi

Frame size integer.

## § bCid

uint8_t phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4::bCid

Card identifier.

## § bNad

uint8_t phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4::bNad

Node ADdress.

## § bDri

uint8_t phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4::bDri

Data Rate received by Initiator.

## § bDsi

uint8_t phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4::bDsi

Data Rate send by Initiator.

## § pAts

uint8_t* phacDiscLoop_Sw_TypeA_Info::phascDiscLoop_TypeA_I3P4::pAts

Holds the answer to select response.

The documentation for this struct was generated from the following file:

- phacDiscLoop.h