NXP NFC Reader Library v4.040.05.011646

Data Fields
phacDiscLoop_Sw_TypeB_Info::phacDiscLoop_TypeB_I3P3B Struct Reference

Structure for Type B (ISO/IEC 14443-B) tags. More...

## Data Fields
uint8_t | aPupi [PHAC_DISCLOOP_I3P3B_PUPI_LENGTH]
| ISO/IEC 14443-3B Pseudo Unique PICC identifier. More...
uint8_t | aAtqB [PHAC_DISCLOOP_I3P3B_MAX_ATQB_LENGTH]
| ATQB received from ISO/IEC 14443-3B compliant device. More...
uint8_t | bAtqBLength
| Length of the ATQB response. More...
uint8_t | bSupportType4B
| Indicates activated TypeB tag supports Type 4B Tag Platform or not. More...

## Detailed Description

Structure for Type B (ISO/IEC 14443-B) tags.

## Field Documentation

## § aPupi

uint8_t phacDiscLoop_Sw_TypeB_Info::phacDiscLoop_TypeB_I3P3B::aPupi[PHAC_DISCLOOP_I3P3B_PUPI_LENGTH]

ISO/IEC 14443-3B Pseudo Unique PICC identifier.

## § aAtqB

uint8_t phacDiscLoop_Sw_TypeB_Info::phacDiscLoop_TypeB_I3P3B::aAtqB[PHAC_DISCLOOP_I3P3B_MAX_ATQB_LENGTH]

ATQB received from ISO/IEC 14443-3B compliant device.

## § bAtqBLength

uint8_t phacDiscLoop_Sw_TypeB_Info::phacDiscLoop_TypeB_I3P3B::bAtqBLength

Length of the ATQB response.

## § bSupportType4B

uint8_t phacDiscLoop_Sw_TypeB_Info::phacDiscLoop_TypeB_I3P3B::bSupportType4B

Indicates activated TypeB tag supports Type 4B Tag Platform or not.

The documentation for this struct was generated from the following file:

- phacDiscLoop.h