NXP NFC Reader Library v4.040.05.011646

Data Fields
phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info Struct Reference

Structure holding information for Type F P2P communication. More...

## Data Fields
uint8_t | bDid
| Device identifier. More...
uint8_t | bLri
| Length reduction of Initiator. More...
uint8_t | bNadEnable
| Enable usage of node address. More...
uint8_t | bNad
| Node address. More...
uint8_t * | pGi
| Optional general bytes. More...
uint8_t | bGiLength
| Length of the optional bytes. More...
uint8_t * | pAtrRes
| Pointer to the Attribute response. More...
uint8_t | bAtrResLength
| Attribute response length. More...

## Detailed Description

Structure holding information for Type F P2P communication.

## Field Documentation

## § bDid

uint8_t phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::bDid

Device identifier.

Disabled if set to 0 else should have a value between 1-14.

## § bLri

uint8_t phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::bLri

Length reduction of Initiator.

Should be a value in range 0-3.

## § bNadEnable

uint8_t phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::bNadEnable

Enable usage of node address.

If set to zero NAD is disabled.

## § bNad

uint8_t phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::bNad

Node address.

## § pGi

uint8_t* phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::pGi

Optional general bytes.

## § bGiLength

uint8_t phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::bGiLength

Length of the optional bytes.

## § pAtrRes

uint8_t* phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::pAtrRes

Pointer to the Attribute response.

## § bAtrResLength

uint8_t phacDiscLoop_Sw_TypeF_Info::phacDiscLoop_TypeF_P2P_Info::bAtrResLength

Attribute response length.

The documentation for this struct was generated from the following file:

- phacDiscLoop.h