NXP NFC Reader Library v4.040.05.011646

Data Structures
Here are the data structures with brief descriptions:
[detail level 1 2]

C phacDiscLoop_I18000p3m3_Info | 18000p3m3 parameter structure
C phacDiscLoop_Sw_DataParams | Discovery loop parameter structure
▼C phacDiscLoop_Sw_TypeA_Info | Type A parameter structure
C phacDiscLoop_Type_P2P_TAGS | Structure holding information on Type A P2P activation/communication
C phacDiscLoop_TypeA_I3P3 | Structure info required for ISO/IEC 14443 communication
C phascDiscLoop_TypeA_I3P4 | Structure info required for ISO/IEC 14443-4 communication
▼C phacDiscLoop_Sw_TypeB_Info | Type B parameter structure
C phacDiscLoop_TypeB_I3P3B | Structure for Type B (ISO/IEC 14443-B) tags
C phacDiscLoop_TypeB_I3P4B | Type B ISO/IEC 14443-4B tag structure
▼C phacDiscLoop_Sw_TypeF_Info | Type F parameter structure
C phacDiscLoop_TypeF_P2P_Info | Structure holding information for Type F P2P communication
C phacDiscLoop_Sw_TypeV_Info | Type V parameter structure
C phacDiscLoop_TargetParams | Target parameter structure
C phalFelica_Sw_DataParams_t | Private parameter structure
C phalI15693_Sw_DataParams_t | Private parameter structure
C phalI18000p3m3_Sw_DataParams_t | Software PAL-I18000P3M3 parameter structure
C phalMfc_Sw_DataParams_t | Private parameter structure
C phalMfdf_Sw_DataParams_t | Struct phalMfdf_Sw_DataParams_t
C phalMful_Sw_DataParams_t | Private parameter structure
C phalSli_Sw_DataParams_t | Private parameter structure
C phalT1T_Sw_DataParams_t | Private parameter structure
C phalTop_Sw_DataParams | Tag Operations parameter structure
C phalTop_T1T | T1T parameter structure
C phalTop_T1T_LockCtrlTlv | T1T Lock Control TLV parameter structure
C phalTop_T1T_MemCtrlTlv | T1T Memory Control TLV parameter structure
C phalTop_T1T_ProprietaryTlv | T1T Proprietary TLV parameter structure
C phalTop_T2T | T2T parameter structure
C phalTop_T2T_LockCtrlTlv | T2T Lock Control TLV parameter structure
C phalTop_T2T_MemCtrlTlv | T2T Memory Control TLV parameter structure
C phalTop_T2T_Sector | T2T Sector parameters
C phalTop_T3T | T3T parameter structure
C phalTop_T4T | T4T parameter structure
C phalTop_T5T | T5T parameter structure
C phalTop_TIT_Segment | T1T Segment parameters
C phbalReg_KinetisI2C_DataParams_t | Kinetis I2C BAL parameter structure
C phbalReg_KinetisSpi_DataParams_t | Kinetis SPI BAL parameter structure
C phbalReg_LinuxKernelSpi_DataParams_t | BAL Linux Kernel Spi parameter structure
C phbalReg_LinuxUserI2C_DataParams_t | BAL Linux User I2C parameter structure
C phbalReg_LinuxUserSpi_DataParams_t | BAL Linux User Spi parameter structure
C phbalReg_LpcOpenI2c_DataParams_t | LPC Open I2C BAL parameter structure
C phbalReg_LpcOpenSpi_DataParams_t | LPC Open SPI BAL parameter structure
C phbalReg_Type_t | BAL type structure
C phceT4T_Sw_DataParams | NFC Type 4A Tag card emulation parameter structure
C phCidManager_Sw_DataParams_t | Cid Manager parameter structure
C phCryptoRng_Sw_DataParams_t | Software parameter structure
C phCryptoSym_Sw_DataParams_t | Software parameter structure
C phhalHw_Nfc_Ic_DataParams_t | HAL parameter structure
C phhalHw_Pn5180_DataParams_t | PN5180 HAL component
C phhalHw_PN7462AU_DataParams | Context Structure for PN7462AU
C phhalHw_Rc523_DataParams_t | Rc523 HAL parameter structure
C phhalHw_Rc663_DataParams_t | Rc663 HAL parameter structure
C phKeyStore_Sw_DataParams_t | Sw parameter structure
C phKeyStore_Sw_KeyEntry_t | Sw KeyEntry structure
C phKeyStore_Sw_KeyVersionPair_t | Sw KeyVersionPair structure
C phKeyStore_Sw_KUCEntry_t | Sw KeyUsageCounter structure
C phlnLlcp_LMDataParams | Link Management parameters that are expected by LLC
C phlnLlcp_Socket_Seq | Socket Sequence
C phlnLlcp_Sw_DataParams | LLCP parameter structure
C phlnLlcp_Transport_Socket | Socket structure of LLCP transport
C phNfcLib_DataParams_t | NFCLIB parameter structure
C phNfcLib_I15693 | Defines parameters that needs be provided by User to communicate with ISO 15693 card
C phNfcLib_I18000p3m3 | Defines parameters that needs be provided by User to communicate with ISO 18000p3m3 card
C phNfcLib_InternalState_t | NFC LIB State
C phNfcLib_MFC | Defines parameters that needs be provided by User to communicate with MIFare Classic card
C phNfcLib_MFdf | Defines parameters that needs be provided by User to communicate with MIFare DESFire card
C phNfcLib_MFUL | Defines parameters that needs be provided by User to communicate with MIFare Ultralight card
C phNfcLib_PeerInfo_t | Peer Information
C phNfcLib_RawTransmit | Defines parameters that needs be provided by User to communicate with raw ISO 14443-3 or ISO 14443-4 peer
C phNfcLib_Transmit | Defines parameters that needs be provided by User to use phNfcLib_Transmit API in ISO mode
C phnpSnep_Sw_DataParams | SNEP parameter structure
C phOsal_EventObj | Osal Event Object
C phOsal_MutexObj | Mutex Object
C phOsal_SemObj | OS Semaphore Object
C phOsal_ThreadObj | Osal Thread Object
C phOsal_TimePeriodObj | Timer Period Object
C phOsal_TimerObj | Osal Timer Object
C phpalFelica_Sw_DataParams_t | Felica parameter structure
C phpalI14443p3a_Sw_DataParams_t | Software PAL-ISO14443P3A parameter structure
C phpalI14443p3b_Sw_DataParams_t | Software PAL-ISO14443P3B parameter structure
C phpalI14443p4_Sw_DataParams_t | ISO14443-4 parameter structure
C phpalI14443p4a_Sw_DataParams_t | Software PAL-ISO14443P4A parameter structure
C phpalI14443p4mC_Sw_DataParams_t | ISO14443-4 card mode PAL parameter structure
C phpalI18000p3m3_Sw_DataParams_t | Software PAL-I18000P3M3 parameter structure
C phpalI18092mPI_Sw_DataParams_t | ISO18092 mode passive initiator parameter structure
C phpalI18092mT_Sw_DataParams_t | ISO18092 mode passive target parameter structure
C phpalMifare_Sw_DataParams_t | Software PAL-MIFARE parameter structure
C phpalSli15693_Sw_DataParams | Software Sli15693 PAL parameter structure
C phPlatform_DataParams_t | OSAL parameter structure
C phTools_Q | Queue structure of Message Queue