NXP NFC Reader Library v4.040.05.011646

Data Fields
phalI18000p3m3_Sw_DataParams_t Struct Reference
Application Layer » ISO/IEC 18000-3 Mode3 » Component : Software

Software PAL-I18000P3M3 parameter structure. More...

## Data Fields
uint16_t | wId
| Layer ID for this component, NEVER MODIFY!
void * | pPalI18000p3m3DataParams
| Pointer to the parameter structure of the underlying PAL layer. More...
uint8_t | abHandle [2]
| Handle retrieved by ReqRn. More...
uint8_t | bHandleValid
| Whether Handle is valid or not. More...

## Detailed Description

Software PAL-I18000P3M3 parameter structure.

## Field Documentation

## § pPalI18000p3m3DataParams

void* phalI18000p3m3_Sw_DataParams_t::pPalI18000p3m3DataParams

Pointer to the parameter structure of the underlying PAL layer.

## § abHandle

uint8_t phalI18000p3m3_Sw_DataParams_t::abHandle[2]

Handle retrieved by ReqRn.

## § bHandleValid

uint8_t phalI18000p3m3_Sw_DataParams_t::bHandleValid

Whether Handle is valid or not.

The documentation for this struct was generated from the following file:

- phalI18000p3m3.h