NXP NFC Reader Library v4.040.05.011646

Data Fields
phNfcLib_I15693 Struct Reference

Defines parameters that needs be provided by User to communicate with ISO 15693 card. More...

## Data Fields
phNfcLib_I15693_Commands_t | bCommand
| [In] ISO-IEC 15693-3 command needs to be provided. More...
uint8_t | bOption
| [In] Option flag shall be set in Request flags. More...
uint8_t | bAfi
| [In] Application family identifier. More...
uint8_t | bDsfid
| [In] Data storage format identifier. More...
uint16_t | wBlockNumber
| [In] Block number on which ISO 15693-3 command to be executed. More...
uint16_t | wNumBlocks
| [In] Number of blocks on which command like ReadMultiple/WriteMultiple blocks command to be executed. More...

## Detailed Description

Defines parameters that needs be provided by User to communicate with ISO 15693 card.

## Field Documentation

## § bCommand

phNfcLib_I15693_Commands_t phNfcLib_I15693::bCommand

[In] ISO-IEC 15693-3 command needs to be provided.

## § bOption

uint8_t phNfcLib_I15693::bOption

[In] Option flag shall be set in Request flags.

Meaning is defined by each command description. For more info refer ISO-IEC 15693-3 Spec.

## § bAfi

uint8_t phNfcLib_I15693::bAfi

[In] Application family identifier.

## § bDsfid

uint8_t phNfcLib_I15693::bDsfid

[In] Data storage format identifier.

## § wBlockNumber

uint16_t phNfcLib_I15693::wBlockNumber

[In] Block number on which ISO 15693-3 command to be executed.

Optional commands block number is single byte. Only in case of Extended commands block number will be 2 bytes.

## § wNumBlocks

uint16_t phNfcLib_I15693::wNumBlocks

[In] Number of blocks on which command like ReadMultiple/WriteMultiple blocks command to be executed.

The documentation for this struct was generated from the following file:

- phNfcLib.h