NXP NFC Reader Library v4.040.05.011646

Data Fields
phacDiscLoop_TargetParams Struct Reference
Activity Layer » Discovery Loop » Component : Software

Target parameter structure. More...

## Data Fields
uint8_t * | pRxBuffer
| Pointer to the Receive Buffer. More...
uint16_t | wRxBufferLen
| Length of Data Present in Receive Buffer. More...
uint16_t | wProtParams
| Frame mode and RX speed information. More...
uint8_t | bRetryCount
| Retry count for AUTOCOLL in case of failure. More...

## Detailed Description

Target parameter structure.

## Field Documentation

## § pRxBuffer

uint8_t* phacDiscLoop_TargetParams::pRxBuffer

Pointer to the Receive Buffer.

## § wRxBufferLen

uint16_t phacDiscLoop_TargetParams::wRxBufferLen

Length of Data Present in Receive Buffer.

## § wProtParams

uint16_t phacDiscLoop_TargetParams::wProtParams

Frame mode and RX speed information.

## § bRetryCount

uint8_t phacDiscLoop_TargetParams::bRetryCount

Retry count for AUTOCOLL in case of failure.

Default is 0.

The documentation for this struct was generated from the following file:

- phacDiscLoop.h