NXP NFC Reader Library v4.040.05.011646

Configuration
Hardware Abstraction Layer » component : Rc523

Custom Configuration of hardware related settings. More...

Collaboration diagram for Configuration:

## Memory related constants
#define | PHHAL_HW_RC523_PRECACHED_BYTES 0x40U
| Maximum number of bytes to precache into FIFO before triggering a command. More...

## Modulation indices
#define | PHHAL_HW_RC523_MODINDEX_I14443B 0x11U
| Default modulation index for ISO14443B. More...
#define | PHHAL_HW_RC523_MODINDEX_FELICA 0x12U
| Default modulation index for Felica. More...
#define | PHHAL_HW_RC523_MODINDEX_TARGET 0xF2U
| Default conductance for LoadModulation. More...

## RxThreshold values
#define | PHHAL_HW_RC523_RXTHRESHOLD_I14443A 0x55U
| RxThreshold for ISO14443A. More...
#define | PHHAL_HW_RC523_RXTHRESHOLD_I14443B 0x50U
| RxThreshold for ISO14443B. More...
#define | PHHAL_HW_RC523_RXTHRESHOLD_FELICA 0x55U
| RxThreshold for Felica. More...

## Feature selection
#define | PHHAL_HW_RC523_FEATURE_FIFO_UNDERFLOW_CHECK
| Checks for FIFO underflow during data transmission if defined. More...

## Detailed Description

Custom Configuration of hardware related settings.

## Macro Definition Documentation

## § PHHAL_HW_RC523_PRECACHED_BYTES

#define PHHAL_HW_RC523_PRECACHED_BYTES 0x40U

Maximum number of bytes to precache into FIFO before triggering a command.

## § PHHAL_HW_RC523_MODINDEX_I14443B

#define PHHAL_HW_RC523_MODINDEX_I14443B 0x11U

Default modulation index for ISO14443B.

## § PHHAL_HW_RC523_MODINDEX_FELICA

#define PHHAL_HW_RC523_MODINDEX_FELICA 0x12U

Default modulation index for Felica.

## § PHHAL_HW_RC523_MODINDEX_TARGET

#define PHHAL_HW_RC523_MODINDEX_TARGET 0xF2U

Default conductance for LoadModulation.

## § PHHAL_HW_RC523_RXTHRESHOLD_I14443A

#define PHHAL_HW_RC523_RXTHRESHOLD_I14443A 0x55U

RxThreshold for ISO14443A.

## § PHHAL_HW_RC523_RXTHRESHOLD_I14443B

#define PHHAL_HW_RC523_RXTHRESHOLD_I14443B 0x50U

RxThreshold for ISO14443B.

## § PHHAL_HW_RC523_RXTHRESHOLD_FELICA

#define PHHAL_HW_RC523_RXTHRESHOLD_FELICA 0x55U

RxThreshold for Felica.

## § PHHAL_HW_RC523_FEATURE_FIFO_UNDERFLOW_CHECK

#define PHHAL_HW_RC523_FEATURE_FIFO_UNDERFLOW_CHECK

Checks for FIFO underflow during data transmission if defined.