NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Typedefs | Functions
Component : Software
Protocol Abstraction Layer » ISO/IEC 14443-4mC
Collaboration diagram for Component : Software:

## Data Structures
struct | phpalI14443p4mC_Sw_DataParams_t
| ISO14443-4 card mode PAL parameter structure. More...

## Macros
#define | PHPAL_I14443P4MC_SW_ID 0x01U
| ID for software I18092 MT component. More...

## Typedefs
typedef void(* | pWtxTimerCallback) (uint8_t bTimerId)
| WTX timer call-back function type.

## Functions
phStatus_t | phpalI14443p4mC_Sw_Init (phpalI14443p4mC_Sw_DataParams_t *pDataParams, uint16_t wSizeOfDataParams, void *pHalDataParams, pWtxTimerCallback pWtxCallback)
| Initializes this layer. More...

## Detailed Description

## Macro Definition Documentation

## § PHPAL_I14443P4MC_SW_ID

#define PHPAL_I14443P4MC_SW_ID 0x01U

ID for software I18092 MT component.

Event posted by response time extension timer ISR. Reader library thread listens to this event and sends the RTOx packet.

## Function Documentation

## § phpalI14443p4mC_Sw_Init()

phStatus_t phpalI14443p4mC_Sw_Init | ( | phpalI14443p4mC_Sw_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams,
|  | void * | pHalDataParams,
|  | pWtxTimerCallback | pWtxCallback
| ) |  |

Initializes this layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.

Parameters

  [in] | pDataParams | Pointer to this layer's parameter structure.
  [in] | wSizeOfDataParams | Specifies the size of the data parameter structure.
  [in] | pHalDataParams | Pointer to the parameter structure of the underlying layer.
  [in] | pWtxCallback | Pointer to WTX timer call-back function