NXP NFC Reader Library v4.040.05.011646

Data Fields
phalTop_T2T_Sector Struct Reference
Application Layer » Tag Operation Layer » Component : Software

T2T Sector parameters. More...

## Data Fields
uint8_t | bAddress
| Current active Sector address.
uint8_t | bBlockAddress
| Current active block address.
uint8_t | bLockReservedOtp [32]
| Lock/reserved/OTP bytes in current Sector.
uint8_t | bValidity
| Read data validity.

## Detailed Description

T2T Sector parameters.

The documentation for this struct was generated from the following file:

- phalTop.h