NXP NFC Reader Library v4.040.05.011646

Data Fields
phalTop_T1T Struct Reference
Application Layer » Tag Operation Layer » Component : Software

T1T parameter structure. More...

## Data Fields
void * | pAlT1TDataParams
| Pointer to T1T data parameters.
uint8_t | bRwa
| Tag read/write size.
uint8_t | bTms
| Tag Memory size.
uint8_t | bTagMemoryType
| Tag memory type (static or dynamic)
uint8_t | bTerminatorTlvPresence
| Terminator TLV presence; 1 -present, 0 - not present.
uint8_t | bLockTlvCount
| Number of lock TLV present in tag.
uint8_t | bMemoryTlvCount
| Number of memory TLV present in tag.
uint16_t | wNdefHeaderAddr
| Header offset of first NDEF message.
uint16_t | wNdefMsgAddr
| NDEF message start address.
uint8_t | bUid [4]
| T1T UID.
phalTop_T1T_MemCtrlTlv_t | asMemCtrlTlv [PHAL_TOP_T1T_MAX_MEM_CTRL_TLV]
| Memory TLV details for each TLV present.
phalTop_T1T_LockCtrlTlv_t | asLockCtrlTlv [PHAL_TOP_T1T_MAX_LOCK_CTRL_TLV]
| Lock TLV details for each TLV present.
phalTop_TIT_Segment_t | sSegment
| Current segment details.

## Detailed Description

T1T parameter structure.

The documentation for this struct was generated from the following file:

- phalTop.h