NXP NFC Reader Library v4.040.05.011646

Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - w -

- wActPollGTimeUs : phacDiscLoop_Sw_DataParams
- wAdditionalInfo : phalFelica_Sw_DataParams_t , phalMfdf_Sw_DataParams_t , phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t , phpalSli15693_Sw_DataParams
- waPasPollGTimeUs : phacDiscLoop_Sw_DataParams
- wAppBufferSize : phceT4T_Sw_DataParams
- wAtqa : phNfcLib_PeerInfo_t
- wBlockNumber : phNfcLib_I15693
- wByteAddr : phalTop_T1T_LockCtrlTlv , phalTop_T1T_MemCtrlTlv , phalTop_T2T_LockCtrlTlv , phalTop_T2T_MemCtrlTlv
- wCcContentLen : phceT4T_Sw_DataParams
- wCcFileSize : phceT4T_Sw_DataParams
- wCCLEN : phalTop_T4T
- wCfgShadow : phhalHw_Pn5180_DataParams_t , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wCrc : phalMfdf_Sw_DataParams_t
- wCurrentSlotCount : phhalHw_PN7462AU_DataParams , phhalHw_Rc663_DataParams_t
- wDetectionTimeUs : phhalHw_Rc663_DataParams_t
- wErrorCode : phacDiscLoop_Sw_DataParams
- wExitStatus : phceT4T_Sw_DataParams
- wFieldOffTime : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wFieldRecoveryTime : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wFrameOpt : phTools_Q
- wHigherLayerInfLen : phpalI14443p3b_Sw_DataParams_t
- wHigherLayerRespLen : phpalI14443p3b_Sw_DataParams_t
- wHigherLayerRespSize : phpalI14443p3b_Sw_DataParams_t
- wId : phacDiscLoop_Sw_DataParams , phalFelica_Sw_DataParams_t , phalI15693_Sw_DataParams_t , phalI18000p3m3_Sw_DataParams_t , phalMfc_Sw_DataParams_t , phalMfdf_Sw_DataParams_t , phalMful_Sw_DataParams_t , phalSli_Sw_DataParams_t , phalT1T_Sw_DataParams_t , phalTop_Sw_DataParams , phbalReg_Type_t , phceT4T_Sw_DataParams , phCidManager_Sw_DataParams_t , phCryptoRng_Sw_DataParams_t , phCryptoSym_Sw_DataParams_t , phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t , phKeyStore_Sw_DataParams_t , phlnLlcp_Sw_DataParams , phNfcLib_DataParams_t , phnpSnep_Sw_DataParams , phpalFelica_Sw_DataParams_t , phpalI14443p3a_Sw_DataParams_t , phpalI14443p3b_Sw_DataParams_t , phpalI14443p4_Sw_DataParams_t , phpalI14443p4a_Sw_DataParams_t , phpalI14443p4mC_Sw_DataParams_t , phpalI18000p3m3_Sw_DataParams_t , phpalI18092mPI_Sw_DataParams_t , phpalI18092mT_Sw_DataParams_t , phpalMifare_Sw_DataParams_t , phpalSli15693_Sw_DataParams , phPlatform_DataParams_t
- wKeepIV : phCryptoSym_Sw_DataParams_t
- wKeyType : phCryptoSym_Sw_DataParams_t , phKeyStore_Sw_KeyEntry_t
- wLastTxLen : phpalI14443p4mC_Sw_DataParams_t , phpalI18092mPI_Sw_DataParams_t , phpalI18092mT_Sw_DataParams_t
- wLc : phceT4T_Sw_DataParams
- wLength : phalTop_T1T_ProprietaryTlv
- wLpcdReference : phhalHw_Pn5180_DataParams_t
- wMaxFileSize : phalTop_T4T
- wMaxNdefLength : phalTop_Sw_DataParams
- wMaxPrecachedBytes : phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wMiu : phlnLlcp_LMDataParams
- wMLc : phalTop_T4T
- wMLe : phalTop_T4T
- wMlen : phalTop_T5T
- wNdefHeaderAddr : phalTop_T1T , phalTop_T2T , phalTop_T5T
- wNdefLength : phalTop_Sw_DataParams
- wNdefMsgAddr : phalTop_T1T , phalTop_T2T , phalTop_T5T
- wNoOfKeyEntries : phKeyStore_Sw_DataParams_t
- wNoOfKUCEntries : phKeyStore_Sw_DataParams_t
- wNoOfVersions : phKeyStore_Sw_DataParams_t
- wNumBlocks : phNfcLib_I15693
- wOffset : phalTop_T1T_LockCtrlTlv , phalTop_T1T_MemCtrlTlv , phalTop_T1T_ProprietaryTlv , phalTop_T2T_LockCtrlTlv , phalTop_T2T_MemCtrlTlv
- wOpeMode : phhalHw_PN7462AU_DataParams
- wOption : phNfcLib_MFdf
- wParity : phhalHw_PN7462AU_DataParams
- wPayLoadLen : phalMfdf_Sw_DataParams_t
- wPowerDownTimeMs : phhalHw_Rc663_DataParams_t
- wProtParams : phacDiscLoop_TargetParams
- wRefNoKUC : phKeyStore_Sw_KeyEntry_t
- wRMiu : phlnLlcp_Transport_Socket
- wRxBufferLen : phacDiscLoop_TargetParams
- wRxBufLen : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wRxBufSize : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wRxBufStartPos : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wRxDataRate : phhalHw_PN7462AU_DataParams
- wRxSubCarrier : phhalHw_PN7462AU_DataParams
- wSelectedFileId : phceT4T_Sw_DataParams
- wSharedDataLen : phceT4T_Sw_DataParams
- wStatus : phlnLlcp_Transport_Socket
- wStatusWord : phceT4T_Sw_DataParams
- wTargetMode : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t
- wTimeoutReloadVal : phhalHw_Rc523_DataParams_t
- wTimingMode : phhalHw_Pn5180_DataParams_t , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wTxBufLen : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wTxBufSize : phhalHw_Pn5180_DataParams_t , phhalHw_PN7462AU_DataParams , phhalHw_Rc523_DataParams_t , phhalHw_Rc663_DataParams_t
- wTxBufStartPos : phhalHw_Pn5180_DataParams_t
- wTxDataRate : phhalHw_PN7462AU_DataParams
- wTxWaitReloadVal : phhalHw_Rc523_DataParams_t
- wUiiLength : phNfcLib_PeerInfo_t
- wUiiMaskLength : phNfcLib_I18000p3m3
- wVersion : phKeyStore_Sw_KeyVersionPair_t
- wWakeupCounterInMs : phhalHw_Pn5180_DataParams_t
- wWks : phlnLlcp_LMDataParams
- wWtDelta : phpalI14443p4mC_Sw_DataParams_t