NXP NFC Reader Library v4.040.05.011646

Data Fields
phCryptoRng_Sw_DataParams_t Struct Reference
Common » CryptoRng » Component : Software

Software parameter structure. More...

## Data Fields
uint16_t | wId
| Layer ID for this component, NEVER MODIFY!
void * | pCryptoDataParams
| Data parameter structure for the AES engine.
uint32_t | dwRequestCounter
| Counts the amount of requests between two seeding procedures. More...

## Detailed Description

Software parameter structure.

## Field Documentation

## § dwRequestCounter

uint32_t phCryptoRng_Sw_DataParams_t::dwRequestCounter

Counts the amount of requests between two seeding procedures.

Note: according to NIST SP800-90 for AES this is 2^48, for storage reasons the limit is set to 2^32 in this particular implementation.

The documentation for this struct was generated from the following file:

- phCryptoRng.h