NXP NFC Reader Library v4.040.05.011646

Data Fields
phlnLlcp_LMDataParams Struct Reference
Link Abstraction Layer » NFCForum-LLCP » Component : Software

Link Management parameters that are expected by LLC. More...

## Data Fields
uint8_t | bVersion
| Denotes major and minor release levels of the LLCP specification. More...
uint8_t | bLto
| Link Timeout (LTO) specifies the local link timeout interval guarantee. More...
uint8_t | bOpt
| Option. More...
uint16_t | wMiu
| maximum information unit (MIU) is max number of octets in information field of an LLC PDU. More...
uint16_t | wWks
| Well-Known Service List. More...
uint16_t | bAvailableTlv
| Bit mask for TLVs availability. More...

## Detailed Description

Link Management parameters that are expected by LLC.

## Field Documentation

## § bVersion

uint8_t phlnLlcp_LMDataParams::bVersion

Denotes major and minor release levels of the LLCP specification.

## § bLto

uint8_t phlnLlcp_LMDataParams::bLto

Link Timeout (LTO) specifies the local link timeout interval guarantee.

## § bOpt

uint8_t phlnLlcp_LMDataParams::bOpt

Option.

## § wMiu

uint16_t phlnLlcp_LMDataParams::wMiu

maximum information unit (MIU) is max number of octets in information field of an LLC PDU.

## § wWks

uint16_t phlnLlcp_LMDataParams::wWks

Well-Known Service List.

## § bAvailableTlv

uint16_t phlnLlcp_LMDataParams::bAvailableTlv

Bit mask for TLVs availability.

The documentation for this struct was generated from the following file:

- phlnLlcp.h