NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Functions
Component : Linux Kernel Spi
Bus Abstraction Layer

Component without functionality to ease implementation of additional busses. More...

Collaboration diagram for Component : Linux Kernel Spi:

## Data Structures
struct | phbalReg_LinuxKernelSpi_DataParams_t
| BAL Linux Kernel Spi parameter structure. More...

## Macros
#define | PHBAL_REG_LINUX_KERNEL_SPI_ID 0x11U
| ID for Linux Kernel Spi BAL component.

## Functions
phStatus_t | phbalReg_LinuxKernelSpi_Init (phbalReg_LinuxKernelSpi_DataParams_t *pDataParams, uint16_t wSizeOfDataParams)
| Initialise the BAL Linux Kernel Spi layer. More...

## Detailed Description

Component without functionality to ease implementation of additional busses.

## Function Documentation

## § phbalReg_LinuxKernelSpi_Init()

phStatus_t phbalReg_LinuxKernelSpi_Init | ( | phbalReg_LinuxKernelSpi_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams
| ) |  |

Initialise the BAL Linux Kernel Spi layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.
  PH_ERR_INVALID_DATA_PARAMS | Parameter structure size is invalid.

Parameters

  [in] | pDataParams | Pointer to this layer's parameter structure.
  [in] | wSizeOfDataParams | Specifies the size of the data parameter structure.