NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Functions
Component : Software
Application Layer » Type 1 tag
Collaboration diagram for Component : Software:

## Data Structures
struct | phalT1T_Sw_DataParams_t
| Private parameter structure. More...

## Macros
#define | PHAL_T1T_SW_ID 0x01U
| ID for Software T1T layer.

## Functions
phStatus_t | phalT1T_Sw_Init (phalT1T_Sw_DataParams_t *pDataParams, uint16_t wSizeOfDataParams, void *pPalI14443p3aDataParams)
| Initialise this layer. More...

## Detailed Description

## Function Documentation

## § phalT1T_Sw_Init()

phStatus_t phalT1T_Sw_Init | ( | phalT1T_Sw_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams,
|  | void * | pPalI14443p3aDataParams
| ) |  |

Initialise this layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.

Parameters

  [in] | pDataParams | Pointer to this layer's parameter structure.
  [in] | wSizeOfDataParams | Specifies the size of the data parameter structure.
  [in] | pPalI14443p3aDataParams | Pointer to the parameter structure of the underlying ISO14443-3 layer.