NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Typedefs | Functions
Component : Software
Protocol Abstraction Layer » ISO/IEC 18092 Mode Target
Collaboration diagram for Component : Software:

## Data Structures
struct | phpalI18092mT_Sw_DataParams_t
| ISO18092 mode passive target parameter structure. More...

## Macros
#define | PHPAL_I18092MT_SW_ID 0x01U
| ID for software I18092 MT component.
#define | PHPAL_I18092MT_NFCID3_LENGTH 0x0AU
| Length of NFCID3. More...

## Typedefs
typedef void(* | pRtoxTimerCallback) (uint8_t bTimerId)
| Typedef for the RTOX call back function.

## Functions
phStatus_t | phpalI18092mT_Sw_Init (phpalI18092mT_Sw_DataParams_t *pDataParams, uint16_t wSizeOfDataParams, void *pHalDataParams, pRtoxTimerCallback pRtoxCallback)
| Initialize this layer. More...

## Detailed Description

## Macro Definition Documentation

## § PHPAL_I18092MT_NFCID3_LENGTH

#define PHPAL_I18092MT_NFCID3_LENGTH 0x0AU

Length of NFCID3.

Event posted by response time extension timer ISR. Reader library thread listens to this event and sends the RTOx packet.

## Function Documentation

## § phpalI18092mT_Sw_Init()

phStatus_t phpalI18092mT_Sw_Init | ( | phpalI18092mT_Sw_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams,
|  | void * | pHalDataParams,
|  | pRtoxTimerCallback | pRtoxCallback
| ) |  |

Initialize this layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.
  PH_ERR_INVALID_DATA_PARAMS | Wrong pointer to this layer's parameter structure is sent.

Parameters

  [in] | pDataParams | Pointer to this layer's parameter structure.
  [in] | wSizeOfDataParams | Specifies the size of the data parameter structure.
  [in] | pHalDataParams | Pointer to the parameter structure of the underlying HAL.
  [in] | pRtoxCallback | Callback to be executed by the RTOX timer. Implementation provided by user.