NXP NFC Reader Library v4.040.05.011646

Data Fields
phacDiscLoop_Sw_TypeA_Info::phacDiscLoop_TypeA_I3P3 Struct Reference

Structure info required for ISO/IEC 14443 communication. More...

## Data Fields
uint8_t | aAtqa [PHAC_DISCLOOP_I3P3A_MAX_ATQA_LENGTH]
| ATQA received from ISO/IEC 14443A compliant device. More...
uint8_t | aUid [PHAC_DISCLOOP_I3P3A_MAX_UID_LENGTH]
| Contains known UID bytes for the given cascade level. More...
uint8_t | bUidSize
| Size of the UID that was received from the PICC. More...
uint8_t | aSak
| Select acknowledge from the ISO/IEC 14443A type A card. More...

## Detailed Description

Structure info required for ISO/IEC 14443 communication.

## Field Documentation

## § aAtqa

uint8_t phacDiscLoop_Sw_TypeA_Info::phacDiscLoop_TypeA_I3P3::aAtqa[PHAC_DISCLOOP_I3P3A_MAX_ATQA_LENGTH]

ATQA received from ISO/IEC 14443A compliant device.

## § aUid

uint8_t phacDiscLoop_Sw_TypeA_Info::phacDiscLoop_TypeA_I3P3::aUid[PHAC_DISCLOOP_I3P3A_MAX_UID_LENGTH]

Contains known UID bytes for the given cascade level.

## § bUidSize

uint8_t phacDiscLoop_Sw_TypeA_Info::phacDiscLoop_TypeA_I3P3::bUidSize

Size of the UID that was received from the PICC.

## § aSak

uint8_t phacDiscLoop_Sw_TypeA_Info::phacDiscLoop_TypeA_I3P3::aSak

Select acknowledge from the ISO/IEC 14443A type A card.

The documentation for this struct was generated from the following file:

- phacDiscLoop.h