NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Functions
Component : Software
Application Layer » MIFARE DESFire (R)
Collaboration diagram for Component : Software:

## Data Structures
struct | phalMfdf_Sw_DataParams_t
| struct phalMfdf_Sw_DataParams_t More...

## Macros
#define | PHAL_MFDF_SW_ID 0x01U
| ID for Software MF DesFire layer. More...

## Functions
phStatus_t | phalMfdf_Sw_Init (phalMfdf_Sw_DataParams_t *pDataParams, uint16_t wSizeOfDataParams, void *pPalMifareDataParams, void *pKeyStoreDataParams, void *pCryptoDataParamsEnc, void *pCryptoRngDataParams, void *pHalDataParams)
| Initialise this layer. More...

## Detailed Description

## Macro Definition Documentation

## § PHAL_MFDF_SW_ID

#define PHAL_MFDF_SW_ID 0x01U

ID for Software MF DesFire layer.

## Function Documentation

## § phalMfdf_Sw_Init()

phStatus_t phalMfdf_Sw_Init | ( | phalMfdf_Sw_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams,
|  | void * | pPalMifareDataParams,
|  | void * | pKeyStoreDataParams,
|  | void * | pCryptoDataParamsEnc,
|  | void * | pCryptoRngDataParams,
|  | void * | pHalDataParams
| ) |  |

Initialise this layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.

Parameters

  [in] | pDataParams | Pointer to this layer's parameter structure.
  [in] | wSizeOfDataParams | Specifies the size of the data parameter structure
  [in] | pPalMifareDataParams | Pointer to a palMifare component context.
  [in] | pKeyStoreDataParams | Pointer to Key Store data parameters.
  [in] | pCryptoDataParamsEnc | Pointer to a Crypto component context for encryption.
  [in] | pCryptoRngDataParams | Pointer to a CryptoRng component context.
  [in] | pHalDataParams | Pointer to the HAL parameters structure.