NXP NFC Reader Library v4.040.05.011646

Data Fields
phNfcLib_MFUL Struct Reference

Defines parameters that needs be provided by User to communicate with MIFare Ultralight card. More...

## Data Fields
phNfcLib_MFUL_Commands_t | bCommand
| [In] Mifare Ultralight command needs to be provided. More...
uint8_t | bPageNumber
| [In] Page number on which Mifare Ultralight command to be executed. More...

## Detailed Description

Defines parameters that needs be provided by User to communicate with MIFare Ultralight card.

## Field Documentation

## § bCommand

phNfcLib_MFUL_Commands_t phNfcLib_MFUL::bCommand

[In] Mifare Ultralight command needs to be provided.

## § bPageNumber

uint8_t phNfcLib_MFUL::bPageNumber

[In] Page number on which Mifare Ultralight command to be executed.

The documentation for this struct was generated from the following file:

- phNfcLib.h