NXP NFC Reader Library v4.040.05.011646

Data Structures | Macros | Functions
Component : Linux User I2C
Bus Abstraction Layer

Component without functionality to ease implementation of additional busses. More...

Collaboration diagram for Component : Linux User I2C:

## Data Structures
struct | phbalReg_LinuxUserI2C_DataParams_t
| BAL Linux User I2C parameter structure. More...

## Macros
#define | PHBAL_REG_LINUX_USER_I2C_ID 0x13U
| ID for Linux User I2C BAL component.

## Functions
phStatus_t | phbalReg_LinuxUserI2C_Init (phbalReg_LinuxUserI2C_DataParams_t *pDataParams, uint16_t wSizeOfDataParams)
| Initialise the BAL Linux User I2C layer. More...

## Detailed Description

Component without functionality to ease implementation of additional busses.

## Function Documentation

## § phbalReg_LinuxUserI2C_Init()

phStatus_t phbalReg_LinuxUserI2C_Init | ( | phbalReg_LinuxUserI2C_DataParams_t * | pDataParams,
|  | uint16_t | wSizeOfDataParams
| ) |  |

Initialise the BAL Linux User I2C layer.

Returns
  Status code

Return values

  PH_ERR_SUCCESS | Operation successful.
  PH_ERR_INVALID_DATA_PARAMS | Parameter structure size is invalid.