NXP NFC Reader Library v4.040.05.011646

Data Fields
phlnLlcp_Socket_Seq Struct Reference
Link Abstraction Layer » NFCForum-LLCP » Component : Software

Socket Sequence. More...

## Data Fields
uint8_t | bSendState_Vs
| Denote the sequence number of the next in-sequence I PDU to be sent. More...
uint8_t | bSendAck_Vsa
| Denote the most recently received N(R) value for a specific data link connection. More...
uint8_t | bRxState_Vr
| Denote the sequence number of the next in-sequence I PDU to be received. More...
uint8_t | bRxAck_Vra
| Denote the most recently sent N(R) value for a specific data link connection. More...

## Detailed Description

Socket Sequence.

## Field Documentation

## § bSendState_Vs

uint8_t phlnLlcp_Socket_Seq::bSendState_Vs

Denote the sequence number of the next in-sequence I PDU to be sent.

## § bSendAck_Vsa

uint8_t phlnLlcp_Socket_Seq::bSendAck_Vsa

Denote the most recently received N(R) value for a specific data link connection.

## § bRxState_Vr

uint8_t phlnLlcp_Socket_Seq::bRxState_Vr

Denote the sequence number of the next in-sequence I PDU to be received.

## § bRxAck_Vra

uint8_t phlnLlcp_Socket_Seq::bRxAck_Vra

Denote the most recently sent N(R) value for a specific data link connection.

The documentation for this struct was generated from the following file:

- phlnLlcp.h