NXP NFC Reader Library v4.040.05.011646

Data Fields
phpalI14443p3a_Sw_DataParams_t Struct Reference
Protocol Abstraction Layer » ISO/IEC 14443-3A » Component : Software

Software PAL-ISO14443P3A parameter structure. More...

## Data Fields
uint16_t | wId
| Layer ID for this component, NEVER MODIFY!
void * | pHalDataParams
| Pointer to the parameter structure of the underlying layer. More...
uint8_t | abUid [10]
| Array holding the activated UID. More...
uint8_t | bUidLength
| Length of UID stored in `abUid`. More...
uint8_t | bUidComplete
| Whether the UID is complete (`1`) or not (`0`). More...
uint8_t | bOpeMode
| Operation mode. More...
uint8_t | bPollCmd
| Used to differentiate which command to send REQA or WakeUpA command for polling.

## Detailed Description

Software PAL-ISO14443P3A parameter structure.

## Field Documentation

## § pHalDataParams

void* phpalI14443p3a_Sw_DataParams_t::pHalDataParams

Pointer to the parameter structure of the underlying layer.

## § abUid

uint8_t phpalI14443p3a_Sw_DataParams_t::abUid[10]

Array holding the activated UID.

## § bUidLength

uint8_t phpalI14443p3a_Sw_DataParams_t::bUidLength

Length of UID stored in `abUid`.

## § bUidComplete

uint8_t phpalI14443p3a_Sw_DataParams_t::bUidComplete

Whether the UID is complete (`1`) or not (`0`).

## § bOpeMode

uint8_t phpalI14443p3a_Sw_DataParams_t::bOpeMode

Operation mode.

One of NFC, EMVCo, ISO.

The documentation for this struct was generated from the following file:

- phpalI14443p3a.h