NXP NFC Reader Library v4.040.05.011646

Macros
NXP Build
Other

Controls build behaviour of components. More...

Collaboration diagram for NXP Build:

## Macros
#define | NXPBUILD__PHBAL_REG
| < DEBUG build definition More...
#define | NXPBUILD__PHHAL_HW
| Generic HAL definition.
#define | NXPBUILD__PHPAL_I14443P3A
| Generic PAL ISO 14443-3A definition.
#define | NXPBUILD__PHPAL_I14443P3B
| Generic PAL ISO 14443-3B definition.
#define | NXPBUILD__PHPAL_I14443P4A
| Generic PAL ISO 14443-4A definition.
#define | NXPBUILD__PHPAL_I14443P4
| Generic PAL ISO 14443-4 definition.
#define | NXPBUILD__PHPAL_I14443P4MC
| Generic PAL ISO 18092 target definition.
#define | NXPBUILD__PHPAL_MIFARE
| Generic PAL MIFARE definition.
#define | NXPBUILD__PHPAL_SLI15693
| Generic PAL Sli 15693 definition.
#define | NXPBUILD__PHPAL_FELICA
| < Enable handling of multiple Felica card response More...
#define | NXPBUILD__PHPAL_EPCUID
| Generic PAL ICode EPC/UID definition.
#define | NXPBUILD__PHPAL_I18000P3M3
| Generic PAL I18000p3m3 definition.
#define | NXPBUILD__PHPAL_I18092MPI
| Generic PAL ISO 18092 definition.
#define | NXPBUILD__PHPAL_I18092MT
| Generic PAL ISO 18092 target definition.
#define | NXPBUILD__PHAC_DISCLOOP
| Generic dicovery loop component.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TAGS
| Detect Passive TypeA Tags/Peers.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_TAGS
| Detect TypeB Tags.
#define | NXPBUILD__PHAC_DISCLOOP_TARGET
| Configure Target Mode.
#define | NXPBUILD__PH_OSAL
| Generic OSAL definition.
#define | NXPBUILD__PHAL_FELICA
| Generic AL Felica definition.
#define | NXPBUILD__PHAL_MFC
| Generic AL MIFARE Classic definition.
#define | NXPBUILD__PHAL_MFDF
| Generic AL MIFARE Desfire definition.
#define | NXPBUILD__PHAL_MFUL
| Generic AL MIFARE Ultralight definition.
#define | NXPBUILD__PHAL_T1T
| Generic AL Type 1 Tag definition.
#define | NXPBUILD__PHAL_TOP
| Generic AL Tag Operations.
#define | NXPBUILD__PHCE_T4T
| Generic HCE.
#define | NXPBUILD__PHAL_I15693
| Generic AL I15693 definition.
#define | NXPBUILD__PHAL_SLI
| Generic AL Sli definition.
#define | NXPBUILD__PHAL_I18000P3M3
| Generic AL I18000p3m3 definition.
#define | NXPBUILD__PH_CIDMANAGER
| Generic CID Manager definition.
#define | NXPBUILD__PH_CRYPTOSYM
| Generic Crypto Sym definition.
#define | NXPBUILD__PH_CRYPTORNG
| Generic CryptoRng definition.
#define | NXPBUILD__PH_KEYSTORE
| Generic KeyStore definition.
#define | NXPBUILD__PHLN_LLCP
| Generic Link layer definition.
#define | NXPBUILD__PHNP_SNEP
| Generic HAL definition.
#define | NXPBUILD__PH_KINETIS
| Kinetis.
#define | NXPBUILD__PH_PLATFORM
| < DEBUG build definition More...
#define | NXPBUILD__PH_PLATFORM
| < DEBUG build definition More...
#define | NXPBUILD__PH_KINETIS_K82
| K82 Freedom Board.
#define | NXPBUILD__PHHAL_HW_PN7462AU
| NFC Controller PN7462AU HAL. More...
#define | NXPBUILD__PHHAL_HW_PN7462AU
| NFC Controller PN7462AU HAL. More...
#define | NXPBUILD__PHHAL_HW_PN7462AU
| NFC Controller PN7462AU HAL. More...
#define | NXPBUILD__PH_LPC1769
| Host Controller LPC1769. More...
#define | NXPBUILD__PH_LPC1769
| Host Controller LPC1769. More...
#define | NXPBUILD__PH_LPC11U68
| Host Controller LPC11U68. More...
#define | NXPBUILD__PH_LPC11U68
| Host Controller LPC11U68. More...
#define | NXPBUILD__PH_RASPBERRY_PI
| Host Controller RaspBerry Pi. More...
#define | NXPBUILD__PH_RASPBERRY_PI
| Host Controller RaspBerry Pi. More...
#define | NXPBUILD__PH_UDOO_NEO
| Host Controller udoo-neo.
#define | NXPBUILD__PH_OSAL_LINUX
| OSAL Implementation of POSIX is included. More...
#define | NXPBUILD__PH_OSAL_LINUX
| OSAL Implementation of POSIX is included. More...
#define | NXPBUILD__PH_OSAL_NULLOS
| OSAL Implementation of NULL OS is included. More...
#define | NXPBUILD__PH_OSAL_NULLOS
| OSAL Implementation of NULL OS is included. More...
#define | NXPBUILD__PH_OSAL_NULLOS
| OSAL Implementation of NULL OS is included. More...
#define | NXPBUILD__PH_OSAL_FREERTOS
| OSAL Implementation of Free RTOS is included. More...
#define | NXPBUILD__PH_OSAL_FREERTOS
| OSAL Implementation of Free RTOS is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_SPI
| LPCOpenStack SPI BAL Component is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_SPI
| LPCOpenStack SPI BAL Component is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_I2C
| LPCOpenStack SPI I2C Component is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_I2C
| LPCOpenStack SPI I2C Component is included. More...
#define | NXPBUILD__PHBAL_REG_PI_SPI
| Raspberry Linux UM/KM SPI BAL Component is included.
#define | NXPBUILD__PHBAL_REG_PI_SPI
| Raspberry Linux UM/KM SPI BAL Component is included.
#define | NXPBUILD__PHBAL_REG_PI_I2C
| Raspberry Linux UM I2C BAL Component is included.
#define | NXPBUILD__PHBAL_REG_PI_I2C
| Raspberry Linux UM I2C BAL Component is included.
#define | NXPBUILD__PHHAL_HW_RC523
| RC523 HAL Component is included. More...
#define | NXPBUILD__PHHAL_HW_RC523
| RC523 HAL Component is included. More...
#define | NXPBUILD__PHHAL_HW_RC663
| RC663 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_RC663
| RC663 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_PN5180
| PN5180 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_PN5180
| PN5180 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_TARGET
| Dependency checking if target mode macros should be enabled.
#define | NXPBUILD__PHHAL_HW_TARGET
| Dependency checking if target mode macros should be enabled.
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_SLI15693_SW
| PAL SLI 15693 Component is included. More...
#define | NXPBUILD__PHPAL_I18000P3M3_SW
| PAL ISO 18000p3m3 Component is included. More...
#define | NXPBUILD__PHPAL_I18000P3M3_SW
| PAL ISO 18000p3m3 Component is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_LPCD
| SRC to enable LPCD is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_LPCD
| SRC to enable LPCD is included. More...
#define | NXPBUILD__PHAL_I18000P3M3_SW
| AL ISO18000p3m3 SW Component is included.
#define | NXPBUILD__PHAL_I18000P3M3_SW
| AL ISO18000p3m3 SW Component is included.
#define | NXPBUILD__PHCE_T4T_SW
| AL HCE T2AT SW Component is included.
#define | NXPBUILD__PHPAL_I18092MPI_SW
| PAL ISO18092 (P2P) SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MPI_SW
| PAL ISO18092 (P2P) SW Component is included. More...
#define | NXPBUILD__PHLN_LLCP_SW
| Link LLCP SW Component is included.
#define | NXPBUILD__PHPAL_I14443P3A_SW
| PAL ISO 14443-3A SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P3B_SW
| PAL ISO 14443-3B SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4A_SW
| PAL ISO 14443-4A SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4_SW
| PAL ISO 14443-4 SW Component is included. More...
#define | NXPBUILD__PHPAL_MIFARE_SW
| PAL MIFARE SW Component is included.
#define | NXPBUILD__PHPAL_FELICA_SW
| PAL Felica SW Component is included. More...
#define | NXPBUILD__PHPAL_EPCUID_SW
| < If FE HAL is RC663, then include EPC UID PAL as required, otherwise exclude. More...
#define | NXPBUILD__PHAC_DISCLOOP_SW
| Discovery Loop Activity SW Component is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS
| SRC/DATA to Detect/CollRes/Activate cards such as MFC, MFUL, MFP SL1 etc is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS
| SRC/DATA to Detect cards such as NFC Forum T1T, Topaz/Jewel is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS
| SRC/DATA to Detect cards such as MFDF, MFP, T4AT NFC Forum Tag or Type A EMVCo is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS
| SRC/DATA to Detect Peer Passive Type A P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type A P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type F212 P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type F424 P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS
| SRC/DATA to Detect FeliCa Cards is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS
| SRC/DATA to Detect Peer Passive Type F P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_I3P3B_TAGS
| SRC/DATA to Detect Type B Cards that operate at Layer3 level is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_I3P4B_TAGS
| SRC/DATA to Detect Type B Cards such as NFC Forum Type 4 Tags, EMVCo Type B Cards etc is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEV_TAGS
| SRC/DATA to Detect Type V Cards such as ICODE SLI/SLIX/SLI2/Tesa Cards is included.
#define | NXPBUILD__PHAC_DISCLOOP_I18000P3M3_TAGS
| SRC/DATA to Detect ICODE ILT Cards such as SMARTRAC StackIt Cards is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE
| SRC to Initialize Type A passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE
| SRC to Initialize Type A active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE
| SRC to Initialize Type F212 passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE
| SRC to Initialize Type F212 active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE
| SRC to Initialize Type F424 passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE
| SRC to Initialize Type F424 active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHNFCLIB
| Simplified API Interface, If enabling this the entry point should be this component in the application.
#define | NXPBUILD__PH_CIDMANAGER_SW
| CID Manager SW Component is included. More...
#define | NXPBUILD__PH_KEYSTORE_SW
| SW KeyStore Component is included. More...
#define | NXPBUILD__PH_CRYPTOSYM_SW
| Crypto Symbols SW Component is included. More...
#define | NXPBUILD__PH_CRYPTORNG_SW
| Crypto RNG SW Component is included. More...
#define | NXPBUILD__PHAL_FELICA_SW
| AL FeliCa SW Component is included.
#define | NXPBUILD__PHAL_MFC_SW
| AL Mifare Classic SW Component is included.
#define | NXPBUILD__PHAL_MFUL_SW
| AL Mifare Ultrlight SW Component is included.
#define | NXPBUILD__PHAL_MFDF_SW
| AL Mifare DesFire SW Component is included.
#define | NXPBUILD__PHAL_T1T_SW
| AL Type T1 Tag SW Component is included.
#define | NXPBUILD__PHAL_I15693_SW
| AL ISO 15693 SW Component is included.
#define | NXPBUILD__PHAL_SLI_SW
| AL SLI SW Component is included.
#define | NXPBUILD__PHAL_TOP_SW
| AL for TagOps Mapping SW Component is included.Required for NDEF operations.
#define | NXPBUILD__PHNP_SNEP_SW
| Protocol SNEP SW Component is included.
#define | NXPBUILD__PH_PLATFORM
| < DEBUG build definition More...
#define | NXPBUILD__PH_PLATFORM
| < DEBUG build definition More...
#define | NXPBUILD__PH_KINETIS_K82
| K82 Freedom Board.
#define | NXPBUILD__PHHAL_HW_PN7462AU
| NFC Controller PN7462AU HAL. More...
#define | NXPBUILD__PHHAL_HW_PN7462AU
| NFC Controller PN7462AU HAL. More...
#define | NXPBUILD__PHHAL_HW_PN7462AU
| NFC Controller PN7462AU HAL. More...
#define | NXPBUILD__PH_LPC1769
| Host Controller LPC1769. More...
#define | NXPBUILD__PH_LPC1769
| Host Controller LPC1769. More...
#define | NXPBUILD__PH_LPC11U68
| Host Controller LPC11U68. More...
#define | NXPBUILD__PH_LPC11U68
| Host Controller LPC11U68. More...
#define | NXPBUILD__PH_RASPBERRY_PI
| Host Controller RaspBerry Pi. More...
#define | NXPBUILD__PH_RASPBERRY_PI
| Host Controller RaspBerry Pi. More...
#define | NXPBUILD__PH_UDOO_NEO
| Host Controller udoo-neo.
#define | NXPBUILD__PH_OSAL_LINUX
| OSAL Implementation of POSIX is included. More...
#define | NXPBUILD__PH_OSAL_LINUX
| OSAL Implementation of POSIX is included. More...
#define | NXPBUILD__PH_OSAL_NULLOS
| OSAL Implementation of NULL OS is included. More...
#define | NXPBUILD__PH_OSAL_NULLOS
| OSAL Implementation of NULL OS is included. More...
#define | NXPBUILD__PH_OSAL_NULLOS
| OSAL Implementation of NULL OS is included. More...
#define | NXPBUILD__PH_OSAL_FREERTOS
| OSAL Implementation of Free RTOS is included. More...
#define | NXPBUILD__PH_OSAL_FREERTOS
| OSAL Implementation of Free RTOS is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_SPI
| LPCOpenStack SPI BAL Component is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_SPI
| LPCOpenStack SPI BAL Component is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_I2C
| LPCOpenStack SPI I2C Component is included. More...
#define | NXPBUILD__PHBAL_REG_LPCOPEN_I2C
| LPCOpenStack SPI I2C Component is included. More...
#define | NXPBUILD__PHBAL_REG_PI_SPI
| Raspberry Linux UM/KM SPI BAL Component is included.
#define | NXPBUILD__PHBAL_REG_PI_SPI
| Raspberry Linux UM/KM SPI BAL Component is included.
#define | NXPBUILD__PHBAL_REG_PI_I2C
| Raspberry Linux UM I2C BAL Component is included.
#define | NXPBUILD__PHBAL_REG_PI_I2C
| Raspberry Linux UM I2C BAL Component is included.
#define | NXPBUILD__PHHAL_HW_RC523
| RC523 HAL Component is included. More...
#define | NXPBUILD__PHHAL_HW_RC523
| RC523 HAL Component is included. More...
#define | NXPBUILD__PHHAL_HW_RC663
| RC663 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_RC663
| RC663 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_PN5180
| PN5180 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_PN5180
| PN5180 HAL Component is included.
#define | NXPBUILD__PHHAL_HW_TARGET
| Dependency checking if target mode macros should be enabled.
#define | NXPBUILD__PHHAL_HW_TARGET
| Dependency checking if target mode macros should be enabled.
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_SLI15693_SW
| PAL SLI 15693 Component is included. More...
#define | NXPBUILD__PHPAL_I18000P3M3_SW
| PAL ISO 18000p3m3 Component is included. More...
#define | NXPBUILD__PHPAL_I18000P3M3_SW
| PAL ISO 18000p3m3 Component is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_LPCD
| SRC to enable LPCD is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_LPCD
| SRC to enable LPCD is included. More...
#define | NXPBUILD__PHAL_I18000P3M3_SW
| AL ISO18000p3m3 SW Component is included.
#define | NXPBUILD__PHAL_I18000P3M3_SW
| AL ISO18000p3m3 SW Component is included.
#define | NXPBUILD__PHCE_T4T_SW
| AL HCE T2AT SW Component is included.
#define | NXPBUILD__PHPAL_I18092MPI_SW
| PAL ISO18092 (P2P) SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MPI_SW
| PAL ISO18092 (P2P) SW Component is included. More...
#define | NXPBUILD__PHLN_LLCP_SW
| Link LLCP SW Component is included.
#define | NXPBUILD__PHPAL_I14443P3A_SW
| PAL ISO 14443-3A SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P3B_SW
| PAL ISO 14443-3B SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4A_SW
| PAL ISO 14443-4A SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4_SW
| PAL ISO 14443-4 SW Component is included. More...
#define | NXPBUILD__PHPAL_MIFARE_SW
| PAL MIFARE SW Component is included.
#define | NXPBUILD__PHPAL_FELICA_SW
| PAL Felica SW Component is included. More...
#define | NXPBUILD__PHPAL_EPCUID_SW
| < If FE HAL is RC663, then include EPC UID PAL as required, otherwise exclude. More...
#define | NXPBUILD__PHAC_DISCLOOP_SW
| Discovery Loop Activity SW Component is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS
| SRC/DATA to Detect/CollRes/Activate cards such as MFC, MFUL, MFP SL1 etc is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS
| SRC/DATA to Detect cards such as NFC Forum T1T, Topaz/Jewel is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS
| SRC/DATA to Detect cards such as MFDF, MFP, T4AT NFC Forum Tag or Type A EMVCo is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS
| SRC/DATA to Detect Peer Passive Type A P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type A P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type F212 P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type F424 P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS
| SRC/DATA to Detect FeliCa Cards is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS
| SRC/DATA to Detect Peer Passive Type F P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_I3P3B_TAGS
| SRC/DATA to Detect Type B Cards that operate at Layer3 level is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_I3P4B_TAGS
| SRC/DATA to Detect Type B Cards such as NFC Forum Type 4 Tags, EMVCo Type B Cards etc is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEV_TAGS
| SRC/DATA to Detect Type V Cards such as ICODE SLI/SLIX/SLI2/Tesa Cards is included.
#define | NXPBUILD__PHAC_DISCLOOP_I18000P3M3_TAGS
| SRC/DATA to Detect ICODE ILT Cards such as SMARTRAC StackIt Cards is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE
| SRC to Initialize Type A passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE
| SRC to Initialize Type A active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE
| SRC to Initialize Type F212 passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE
| SRC to Initialize Type F212 active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE
| SRC to Initialize Type F424 passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE
| SRC to Initialize Type F424 active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHNFCLIB
| Simplified API Interface, If enabling this the entry point should be this component in the application.
#define | NXPBUILD__PH_CIDMANAGER_SW
| CID Manager SW Component is included. More...
#define | NXPBUILD__PH_KEYSTORE_SW
| SW KeyStore Component is included. More...
#define | NXPBUILD__PH_CRYPTOSYM_SW
| Crypto Symbols SW Component is included. More...
#define | NXPBUILD__PH_CRYPTORNG_SW
| Crypto RNG SW Component is included. More...
#define | NXPBUILD__PHAL_FELICA_SW
| AL FeliCa SW Component is included.
#define | NXPBUILD__PHAL_MFC_SW
| AL Mifare Classic SW Component is included.
#define | NXPBUILD__PHAL_MFUL_SW
| AL Mifare Ultrlight SW Component is included.
#define | NXPBUILD__PHAL_MFDF_SW
| AL Mifare DesFire SW Component is included.
#define | NXPBUILD__PHAL_T1T_SW
| AL Type T1 Tag SW Component is included.
#define | NXPBUILD__PHAL_I15693_SW
| AL ISO 15693 SW Component is included.
#define | NXPBUILD__PHAL_SLI_SW
| AL SLI SW Component is included.
#define | NXPBUILD__PHAL_TOP_SW
| AL for TagOps Mapping SW Component is included.Required for NDEF operations.
#define | NXPBUILD__PHNP_SNEP_SW
| Protocol SNEP SW Component is included.
#define | NXPRDLIB_REM_GEN_INTFS
| < DEBUG build definition
#define | NXPBUILD__PH_PLATFORM
| Embedded Platform Porting and Abstraction Component included. More...
#define | NXPBUILD__PH_OSAL_FREERTOS
| OSAL Implementation of Free RTOS is included. More...
#define | NXPBUILD__PHHAL_HW_PN5180
| < If the used NFC HW is not NFC Controller like PN7462AU, then include one of the front end HAL More...
#define | NXPBUILD__PHHAL_HW_TARGET
| Dependency checking if target mode macros should be enabled.
#define | NXPBUILD__PHPAL_I14443P3A_SW
| PAL ISO 14443-3A SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P3B_SW
| PAL ISO 14443-3B SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4A_SW
| PAL ISO 14443-4A SW Component is included. More...
#define | NXPBUILD__PHPAL_I14443P4_SW
| PAL ISO 14443-4 SW Component is included. More...
#define | NXPBUILD__PHPAL_MIFARE_SW
| PAL MIFARE SW Component is included.
#define | NXPBUILD__PHPAL_FELICA_SW
| PAL Felica SW Component is included. More...
#define | NXPBUILD__PHPAL_SLI15693_SW
| PAL SLI 15693 Component is included. More...
#define | NXPBUILD__PHPAL_I18000P3M3_SW
| PAL ISO 18000p3m3 Component is included. More...
#define | NXPBUILD__PHPAL_I18092MPI_SW
| < If FE HAL is RC663, then include EPC UID PAL as required, otherwise exclude. More...
#define | NXPBUILD__PHPAL_I14443P4MC_SW
| PAL ISO 14443-4 Card Mode SW Component is included. More...
#define | NXPBUILD__PHPAL_I18092MT_SW
| PAL ISO 18092 Target Mode SW Component is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_SW
| Discovery Loop Activity SW Component is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_LPCD
| SRC to enable LPCD is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS
| SRC/DATA to Detect/CollRes/Activate cards such as MFC, MFUL, MFP SL1 etc is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS
| SRC/DATA to Detect cards such as NFC Forum T1T, Topaz/Jewel is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS
| SRC/DATA to Detect cards such as MFDF, MFP, T4AT NFC Forum Tag or Type A EMVCo is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS
| SRC/DATA to Detect Peer Passive Type A P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type A P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type F212 P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE
| SRC/DATA to Detect Peer Active Type F424 P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS
| SRC/DATA to Detect FeliCa Cards is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS
| SRC/DATA to Detect Peer Passive Type F P2P Target mode devices is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_I3P3B_TAGS
| SRC/DATA to Detect Type B Cards that operate at Layer3 level is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEB_I3P4B_TAGS
| SRC/DATA to Detect Type B Cards such as NFC Forum Type 4 Tags, EMVCo Type B Cards etc is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEV_TAGS
| SRC/DATA to Detect Type V Cards such as ICODE SLI/SLIX/SLI2/Tesa Cards is included.
#define | NXPBUILD__PHAC_DISCLOOP_I18000P3M3_TAGS
| SRC/DATA to Detect ICODE ILT Cards such as SMARTRAC StackIt Cards is included.
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE
| < If FE HAL is RC663, target mode is not supported at all, hence exclude those SRC, otherwise include as required More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE
| SRC to Initialize Type A active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE
| SRC to Initialize Type F212 passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE
| SRC to Initialize Type F212 active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE
| SRC to Initialize Type F424 passive listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE
| SRC to Initialize Type F424 active listen config and subsequently call HAL AutoColl is included. More...
#define | NXPBUILD__PHNFCLIB
| Simplified API Interface, If enabling this the entry point should be this component in the application. More...
#define | NXPBUILD__PHNFCLIB
| Simplified API Interface, If enabling this the entry point should be this component in the application. More...
#define | NXPBUILD__PH_KEYSTORE_SW
| SW KeyStore Component is included. More...
#define | NXPBUILD__PH_NDA_MFDF
| Mifare DESFire implementation under NDA.
#define | NXPBUILD__PH_CRYPTOSYM_SW
| Crypto Symbols SW Component is included. More...
#define | NXPBUILD__PH_CRYPTORNG_SW
| Crypto RNG SW Component is included. More...
#define | NXPBUILD__PHAL_FELICA_SW
| AL FeliCa SW Component is included.
#define | NXPBUILD__PHAL_MFC_SW
| AL Mifare Classic SW Component is included.
#define | NXPBUILD__PHAL_MFUL_SW
| AL Mifare Ultrlight SW Component is included.
#define | NXPBUILD__PHAL_MFDF_SW
| AL Mifare DesFire SW Component is included.
#define | NXPBUILD__PHAL_T1T_SW
| AL Type T1 Tag SW Component is included.
#define | NXPBUILD__PHAL_I15693_SW
| AL ISO 15693 SW Component is included.
#define | NXPBUILD__PHAL_SLI_SW
| AL SLI SW Component is included.
#define | NXPBUILD__PHAL_TOP_SW
| AL for TagOps Mapping SW Component is included.Required for NDEF operations.
#define | NXPBUILD__PHAL_I18000P3M3_SW
| AL ISO18000p3m3 SW Component is included.
#define | NXPBUILD__PHCE_T4T_SW
| AL HCE T2AT SW Component is included.
#define | NXPBUILD__PHLN_LLCP_SW
| < SRC to handle Extended NDEF Support as per T4T spec 3.0 is included More...
#define | NXPBUILD__PHNP_SNEP_SW
| Protocol SNEP SW Component is included.

## Detailed Description

Controls build behaviour of components.

Controls the Inclusion of required components, Inclusion SRC/DATA within components and the Build Dependencies between the components.

## Macro Definition Documentation

## § NXPBUILD__PHBAL_REG

#define NXPBUILD__PHBAL_REG

< DEBUG build definition

Generic BAL definition

## § NXPBUILD__PHPAL_FELICA

#define NXPBUILD__PHPAL_FELICA

< Enable handling of multiple Felica card response

Generic PAL Felica definition

## § NXPBUILD__PH_PLATFORM [1/5]

#define NXPBUILD__PH_PLATFORM

< DEBUG build definition

Embedded Platform Porting and Abstraction Component included. Used for LPC_XXX, Kinetis_XXX,Raspberry_XXX,iMX_XXX etc. If RdLib executing on embedded platform, then include one of the below embedded platform and one of the OS used as required.

## § NXPBUILD__PH_PLATFORM [2/5]

#define NXPBUILD__PH_PLATFORM

< DEBUG build definition

Embedded Platform Porting and Abstraction Component included. Used for LPC_XXX, Kinetis_XXX,Raspberry_XXX,iMX_XXX etc. If RdLib executing on embedded platform, then include one of the below embedded platform and one of the OS used as required.

## § NXPBUILD__PHHAL_HW_PN7462AU [1/6]

#define NXPBUILD__PHHAL_HW_PN7462AU

NFC Controller PN7462AU HAL.

NFC Controller PN7462AU HAL and Porting Component is included.

## § NXPBUILD__PHHAL_HW_PN7462AU [2/6]

#define NXPBUILD__PHHAL_HW_PN7462AU

NFC Controller PN7462AU HAL.

NFC Controller PN7462AU HAL and Porting Component is included.

## § NXPBUILD__PHHAL_HW_PN7462AU [3/6]

#define NXPBUILD__PHHAL_HW_PN7462AU

NFC Controller PN7462AU HAL.

NFC Controller PN7462AU HAL and Porting Component is included.

## § NXPBUILD__PH_LPC1769 [1/4]

#define NXPBUILD__PH_LPC1769

Host Controller LPC1769.

Host Controller LPC1769 Porting Component is included.RdLib is linked to LPC1769 Driver from LPCOpenStack.

## § NXPBUILD__PH_LPC1769 [2/4]

#define NXPBUILD__PH_LPC1769

Host Controller LPC1769.

Host Controller LPC1769 Porting Component is included.RdLib is linked to LPC1769 Driver from LPCOpenStack.

## § NXPBUILD__PH_LPC11U68 [1/4]

#define NXPBUILD__PH_LPC11U68

Host Controller LPC11U68.

Host Controller LPC11U68 Porting Component is included.

## § NXPBUILD__PH_LPC11U68 [2/4]

#define NXPBUILD__PH_LPC11U68

Host Controller LPC11U68.

Host Controller LPC11U68 Porting Component is included.

## § NXPBUILD__PH_RASPBERRY_PI [1/4]

#define NXPBUILD__PH_RASPBERRY_PI

Host Controller RaspBerry Pi.

Host Controller RaspBerry Pi Porting Component is included.

## § NXPBUILD__PH_RASPBERRY_PI [2/4]

#define NXPBUILD__PH_RASPBERRY_PI

Host Controller RaspBerry Pi.

Host Controller RaspBerry Pi Porting Component is included.

## § NXPBUILD__PH_OSAL_LINUX [1/4]

#define NXPBUILD__PH_OSAL_LINUX

OSAL Implementation of POSIX is included.

RdLib is executed as UM application in Linux

## § NXPBUILD__PH_OSAL_LINUX [2/4]

#define NXPBUILD__PH_OSAL_LINUX

OSAL Implementation of POSIX is included.

RdLib is executed as UM application in Linux

## § NXPBUILD__PH_OSAL_NULLOS [1/6]

#define NXPBUILD__PH_OSAL_NULLOS

OSAL Implementation of NULL OS is included.

RdLib executed in Executive Loop.

## § NXPBUILD__PH_OSAL_NULLOS [2/6]

#define NXPBUILD__PH_OSAL_NULLOS

OSAL Implementation of NULL OS is included.

RdLib executed in Executive Loop.

## § NXPBUILD__PH_OSAL_NULLOS [3/6]

#define NXPBUILD__PH_OSAL_NULLOS

OSAL Implementation of NULL OS is included.

RdLib executed in Executive Loop.

## § NXPBUILD__PH_OSAL_FREERTOS [1/5]

#define NXPBUILD__PH_OSAL_FREERTOS

OSAL Implementation of Free RTOS is included.

RdLib is linked to Free RTOS Library

## § NXPBUILD__PH_OSAL_FREERTOS [2/5]

#define NXPBUILD__PH_OSAL_FREERTOS

OSAL Implementation of Free RTOS is included.

RdLib is linked to Free RTOS Library

## § NXPBUILD__PHBAL_REG_LPCOPEN_SPI [1/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_SPI

LPCOpenStack SPI BAL Component is included.

## § NXPBUILD__PHBAL_REG_LPCOPEN_SPI [2/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_SPI

LPCOpenStack SPI BAL Component is included.

## § NXPBUILD__PHBAL_REG_LPCOPEN_I2C [1/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_I2C

LPCOpenStack SPI I2C Component is included.

## § NXPBUILD__PHBAL_REG_LPCOPEN_I2C [2/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_I2C

LPCOpenStack SPI I2C Component is included.

## § NXPBUILD__PHHAL_HW_RC523 [1/4]

#define NXPBUILD__PHHAL_HW_RC523

RC523 HAL Component is included.

## § NXPBUILD__PHHAL_HW_RC523 [2/4]

#define NXPBUILD__PHHAL_HW_RC523

RC523 HAL Component is included.

## § NXPBUILD__PHPAL_I14443P4MC_SW [1/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

< ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I14443P4MC_SW [2/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

< ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I14443P4MC_SW [3/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

< ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [1/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [2/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [3/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHPAL_SLI15693_SW [1/3]

#define NXPBUILD__PHPAL_SLI15693_SW

PAL SLI 15693 Component is included.

## § NXPBUILD__PHPAL_I18000P3M3_SW [1/5]

#define NXPBUILD__PHPAL_I18000P3M3_SW

PAL ISO 18000p3m3 Component is included.

## § NXPBUILD__PHPAL_I18000P3M3_SW [2/5]

#define NXPBUILD__PHPAL_I18000P3M3_SW

PAL ISO 18000p3m3 Component is included.

## § NXPBUILD__PHAC_DISCLOOP_LPCD [1/5]

#define NXPBUILD__PHAC_DISCLOOP_LPCD

SRC to enable LPCD is included.

## § NXPBUILD__PHAC_DISCLOOP_LPCD [2/5]

#define NXPBUILD__PHAC_DISCLOOP_LPCD

SRC to enable LPCD is included.

## § NXPBUILD__PHPAL_I18092MPI_SW [1/5]

#define NXPBUILD__PHPAL_I18092MPI_SW

PAL ISO18092 (P2P) SW Component is included.

## § NXPBUILD__PHPAL_I18092MPI_SW [2/5]

#define NXPBUILD__PHPAL_I18092MPI_SW

PAL ISO18092 (P2P) SW Component is included.

## § NXPBUILD__PHPAL_I14443P3A_SW [1/3]

#define NXPBUILD__PHPAL_I14443P3A_SW

PAL ISO 14443-3A SW Component is included.

## § NXPBUILD__PHPAL_I14443P3B_SW [1/3]

#define NXPBUILD__PHPAL_I14443P3B_SW

PAL ISO 14443-3B SW Component is included.

## § NXPBUILD__PHPAL_I14443P4A_SW [1/3]

#define NXPBUILD__PHPAL_I14443P4A_SW

PAL ISO 14443-4A SW Component is included.

## § NXPBUILD__PHPAL_I14443P4_SW [1/3]

#define NXPBUILD__PHPAL_I14443P4_SW

PAL ISO 14443-4 SW Component is included.

## § NXPBUILD__PHPAL_FELICA_SW [1/3]

#define NXPBUILD__PHPAL_FELICA_SW

PAL Felica SW Component is included.

If FE HAL is RC523, then exclude ISO15693 & ISO18000p3m3 PAL, otherwise include as required.

## § NXPBUILD__PHPAL_EPCUID_SW [1/2]

#define NXPBUILD__PHPAL_EPCUID_SW

< If FE HAL is RC663, then include EPC UID PAL as required, otherwise exclude.

PAL EPC UID SW Component is included.

## § NXPBUILD__PHAC_DISCLOOP_SW [1/3]

#define NXPBUILD__PHAC_DISCLOOP_SW

Discovery Loop Activity SW Component is included.

If DiscLoop SW Component is included, macros( & it's dependencies) to include/exclude SRC/DATA within Discloop is defined.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS

SRC/DATA to Detect/CollRes/Activate cards such as MFC, MFUL, MFP SL1 etc is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS

SRC/DATA to Detect cards such as NFC Forum T1T, Topaz/Jewel is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS

SRC/DATA to Detect cards such as MFDF, MFP, T4AT NFC Forum Tag or Type A EMVCo is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS

SRC/DATA to Detect Peer Passive Type A P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type A P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type F212 P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type F424 P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS [1/3]

#define NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS

SRC/DATA to Detect FeliCa Cards is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS

SRC/DATA to Detect Peer Passive Type F P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE

SRC to Initialize Type A passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE

SRC to Initialize Type A active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE

SRC to Initialize Type F212 passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE

SRC to Initialize Type F212 active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE

SRC to Initialize Type F424 passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE [1/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE

SRC to Initialize Type F424 active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PH_CIDMANAGER_SW [1/2]

#define NXPBUILD__PH_CIDMANAGER_SW

CID Manager SW Component is included.

## § NXPBUILD__PH_KEYSTORE_SW [1/3]

#define NXPBUILD__PH_KEYSTORE_SW

SW KeyStore Component is included.

## § NXPBUILD__PH_CRYPTOSYM_SW [1/3]

#define NXPBUILD__PH_CRYPTOSYM_SW

Crypto Symbols SW Component is included.

## § NXPBUILD__PH_CRYPTORNG_SW [1/3]

#define NXPBUILD__PH_CRYPTORNG_SW

Crypto RNG SW Component is included.

## § NXPBUILD__PH_PLATFORM [3/5]

#define NXPBUILD__PH_PLATFORM

< DEBUG build definition

Embedded Platform Porting and Abstraction Component included. Used for LPC_XXX, Kinetis_XXX,Raspberry_XXX,iMX_XXX etc. If RdLib executing on embedded platform, then include one of the below embedded platform and one of the OS used as required.

## § NXPBUILD__PH_PLATFORM [4/5]

#define NXPBUILD__PH_PLATFORM

< DEBUG build definition

Embedded Platform Porting and Abstraction Component included. Used for LPC_XXX, Kinetis_XXX,Raspberry_XXX,iMX_XXX etc. If RdLib executing on embedded platform, then include one of the below embedded platform and one of the OS used as required.

## § NXPBUILD__PHHAL_HW_PN7462AU [4/6]

#define NXPBUILD__PHHAL_HW_PN7462AU

NFC Controller PN7462AU HAL.

NFC Controller PN7462AU HAL and Porting Component is included.

## § NXPBUILD__PHHAL_HW_PN7462AU [5/6]

#define NXPBUILD__PHHAL_HW_PN7462AU

NFC Controller PN7462AU HAL.

NFC Controller PN7462AU HAL and Porting Component is included.

## § NXPBUILD__PHHAL_HW_PN7462AU [6/6]

#define NXPBUILD__PHHAL_HW_PN7462AU

NFC Controller PN7462AU HAL.

NFC Controller PN7462AU HAL and Porting Component is included.

## § NXPBUILD__PH_LPC1769 [3/4]

#define NXPBUILD__PH_LPC1769

Host Controller LPC1769.

Host Controller LPC1769 Porting Component is included.RdLib is linked to LPC1769 Driver from LPCOpenStack.

## § NXPBUILD__PH_LPC1769 [4/4]

#define NXPBUILD__PH_LPC1769

Host Controller LPC1769.

Host Controller LPC1769 Porting Component is included.RdLib is linked to LPC1769 Driver from LPCOpenStack.

## § NXPBUILD__PH_LPC11U68 [3/4]

#define NXPBUILD__PH_LPC11U68

Host Controller LPC11U68.

Host Controller LPC11U68 Porting Component is included.

## § NXPBUILD__PH_LPC11U68 [4/4]

#define NXPBUILD__PH_LPC11U68

Host Controller LPC11U68.

Host Controller LPC11U68 Porting Component is included.

## § NXPBUILD__PH_RASPBERRY_PI [3/4]

#define NXPBUILD__PH_RASPBERRY_PI

Host Controller RaspBerry Pi.

Host Controller RaspBerry Pi Porting Component is included.

## § NXPBUILD__PH_RASPBERRY_PI [4/4]

#define NXPBUILD__PH_RASPBERRY_PI

Host Controller RaspBerry Pi.

Host Controller RaspBerry Pi Porting Component is included.

## § NXPBUILD__PH_OSAL_LINUX [3/4]

#define NXPBUILD__PH_OSAL_LINUX

OSAL Implementation of POSIX is included.

RdLib is executed as UM application in Linux

## § NXPBUILD__PH_OSAL_LINUX [4/4]

#define NXPBUILD__PH_OSAL_LINUX

OSAL Implementation of POSIX is included.

RdLib is executed as UM application in Linux

## § NXPBUILD__PH_OSAL_NULLOS [4/6]

#define NXPBUILD__PH_OSAL_NULLOS

OSAL Implementation of NULL OS is included.

RdLib executed in Executive Loop.

## § NXPBUILD__PH_OSAL_NULLOS [5/6]

#define NXPBUILD__PH_OSAL_NULLOS

OSAL Implementation of NULL OS is included.

RdLib executed in Executive Loop.

## § NXPBUILD__PH_OSAL_NULLOS [6/6]

#define NXPBUILD__PH_OSAL_NULLOS

OSAL Implementation of NULL OS is included.

RdLib executed in Executive Loop.

## § NXPBUILD__PH_OSAL_FREERTOS [3/5]

#define NXPBUILD__PH_OSAL_FREERTOS

OSAL Implementation of Free RTOS is included.

RdLib is linked to Free RTOS Library

## § NXPBUILD__PH_OSAL_FREERTOS [4/5]

#define NXPBUILD__PH_OSAL_FREERTOS

OSAL Implementation of Free RTOS is included.

RdLib is linked to Free RTOS Library

## § NXPBUILD__PHBAL_REG_LPCOPEN_SPI [3/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_SPI

LPCOpenStack SPI BAL Component is included.

## § NXPBUILD__PHBAL_REG_LPCOPEN_SPI [4/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_SPI

LPCOpenStack SPI BAL Component is included.

## § NXPBUILD__PHBAL_REG_LPCOPEN_I2C [3/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_I2C

LPCOpenStack SPI I2C Component is included.

## § NXPBUILD__PHBAL_REG_LPCOPEN_I2C [4/4]

#define NXPBUILD__PHBAL_REG_LPCOPEN_I2C

LPCOpenStack SPI I2C Component is included.

## § NXPBUILD__PHHAL_HW_RC523 [3/4]

#define NXPBUILD__PHHAL_HW_RC523

RC523 HAL Component is included.

## § NXPBUILD__PHHAL_HW_RC523 [4/4]

#define NXPBUILD__PHHAL_HW_RC523

RC523 HAL Component is included.

## § NXPBUILD__PHPAL_I14443P4MC_SW [4/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

< ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I14443P4MC_SW [5/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

< ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I14443P4MC_SW [6/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

< ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [4/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [5/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [6/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHPAL_SLI15693_SW [2/3]

#define NXPBUILD__PHPAL_SLI15693_SW

PAL SLI 15693 Component is included.

## § NXPBUILD__PHPAL_I18000P3M3_SW [3/5]

#define NXPBUILD__PHPAL_I18000P3M3_SW

PAL ISO 18000p3m3 Component is included.

## § NXPBUILD__PHPAL_I18000P3M3_SW [4/5]

#define NXPBUILD__PHPAL_I18000P3M3_SW

PAL ISO 18000p3m3 Component is included.

## § NXPBUILD__PHAC_DISCLOOP_LPCD [3/5]

#define NXPBUILD__PHAC_DISCLOOP_LPCD

SRC to enable LPCD is included.

## § NXPBUILD__PHAC_DISCLOOP_LPCD [4/5]

#define NXPBUILD__PHAC_DISCLOOP_LPCD

SRC to enable LPCD is included.

## § NXPBUILD__PHPAL_I18092MPI_SW [3/5]

#define NXPBUILD__PHPAL_I18092MPI_SW

PAL ISO18092 (P2P) SW Component is included.

## § NXPBUILD__PHPAL_I18092MPI_SW [4/5]

#define NXPBUILD__PHPAL_I18092MPI_SW

PAL ISO18092 (P2P) SW Component is included.

## § NXPBUILD__PHPAL_I14443P3A_SW [2/3]

#define NXPBUILD__PHPAL_I14443P3A_SW

PAL ISO 14443-3A SW Component is included.

## § NXPBUILD__PHPAL_I14443P3B_SW [2/3]

#define NXPBUILD__PHPAL_I14443P3B_SW

PAL ISO 14443-3B SW Component is included.

## § NXPBUILD__PHPAL_I14443P4A_SW [2/3]

#define NXPBUILD__PHPAL_I14443P4A_SW

PAL ISO 14443-4A SW Component is included.

## § NXPBUILD__PHPAL_I14443P4_SW [2/3]

#define NXPBUILD__PHPAL_I14443P4_SW

PAL ISO 14443-4 SW Component is included.

## § NXPBUILD__PHPAL_FELICA_SW [2/3]

#define NXPBUILD__PHPAL_FELICA_SW

PAL Felica SW Component is included.

If FE HAL is RC523, then exclude ISO15693 & ISO18000p3m3 PAL, otherwise include as required.

## § NXPBUILD__PHPAL_EPCUID_SW [2/2]

#define NXPBUILD__PHPAL_EPCUID_SW

< If FE HAL is RC663, then include EPC UID PAL as required, otherwise exclude.

PAL EPC UID SW Component is included.

## § NXPBUILD__PHAC_DISCLOOP_SW [2/3]

#define NXPBUILD__PHAC_DISCLOOP_SW

Discovery Loop Activity SW Component is included.

If DiscLoop SW Component is included, macros( & it's dependencies) to include/exclude SRC/DATA within Discloop is defined.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS

SRC/DATA to Detect/CollRes/Activate cards such as MFC, MFUL, MFP SL1 etc is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS

SRC/DATA to Detect cards such as NFC Forum T1T, Topaz/Jewel is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS

SRC/DATA to Detect cards such as MFDF, MFP, T4AT NFC Forum Tag or Type A EMVCo is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS

SRC/DATA to Detect Peer Passive Type A P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type A P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type F212 P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type F424 P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS [2/3]

#define NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS

SRC/DATA to Detect FeliCa Cards is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS

SRC/DATA to Detect Peer Passive Type F P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE

SRC to Initialize Type A passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE

SRC to Initialize Type A active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE

SRC to Initialize Type F212 passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE

SRC to Initialize Type F212 active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE

SRC to Initialize Type F424 passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE [2/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE

SRC to Initialize Type F424 active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PH_CIDMANAGER_SW [2/2]

#define NXPBUILD__PH_CIDMANAGER_SW

CID Manager SW Component is included.

## § NXPBUILD__PH_KEYSTORE_SW [2/3]

#define NXPBUILD__PH_KEYSTORE_SW

SW KeyStore Component is included.

## § NXPBUILD__PH_CRYPTOSYM_SW [2/3]

#define NXPBUILD__PH_CRYPTOSYM_SW

Crypto Symbols SW Component is included.

## § NXPBUILD__PH_CRYPTORNG_SW [2/3]

#define NXPBUILD__PH_CRYPTORNG_SW

Crypto RNG SW Component is included.

## § NXPBUILD__PH_PLATFORM [5/5]

#define NXPBUILD__PH_PLATFORM

Embedded Platform Porting and Abstraction Component included.

Used for LPC_XXX, Kinetis_XXX,Raspberry_XXX,iMX_XXX etc. If RdLib executing on embedded platform, then include one of the below embedded platform and one of the OS used as required.

## § NXPBUILD__PH_OSAL_FREERTOS [5/5]

#define NXPBUILD__PH_OSAL_FREERTOS

OSAL Implementation of Free RTOS is included.

RdLib is linked to Free RTOS Library

## § NXPBUILD__PHHAL_HW_PN5180

#define NXPBUILD__PHHAL_HW_PN5180

< If the used NFC HW is not NFC Controller like PN7462AU, then include one of the front end HAL

PN5180 HAL Component is included

## § NXPBUILD__PHPAL_I14443P3A_SW [3/3]

#define NXPBUILD__PHPAL_I14443P3A_SW

PAL ISO 14443-3A SW Component is included.

## § NXPBUILD__PHPAL_I14443P3B_SW [3/3]

#define NXPBUILD__PHPAL_I14443P3B_SW

PAL ISO 14443-3B SW Component is included.

## § NXPBUILD__PHPAL_I14443P4A_SW [3/3]

#define NXPBUILD__PHPAL_I14443P4A_SW

PAL ISO 14443-4A SW Component is included.

## § NXPBUILD__PHPAL_I14443P4_SW [3/3]

#define NXPBUILD__PHPAL_I14443P4_SW

PAL ISO 14443-4 SW Component is included.

## § NXPBUILD__PHPAL_FELICA_SW [3/3]

#define NXPBUILD__PHPAL_FELICA_SW

PAL Felica SW Component is included.

If FE HAL is RC523, then exclude ISO15693 & ISO18000p3m3 PAL, otherwise include as required.

## § NXPBUILD__PHPAL_SLI15693_SW [3/3]

#define NXPBUILD__PHPAL_SLI15693_SW

PAL SLI 15693 Component is included.

## § NXPBUILD__PHPAL_I18000P3M3_SW [5/5]

#define NXPBUILD__PHPAL_I18000P3M3_SW

PAL ISO 18000p3m3 Component is included.

## § NXPBUILD__PHPAL_I18092MPI_SW [5/5]

#define NXPBUILD__PHPAL_I18092MPI_SW

< If FE HAL is RC663, then include EPC UID PAL as required, otherwise exclude.

PAL ISO18092 (P2P) SW Component is included. If FE HAL is RC663, then exclude ISO14443 Card Mode PAL & ISO18092 Target Mode PAL, otherwise include as required. ISO14443 Card Mode PAL & ISO18092 Target Mode PAL will execute only in an embedded platform and not in PC platform.

## § NXPBUILD__PHPAL_I14443P4MC_SW [7/7]

#define NXPBUILD__PHPAL_I14443P4MC_SW

PAL ISO 14443-4 Card Mode SW Component is included.

## § NXPBUILD__PHPAL_I18092MT_SW [7/7]

#define NXPBUILD__PHPAL_I18092MT_SW

PAL ISO 18092 Target Mode SW Component is included.

## § NXPBUILD__PHAC_DISCLOOP_SW [3/3]

#define NXPBUILD__PHAC_DISCLOOP_SW

Discovery Loop Activity SW Component is included.

If DiscLoop SW Component is included, macros( & it's dependencies) to include/exclude SRC/DATA within Discloop is defined.

## § NXPBUILD__PHAC_DISCLOOP_LPCD [5/5]

#define NXPBUILD__PHAC_DISCLOOP_LPCD

SRC to enable LPCD is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P3_TAGS

SRC/DATA to Detect/CollRes/Activate cards such as MFC, MFUL, MFP SL1 etc is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_JEWEL_TAGS

SRC/DATA to Detect cards such as NFC Forum T1T, Topaz/Jewel is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_I3P4_TAGS

SRC/DATA to Detect cards such as MFDF, MFP, T4AT NFC Forum Tag or Type A EMVCo is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_TAGS

SRC/DATA to Detect Peer Passive Type A P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type A P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type F212 P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_P2P_ACTIVE

SRC/DATA to Detect Peer Active Type F424 P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS [3/3]

#define NXPBUILD__PHAC_DISCLOOP_FELICA_TAGS

SRC/DATA to Detect FeliCa Cards is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF_P2P_TAGS

SRC/DATA to Detect Peer Passive Type F P2P Target mode devices is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_PASSIVE

< If FE HAL is RC663, target mode is not supported at all, hence exclude those SRC, otherwise include as required

SRC to Initialize Type A passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEA_TARGET_ACTIVE

SRC to Initialize Type A active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_PASSIVE

SRC to Initialize Type F212 passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF212_TARGET_ACTIVE

SRC to Initialize Type F212 active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_PASSIVE

SRC to Initialize Type F424 passive listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE [3/3]

#define NXPBUILD__PHAC_DISCLOOP_TYPEF424_TARGET_ACTIVE

SRC to Initialize Type F424 active listen config and subsequently call HAL AutoColl is included.

## § NXPBUILD__PHNFCLIB [1/2]

#define NXPBUILD__PHNFCLIB

Simplified API Interface, If enabling this the entry point should be this component in the application.

Simplified layer Component.

## § NXPBUILD__PHNFCLIB [2/2]

#define NXPBUILD__PHNFCLIB

Simplified API Interface, If enabling this the entry point should be this component in the application.

Simplified layer Component.

## § NXPBUILD__PH_KEYSTORE_SW [3/3]

#define NXPBUILD__PH_KEYSTORE_SW

SW KeyStore Component is included.

## § NXPBUILD__PH_CRYPTOSYM_SW [3/3]

#define NXPBUILD__PH_CRYPTOSYM_SW

Crypto Symbols SW Component is included.

## § NXPBUILD__PH_CRYPTORNG_SW [3/3]

#define NXPBUILD__PH_CRYPTORNG_SW

Crypto RNG SW Component is included.

## § NXPBUILD__PHLN_LLCP_SW

#define NXPBUILD__PHLN_LLCP_SW

< SRC to handle Extended NDEF Support as per T4T spec 3.0 is included

Link LLCP SW Component is included