NXP NFC Reader Library v4.040.05.011646

Modules
Protocol Abstraction Layer

Contains Hardware-Independent implementations of various contactless protocols. More...

Collaboration diagram for Protocol Abstraction Layer:

## Modules
| ISO/IEC 14443-3A
| These Components implement the ISO/IEC 14443-3 Type-A contactless protocol.
| ISO/IEC 14443-3B
| These Components implement the ISO/IEC 14443-3 Type-B contactless protocol.
| ISO/IEC 14443-4A
| These Components configure PHPAL_I14443P4A.
| ISO/IEC 14443-4
| These Components implement the ISO/IEC 14443-4:2008(E) contactless protocol.
| MIFARE(R)
| These Components implement the MIFARE(R) Classic, MIFARE(R) Ultralight, MIFARE(R) DESFire and MIFARE(R) Plus products.
| ISO/IEC 14443-4mC
| This component implements the PICC side of ISO/IEC 14443-4 Protocol.
| Felica
| These Components implement the Felica (contactless) protocol.
| ISO/IEC 15693 / ISO/IEC 18000-3M1
| These component implements the protocol layer (activation) commands of ISO/IEC 15693 (ISO/IEC 18000-3M1) vicinity protocol.
| ISO/IEC 18000-3 Mode3
| These Components implement the ISO/IEC 18000-3 Mode3 support.
| ISO/IEC 18092 Mode Initiator
| These Components implement the ISO/IEC ISO18092 contact-less protocol.
| ISO/IEC 18092 Mode Target
| This Component implements the ISO/IEC ISO18092 Target mode contact-less protocol.

## Detailed Description

Contains Hardware-Independent implementations of various contactless protocols.