NXP NFC Reader Library v4.040.05.011646

Data Fields
phalTop_T3T Struct Reference
Application Layer » Tag Operation Layer » Component : Software

T3T parameter structure. More...

## Data Fields
void * | pAlT3TDataParams
| Pointer to Felica data parameters.
uint8_t | bRwa
| Tag read/write access; 1 - Read/Write, 0 - Read Only.
uint8_t | bNbr
| Number of Blocks that can be read at one time.
uint8_t | bNbw
| Number of Blocks that can be written at one time.
uint16_t | bNmaxb
| Maximum number of 'Blocks * 16' available for NDEF data.
uint8_t | bUid [16]
| UID to address T3T.
uint8_t | bAttributeBlock [16]
| Contains the attribute block of the Ndef Type 3 tag.

## Detailed Description

T3T parameter structure.

The documentation for this struct was generated from the following file:

- phalTop.h