/*!
@page middleware_log Middleware Change Log

@section lwip lwIP for MCUXpresso SDK.
  The current version of lwIP is based on lwIP 2.0.3.

  - 2.0.3_rev1
    - New features:
      - Ported lwIP 2.0.3 (2017-09-15, SHA-1: 92f23d6ca0971a32f2085b9480e738d34174417b) to KSDK 2.0.0.

  - 2.0.2_rev1
    - New features:
      - Ported lwIP 2.0.2 (2017-03-13, SHA-1: c0862d60746e2d1ceae69af4c6f24e469570ecef) to KSDK 2.0.0.
	  
  - 2.0.0_rev3
    - New features:
      - Ported lwIP 2.0.0 (2016-11-10, SHA-1: 216bf89491815029aa15463a18744afa04df58fe) to KSDK 2.0.0.
	  
  - 2.0.0_rev2
    - New features:
      - Ported lwIP 2.0.0 RC2 (2016-08-08, SHA-1: b1dfd00f9233d124514a36a8c8606990016f2ad4) to KSDK 2.0.0.
	  
  - 2.0.0_rev1
    - New features:
      - Ported lwIP 2.0.0 RC0 (2016-05-26) to KSDK 2.0.0. 
	  - Changed lwIP bare-metal examples to use poll-driven approach instead of interrupt-driven one.
	  
  - 1.4.1_rev2
    - New features:
      - Enabled critical sections in lwIP.
    - Bug fixes:
      - Fixed default lwIP packet-buffer size to be able to accept a maximum size frame from the ENET driver.
      - Fixed possible drop of multi-frame packets during transmission.
 
  - 1.4.1_rev1
    - New features:
      - Ported lwIP 1.4.1 to KSDK 2.0.0.
*/


