
steps:

1. download the Uart2ndBootloader project to lpc54608xpresso board.
2. use Tera Team UART terminal tool which support y-modem to load the bin generated by test project.
3. see to application note's description for more.
