EVK-MIMXRT1060 EIQ MNIST DATASET

This is an example project for the EVK-MIMXRT1060 with the RK043FN02H-CT LCD Display.
The project expects the EVK to have an SD card inserted and the SD card to contain
the following folder structure:

/0/
/1/
/2/
...
/9/

where each digit class has a separate folder from 0 to 9 and they are all in
the root folder of the SD card.

The project is supported in the MCUXpresso IDE.

The example collects handwritten digits for the purpose of gathering a dataset.
The GUI consists of 4 input areas, each for one digit, and buttons to clear
the screen and submit the input. Lastly, it also contains a text area, which
informs the user, which digit they should write and submit next. The collected
submissions are stored on the SD card in appropriate folders.

The GUI was created in Embedded Wizard Studio. An RT1060 project was exported from
EWS and merged into an SDK project.
