# Static Call Graph for image debug\hello_world.out

#<CALLGRAPH># ARM Linker, 6190004: Last Updated: Fri Jul 28 11:34:23 2023

### Maximum Stack Usage = 4952 bytes + Unknown(Functions without stacksize, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

task_pq_mat_inv ⇒ arm_mat_inverse_f32 ⇒ PQ_MatrixInversion ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

### Functions with no stack information

- Reset_Handler
- ACMP_DriverIRQHandler
- ADC0_DriverIRQHandler
- ADC1_DriverIRQHandler
- BusFault_Handler
- CAN0_IRQ0_DriverIRQHandler
- CAN0_IRQ1_DriverIRQHandler
- CDOG_DriverIRQHandler
- CTIMER0_DriverIRQHandler
- CTIMER1_DriverIRQHandler
- CTIMER2_DriverIRQHandler
- CTIMER3_DriverIRQHandler
- CTIMER4_DriverIRQHandler
- DAC0_DriverIRQHandler
- DAC1_DriverIRQHandler
- DAC2_DriverIRQHandler
- DMIC_DriverIRQHandler
- DebugMon_Handler
- DefaultISR
- ELS_DriverIRQHandler
- ELS_ERR_DriverIRQHandler
- ELS_IRQ1_DriverIRQHandler
- ENC0_COMPARE_DriverIRQHandler
- ENC0_HOME_DriverIRQHandler
- ENC0_IDX_DriverIRQHandler
- ENC0_WDG_DriverIRQHandler
- ENC1_COMPARE_DriverIRQHandler
- ENC1_HOME_DriverIRQHandler
- ENC1_IDX_DriverIRQHandler
- ENC1_WDG_DriverIRQHandler
- EZH_ARCH_B0_DriverIRQHandler
- FLASH_DriverIRQHandler
- FLEXPWM0_CAPTURE_DriverIRQHandler
- FLEXPWM0_COMPARE0_DriverIRQHandler
- FLEXPWM0_COMPARE1_DriverIRQHandler
- FLEXPWM0_COMPARE2_DriverIRQHandler
- FLEXPWM0_COMPARE3_DriverIRQHandler
- FLEXPWM0_FAULT_DriverIRQHandler
- FLEXPWM0_RELOAD0_DriverIRQHandler
- FLEXPWM0_RELOAD1_DriverIRQHandler
- FLEXPWM0_RELOAD2_DriverIRQHandler
- FLEXPWM0_RELOAD3_DriverIRQHandler
- FLEXPWM0_RELOAD_ERROR_DriverIRQHandler
- FLEXPWM1_CAPTURE_DriverIRQHandler
- FLEXPWM1_COMPARE0_DriverIRQHandler
- FLEXPWM1_COMPARE1_DriverIRQHandler
- FLEXPWM1_COMPARE2_DriverIRQHandler
- FLEXPWM1_COMPARE3_DriverIRQHandler
- FLEXPWM1_FAULT_DriverIRQHandler
- FLEXPWM1_RELOAD0_DriverIRQHandler
- FLEXPWM1_RELOAD1_DriverIRQHandler
- FLEXPWM1_RELOAD2_DriverIRQHandler
- FLEXPWM1_RELOAD3_DriverIRQHandler
- FLEXPWM1_RELOAD_ERROR_DriverIRQHandler
- FlexSPI0_DriverIRQHandler
- Freqme_DriverIRQHandler
- GINT0_DriverIRQHandler
- GINT1_DriverIRQHandler
- HSCMP0_DriverIRQHandler
- HSCMP1_DriverIRQHandler
- HSCMP2_DriverIRQHandler
- HWVAD0_DriverIRQHandler
- I3C0_DriverIRQHandler
- ITRC0_DriverIRQHandler
- MRT0_DriverIRQHandler
- MemManage_Handler
- OS_EVENT_DriverIRQHandler
- PKC_DriverIRQHandler
- PKC_ERR_DriverIRQHandler
- POWERQUAD_DriverIRQHandler
- PUF_DriverIRQHandler
- RAM_PARITY_ECC_ERR_DriverIRQHandler
- RTC_DriverIRQHandler
- Reserved127_DriverIRQHandler
- Reserved130_DriverIRQHandler
- Reserved131_DriverIRQHandler
- Reserved132_DriverIRQHandler
- Reserved133_DriverIRQHandler
- Reserved56_DriverIRQHandler
- Reserved57_DriverIRQHandler
- Reserved58_DriverIRQHandler
- Reserved62_DriverIRQHandler
- Reserved63_DriverIRQHandler
- Reserved64_DriverIRQHandler
- Reserved77_DriverIRQHandler
- Reserved79_DriverIRQHandler
- Reserved80_DriverIRQHandler
- Reserved83_DriverIRQHandler
- Reserved84_DriverIRQHandler
- Reserved85_DriverIRQHandler
- Reserved86_DriverIRQHandler
- Reserved87_DriverIRQHandler
- Reserved88_DriverIRQHandler
- Reserved89_DriverIRQHandler
- SCT0_DriverIRQHandler
- SEC_HYPERVISOR_CALL_DriverIRQHandler
- SEC_VIO_DriverIRQHandler
- SPI_FILTER_DriverIRQHandler
- SecureFault_Handler
- Tamper_DriverIRQHandler
- USB0_DriverIRQHandler
- USB0_NEEDCLK_DriverIRQHandler
- UTICK0_DriverIRQHandler
- UsageFault_Handler
- WAKEUP_DriverIRQHandler
- WDT_BOD_DriverIRQHandler
- NMI_Handler
- HardFault_Handler
- SVC_Handler
- PendSV_Handler
- SysTick_Handler
- WDT_BOD_IRQHandler
- DMA0_IRQHandler
- GINT0_IRQHandler
- GINT1_IRQHandler
- PIN_INT0_IRQHandler
- PIN_INT1_IRQHandler
- PIN_INT2_IRQHandler
- PIN_INT3_IRQHandler
- UTICK0_IRQHandler
- MRT0_IRQHandler
- CTIMER0_IRQHandler
- CTIMER1_IRQHandler
- SCT0_IRQHandler
- CTIMER3_IRQHandler
- FLEXCOMM0_IRQHandler
- FLEXCOMM1_IRQHandler
- FLEXCOMM2_IRQHandler
- FLEXCOMM3_IRQHandler
- FLEXCOMM4_IRQHandler
- FLEXCOMM5_IRQHandler
- FLEXCOMM6_IRQHandler
- FLEXCOMM7_IRQHandler
- ADC0_IRQHandler
- ADC1_IRQHandler
- ACMP_IRQHandler
- DMIC_IRQHandler
- HWVAD0_IRQHandler
- USB0_NEEDCLK_IRQHandler
- USB0_IRQHandler
- RTC_IRQHandler
- EZH_ARCH_B0_IRQHandler
- WAKEUP_IRQHandler
- PIN_INT4_IRQHandler
- PIN_INT5_IRQHandler
- PIN_INT6_IRQHandler
- PIN_INT7_IRQHandler
- CTIMER2_IRQHandler
- CTIMER4_IRQHandler
- OS_EVENT_IRQHandler
- FlexSPI0_IRQHandler
- Reserved56_IRQHandler
- Reserved57_IRQHandler
- Reserved58_IRQHandler
- CAN0_IRQ0_IRQHandler
- CAN0_IRQ1_IRQHandler
- SPI_FILTER_IRQHandler
- Reserved62_IRQHandler
- Reserved63_IRQHandler
- Reserved64_IRQHandler
- SEC_HYPERVISOR_CALL_IRQHandler
- SEC_GPIO_INT0_IRQ0_IRQHandler
- SEC_GPIO_INT0_IRQ1_IRQHandler
- Freqme_IRQHandler
- SEC_VIO_IRQHandler
- ELS_IRQHandler
- PKC_IRQHandler
- PUF_IRQHandler
- POWERQUAD_IRQHandler
- DMA1_IRQHandler
- FLEXCOMM8_IRQHandler
- CDOG_IRQHandler
- Reserved77_IRQHandler
- I3C0_IRQHandler
- Reserved79_IRQHandler
- Reserved80_IRQHandler
- ELS_IRQ1_IRQHandler
- Tamper_IRQHandler
- Reserved83_IRQHandler
- Reserved84_IRQHandler
- Reserved85_IRQHandler
- Reserved86_IRQHandler
- Reserved87_IRQHandler
- Reserved88_IRQHandler
- Reserved89_IRQHandler
- DAC0_IRQHandler
- DAC1_IRQHandler
- DAC2_IRQHandler
- HSCMP0_IRQHandler
- HSCMP1_IRQHandler
- HSCMP2_IRQHandler
- FLEXPWM0_CAPTURE_IRQHandler
- FLEXPWM0_FAULT_IRQHandler
- FLEXPWM0_RELOAD_ERROR_IRQHandler
- FLEXPWM0_COMPARE0_IRQHandler
- FLEXPWM0_RELOAD0_IRQHandler
- FLEXPWM0_COMPARE1_IRQHandler
- FLEXPWM0_RELOAD1_IRQHandler
- FLEXPWM0_COMPARE2_IRQHandler
- FLEXPWM0_RELOAD2_IRQHandler
- FLEXPWM0_COMPARE3_IRQHandler
- FLEXPWM0_RELOAD3_IRQHandler
- FLEXPWM1_CAPTURE_IRQHandler
- FLEXPWM1_FAULT_IRQHandler
- FLEXPWM1_RELOAD_ERROR_IRQHandler
- FLEXPWM1_COMPARE0_IRQHandler
- FLEXPWM1_RELOAD0_IRQHandler
- FLEXPWM1_COMPARE1_IRQHandler
- FLEXPWM1_RELOAD1_IRQHandler
- FLEXPWM1_COMPARE2_IRQHandler
- FLEXPWM1_RELOAD2_IRQHandler
- FLEXPWM1_COMPARE3_IRQHandler
- FLEXPWM1_RELOAD3_IRQHandler
- ENC0_COMPARE_IRQHandler
- ENC0_HOME_IRQHandler
- ENC0_WDG_IRQHandler
- ENC0_IDX_IRQHandler
- ENC1_COMPARE_IRQHandler
- ENC1_HOME_IRQHandler
- ENC1_WDG_IRQHandler
- ENC1_IDX_IRQHandler
- ITRC0_IRQHandler
- Reserved127_IRQHandler
- ELS_ERR_IRQHandler
- PKC_ERR_IRQHandler
- Reserved130_IRQHandler
- Reserved131_IRQHandler
- Reserved132_IRQHandler
- Reserved133_IRQHandler
- FLASH_IRQHandler
- RAM_PARITY_ECC_ERR_IRQHandler

### Function Pointers

- ACMP_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ACMP_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ADC0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ADC0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ADC1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ADC1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- BusFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CAN0_IRQ0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CAN0_IRQ0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CAN0_IRQ1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CAN0_IRQ1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CDOG_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CDOG_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER4_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER4_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DAC0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DAC0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DAC1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DAC1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DAC2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DAC2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DMA0_DriverIRQHandler from fsl_dma.o(.text.DMA0_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- DMA0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DMA1_DriverIRQHandler from fsl_dma.o(.text.DMA1_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- DMA1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DMIC_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DMIC_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DebugMon_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ELS_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ELS_ERR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ELS_ERR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ELS_IRQ1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ELS_IRQ1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ELS_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_COMPARE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_COMPARE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_HOME_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_HOME_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_IDX_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_IDX_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_WDG_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_WDG_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_COMPARE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_COMPARE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_HOME_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_HOME_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_IDX_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_IDX_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_WDG_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_WDG_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- EZH_ARCH_B0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- EZH_ARCH_B0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLASH_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLASH_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM0_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM0_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM1_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM1_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM2_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM2_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM3_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM3_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM4_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM4_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM4_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM5_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM5_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM5_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM6_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM6_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM6_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM7_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM7_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM7_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM8_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM8_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM8_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_CAPTURE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_CAPTURE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_FAULT_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_FAULT_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD_ERROR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD_ERROR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_CAPTURE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_CAPTURE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_FAULT_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_FAULT_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD_ERROR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD_ERROR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FlexSPI0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FlexSPI0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Freqme_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Freqme_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- GINT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- GINT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- GINT1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- GINT1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HAL_UartReceiveBlocking from fsl_adapter_usart.o(.text.HAL_UartReceiveBlocking) referenced 2 times from fsl_debug_console.o(.text.DbgConsole_Init)
- HAL_UartSendBlocking from fsl_adapter_usart.o(.text.HAL_UartSendBlocking) referenced 2 times from fsl_debug_console.o(.text.DbgConsole_Init)
- HSCMP0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HSCMP0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HSCMP1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HSCMP1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HSCMP2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HSCMP2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HWVAD0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HWVAD0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HardFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HardFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- I3C0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- I3C0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ITRC0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ITRC0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- LCD_WrCmd from lcd.o(.text.LCD_WrCmd) referenced 2 times from lcd.o(.text.LCD_Init)
- LCD_WrData from lcd.o(.text.LCD_WrData) referenced 2 times from lcd.o(.text.LCD_Init)
- MRT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- MRT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- MemManage_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- NMI_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- NMI_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- OS_EVENT_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- OS_EVENT_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT0_DriverIRQHandler from fsl_pint.o(.text.PIN_INT0_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT1_DriverIRQHandler from fsl_pint.o(.text.PIN_INT1_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT2_DriverIRQHandler from fsl_pint.o(.text.PIN_INT2_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT3_DriverIRQHandler from fsl_pint.o(.text.PIN_INT3_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT4_DriverIRQHandler from fsl_pint.o(.text.PIN_INT4_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT4_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT5_DriverIRQHandler from fsl_pint.o(.text.PIN_INT5_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT5_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT6_DriverIRQHandler from fsl_pint.o(.text.PIN_INT6_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT6_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT7_DriverIRQHandler from fsl_pint.o(.text.PIN_INT7_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- PIN_INT7_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PKC_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PKC_ERR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PKC_ERR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PKC_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- POWERQUAD_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- POWERQUAD_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PUF_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PUF_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PendSV_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PendSV_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- RAM_PARITY_ECC_ERR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- RAM_PARITY_ECC_ERR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- RTC_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- RTC_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved127_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved127_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved130_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved130_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved131_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved131_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved132_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved132_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved133_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved133_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved56_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved56_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved57_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved57_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved58_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved58_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved62_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved62_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved63_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved63_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved64_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved64_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved77_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved77_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved79_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved79_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved80_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved80_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved83_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved83_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved84_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved84_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved85_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved85_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved86_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved86_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved87_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved87_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved88_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved88_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved89_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved89_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reset_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SCT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SCT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_GPIO_INT0_IRQ0_DriverIRQHandler from fsl_pint.o(.text.SEC_GPIO_INT0_IRQ0_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- SEC_GPIO_INT0_IRQ0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_GPIO_INT0_IRQ1_DriverIRQHandler from fsl_pint.o(.text.SEC_GPIO_INT0_IRQ1_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- SEC_GPIO_INT0_IRQ1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_HYPERVISOR_CALL_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SEC_HYPERVISOR_CALL_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_VIO_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SEC_VIO_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SPI_FILTER_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SPI_FILTER_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SVC_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SVC_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SecureFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SysTick_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SysTick_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SystemInit from system_lpc55s36.o(.text.SystemInit) referenced from startup_lpc55s36.o(.text)
- Tamper_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Tamper_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- USB0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- USB0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- USB0_NEEDCLK_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- USB0_NEEDCLK_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- UTICK0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- UTICK0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- UsageFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- WAKEUP_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- WAKEUP_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- WDT_BOD_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- WDT_BOD_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc55s36.o(.text)
- _sputc from printf6.o(i._sputc) referenced from printf6.o(i.__0sprintf$6)
- main from main.o(.text.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
- task_pq_fft_128 from task_pq_fft_128.o(.text.task_pq_fft_128) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_fft_256 from task_pq_fft_256.o(.text.task_pq_fft_256) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_fft_512 from task_pq_fft_512.o(.text.task_pq_fft_512) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_fir_highpass from task_pq_fir.o(.text.task_pq_fir_highpass) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_fir_lowpass from task_pq_fir.o(.text.task_pq_fir_lowpass) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_mat_add from task_pq_mat_add.o(.text.task_pq_mat_add) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_mat_inv from task_pq_mat_inv.o(.text.task_pq_mat_inv) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_mat_mul from task_pq_mat_mul.o(.text.task_pq_mat_mul) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- task_pq_records from task_pq_recods.o(.text.task_pq_records) referenced 2 times from main.o(.data.cAppLcdDisplayPageFunc)
- user_button_callback from task_user_key.o(.text.user_button_callback) referenced 2 times from task_user_key.o(.text.APP_InitUserKey)

### Global Symbols

__main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

_main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry4.o(.ARM.Collect$$$$00000003))

_main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Calls]

- >> __scatterload

__main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Called By]

- >> __scatterload

_main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

_main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

_main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

__rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

__rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

Reset_Handler (Thumb, 40 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ACMP_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ADC0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ADC1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

BusFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CAN0_IRQ0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CAN0_IRQ1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CDOG_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER4_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DAC0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DAC1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DAC2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DMIC_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DebugMon_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DefaultISR (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Called By]

- >> ACMP_DriverIRQHandler

ELS_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ELS_ERR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ELS_IRQ1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_COMPARE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_HOME_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_IDX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_WDG_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_COMPARE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_HOME_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_IDX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_WDG_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

EZH_ARCH_B0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLASH_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_CAPTURE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_FAULT_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD_ERROR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_CAPTURE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_FAULT_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD_ERROR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FlexSPI0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Freqme_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

GINT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

GINT1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HSCMP0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HSCMP1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HSCMP2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HWVAD0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

I3C0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ITRC0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

MRT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

MemManage_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

OS_EVENT_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PKC_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PKC_ERR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

POWERQUAD_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PUF_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

RAM_PARITY_ECC_ERR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

RTC_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved127_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved130_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved131_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved132_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved133_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved56_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved57_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved58_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved62_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved63_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved64_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved77_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved79_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved80_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved83_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved84_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved85_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved86_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved87_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved88_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved89_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SCT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_HYPERVISOR_CALL_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_VIO_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SPI_FILTER_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SecureFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Tamper_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

USB0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

USB0_NEEDCLK_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

UTICK0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

UsageFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

WAKEUP_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

WDT_BOD_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

NMI_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

HardFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

SVC_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

PendSV_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

SysTick_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

WDT_BOD_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DMA0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

GINT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

GINT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

UTICK0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

MRT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SCT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ADC0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ADC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ACMP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DMIC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HWVAD0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

USB0_NEEDCLK_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

USB0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

RTC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

EZH_ARCH_B0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

WAKEUP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

OS_EVENT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FlexSPI0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved56_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved57_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved58_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CAN0_IRQ0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CAN0_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SPI_FILTER_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved62_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved63_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved64_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_HYPERVISOR_CALL_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_GPIO_INT0_IRQ0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_GPIO_INT0_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Freqme_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_VIO_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ELS_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PKC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PUF_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

POWERQUAD_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DMA1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM8_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CDOG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved77_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

I3C0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved79_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved80_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ELS_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Tamper_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved83_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved84_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved85_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved86_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved87_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved88_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved89_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DAC0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DAC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DAC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HSCMP0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HSCMP1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HSCMP2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_CAPTURE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_CAPTURE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_COMPARE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_HOME_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_WDG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_IDX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_COMPARE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_HOME_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_WDG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_IDX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ITRC0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved127_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ELS_ERR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PKC_ERR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved130_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved131_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved132_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved133_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLASH_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

RAM_PARITY_ECC_ERR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

__aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
[Stack]

- Max Depth = 40
- Call Chain = __aeabi_uldivmod

[Calls]

- >> __aeabi_llsr
- >> __aeabi_llsl

[Called By]

- >> SDK_DelayAtLeastUs

___aeabi_memcpy4$ret (Thumb, 0 bytes, Stack size 8 bytes, memcpy.o(.text), UNUSED)

___aeabi_memcpy8$ret (Thumb, 0 bytes, Stack size 8 bytes, memcpy.o(.text), UNUSED)

__aeabi_memcpy (Thumb, 40 bytes, Stack size 8 bytes, memcpy.o(.text), UNUSED)

memcpy (Thumb, 0 bytes, Stack size 8 bytes, memcpy.o(.text))
[Stack]

- Max Depth = 8
- Call Chain = memcpy

[Called By]

- >> DbgConsole_Vprintf

__aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
[Called By]

- >> memset
- >> __aeabi_memclr

__aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

__aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

__aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
[Calls]

- >> __aeabi_memset

__aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
[Called By]

- >> task_pq_mat_mul
- >> task_pq_mat_inv

__aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

memset (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text))
[Stack]

- Max Depth = 8
- Call Chain = memset

[Calls]

- >> __aeabi_memset

[Called By]

- >> USART_GetDefaultConfig
- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128
- >> main
- >> SPI_MasterGetDefaultConfig

strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
[Called By]

- >> DbgConsole_Vprintf

__aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
[Stack]

- Max Depth = 88
- Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round

[Calls]

- >> __aeabi_lasr
- >> __aeabi_llsl
- >> _double_round
- >> _double_epilogue

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> __aeabi_drsub
- >> __aeabi_dsub

__aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
[Calls]

- >> __aeabi_dadd

__aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
[Calls]

- >> __aeabi_dadd

__aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
[Stack]

- Max Depth = 88
- Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round

[Calls]

- >> _double_epilogue

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

__aeabi_d2iz (Thumb, 62 bytes, Stack size 16 bytes, dfixi.o(.text))
[Stack]

- Max Depth = 16
- Call Chain = __aeabi_d2iz

[Calls]

- >> __aeabi_llsr

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

__aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

__aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
[Stack]

- Max Depth = 8
- Call Chain = __aeabi_d2f

[Calls]

- >> _float_round

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass

__aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

__aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
[Called By]

- >> _printf_core

__aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
[Called By]

- >> __aeabi_dadd
- >> __aeabi_uldivmod
- >> _double_epilogue

_ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

__aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
[Called By]

- >> __aeabi_d2iz
- >> __aeabi_uldivmod
- >> _double_epilogue

_ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

__aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
[Called By]

- >> __aeabi_dadd

_ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

__I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

_float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
[Called By]

- >> __aeabi_d2f

_float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text), UNUSED)

_double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
[Stack]

- Max Depth = 8
- Call Chain = _double_round

[Called By]

- >> __aeabi_dadd
- >> _double_epilogue

_double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
[Stack]

- Max Depth = 40
- Call Chain = _double_epilogue ⇒ _double_round

[Calls]

- >> __aeabi_llsr
- >> __aeabi_llsl
- >> _double_round

[Called By]

- >> __aeabi_dadd
- >> __aeabi_dmul

__scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
[Calls]

- >> __main_after_scatterload

[Called By]

- >> _main_scatterload

__scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

__decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

__decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

APP_InitUserKey (Thumb, 78 bytes, Stack size 8 bytes, task_user_key.o(.text.APP_InitUserKey))
[Stack]

- Max Depth = 168
- Call Chain = APP_InitUserKey ⇒ PINT_Init ⇒ RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> PINT_EnableCallbackByIndex
- >> PINT_PinInterruptConfig
- >> PINT_Init
- >> INPUTMUX_Deinit
- >> INPUTMUX_AttachSignal
- >> INPUTMUX_Init

[Called By]

- >> main

BOARD_BootClockPLL150M (Thumb, 244 bytes, Stack size 56 bytes, clock_config.o(.text.BOARD_BootClockPLL150M))
[Stack]

- Max Depth = 224
- Call Chain = BOARD_BootClockPLL150M ⇒ CLOCK_SetPLL0Freq ⇒ SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> CLOCK_SetPLL0Freq
- >> CLOCK_SetupExtClocking
- >> CLOCK_SetClkDiv
- >> CLOCK_SetFLASHAccessCyclesForFreq
- >> POWER_SetVoltageForFreq
- >> CLOCK_SetupFROClocking
- >> POWER_PowerInit
- >> CLOCK_AttachClk

[Called By]

- >> BOARD_InitHardware

BOARD_InitDebugConsole (Thumb, 44 bytes, Stack size 8 bytes, board.o(.text.BOARD_InitDebugConsole))
[Stack]

- Max Depth = 288
- Call Chain = BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> DbgConsole_Init
- >> RESET_ClearPeripheralReset
- >> CLOCK_AttachClk

[Called By]

- >> BOARD_InitHardware

BOARD_InitHardware (Thumb, 26 bytes, Stack size 8 bytes, hardware_init.o(.text.BOARD_InitHardware))
[Stack]

- Max Depth = 296
- Call Chain = BOARD_InitHardware ⇒ BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> BOARD_InitDebugConsole
- >> BOARD_InitPins
- >> CLOCK_AttachClk
- >> BOARD_BootClockPLL150M

[Called By]

- >> main

BOARD_InitPins (Thumb, 38 bytes, Stack size 0 bytes, pin_mux.o(.text.BOARD_InitPins))
[Called By]

- >> BOARD_InitHardware

CLOCK_AttachClk (Thumb, 116 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_AttachClk))
[Stack]

- Max Depth = 8
- Call Chain = CLOCK_AttachClk

[Called By]

- >> LCD_Init
- >> BOARD_InitDebugConsole
- >> BOARD_BootClockPLL150M
- >> BOARD_InitHardware

CLOCK_GetCoreSysClkFreq (Thumb, 216 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetCoreSysClkFreq))
[Called By]

- >> CLOCK_GetHsLspiClkFreq

CLOCK_GetHsLspiClkFreq (Thumb, 178 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetHsLspiClkFreq))
[Calls]

- >> CLOCK_GetCoreSysClkFreq

[Called By]

- >> LCD_Init

CLOCK_SetClkDiv (Thumb, 58 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_SetClkDiv))
[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetFLASHAccessCyclesForFreq (Thumb, 140 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_SetFLASHAccessCyclesForFreq))
[Stack]

- Max Depth = 8
- Call Chain = CLOCK_SetFLASHAccessCyclesForFreq

[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetPLL0Freq (Thumb, 350 bytes, Stack size 24 bytes, fsl_clock.o(.text.CLOCK_SetPLL0Freq))
[Stack]

- Max Depth = 168
- Call Chain = CLOCK_SetPLL0Freq ⇒ SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> SDK_DelayAtLeastUs

[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetupExtClocking (Thumb, 64 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_SetupExtClocking))
[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetupFROClocking (Thumb, 134 bytes, Stack size 12 bytes, fsl_clock.o(.text.CLOCK_SetupFROClocking))
[Stack]

- Max Depth = 12
- Call Chain = CLOCK_SetupFROClocking

[Called By]

- >> BOARD_BootClockPLL150M

DMA0_DriverIRQHandler (Thumb, 12 bytes, Stack size 0 bytes, fsl_dma.o(.text.DMA0_DriverIRQHandler))
[Stack]

- Max Depth = 168
- Call Chain = DMA0_DriverIRQHandler ⇒ DMA_IRQHandle ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> DMA_IRQHandle

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DMA1_DriverIRQHandler (Thumb, 12 bytes, Stack size 0 bytes, fsl_dma.o(.text.DMA1_DriverIRQHandler))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DMA_IRQHandle (Thumb, 290 bytes, Stack size 32 bytes, fsl_dma.o(.text.DMA_IRQHandle))
[Stack]

- Max Depth = 168
- Call Chain = DMA_IRQHandle ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> DMA0_DriverIRQHandler

DbgConsole_Init (Thumb, 82 bytes, Stack size 40 bytes, fsl_debug_console.o(.text.DbgConsole_Init))
[Stack]

- Max Depth = 280
- Call Chain = DbgConsole_Init ⇒ HAL_UartInit ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> HAL_UartInit

[Called By]

- >> BOARD_InitDebugConsole

DbgConsole_Printf (Thumb, 32 bytes, Stack size 24 bytes, fsl_debug_console.o(.text.DbgConsole_Printf))
[Stack]

- Max Depth = 136
- Call Chain = DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> DbgConsole_Vprintf

[Called By]

- >> user_button_callback
- >> task_pq_mat_mul
- >> task_pq_mat_inv
- >> task_pq_mat_add
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128
- >> main
- >> LCD_WrChar
- >> __aeabi_assert

DbgConsole_Vprintf (Thumb, 1030 bytes, Stack size 104 bytes, fsl_debug_console.o(.text.DbgConsole_Vprintf))
[Stack]

- Max Depth = 112
- Call Chain = DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> strlen
- >> memcpy

[Called By]

- >> DbgConsole_Printf

FLEXCOMM0_DriverIRQHandler (Thumb, 54 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM0_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM0_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM1_DriverIRQHandler (Thumb, 54 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM1_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM1_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM2_DriverIRQHandler (Thumb, 54 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM2_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM2_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM3_DriverIRQHandler (Thumb, 54 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM3_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM3_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM4_DriverIRQHandler (Thumb, 54 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM4_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM4_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM5_DriverIRQHandler (Thumb, 54 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM5_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM5_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM6_DriverIRQHandler (Thumb, 56 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM6_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM6_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM7_DriverIRQHandler (Thumb, 56 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM7_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM7_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM8_DriverIRQHandler (Thumb, 56 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM8_DriverIRQHandler))
[Stack]

- Max Depth = 136
- Call Chain = FLEXCOMM8_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM_Init (Thumb, 236 bytes, Stack size 16 bytes, fsl_flexcomm.o(.text.FLEXCOMM_Init))
[Stack]

- Max Depth = 160
- Call Chain = FLEXCOMM_Init ⇒ RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> RESET_PeripheralReset
- >> __aeabi_assert

[Called By]

- >> USART_Init
- >> SPI_MasterInit

FLEXSPI_NorFlash_GetConfig (Thumb, 14 bytes, Stack size 0 bytes, fsl_flash.o(.text.FLEXSPI_NorFlash_GetConfig))
[Called By]

- >> main

FLEXSPI_NorFlash_Init (Thumb, 14 bytes, Stack size 0 bytes, fsl_flash.o(.text.FLEXSPI_NorFlash_Init))
[Called By]

- >> main

GPIO_PinInit (Thumb, 218 bytes, Stack size 16 bytes, fsl_gpio.o(.text.GPIO_PinInit))
[Stack]

- Max Depth = 152
- Call Chain = GPIO_PinInit ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> LCD_Init

GPIO_PortInit (Thumb, 148 bytes, Stack size 0 bytes, fsl_gpio.o(.text.GPIO_PortInit))
[Stack]

- Max Depth = 144
- Call Chain = GPIO_PortInit ⇒ RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> RESET_PeripheralReset
- >> __aeabi_assert

[Called By]

- >> LCD_Init

HAL_UartInit (Thumb, 220 bytes, Stack size 48 bytes, fsl_adapter_usart.o(.text.HAL_UartInit))
[Stack]

- Max Depth = 240
- Call Chain = HAL_UartInit ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> USART_GetDefaultConfig
- >> USART_Init
- >> __aeabi_assert

[Called By]

- >> DbgConsole_Init

HAL_UartReceiveBlocking (Thumb, 108 bytes, Stack size 8 bytes, fsl_adapter_usart.o(.text.HAL_UartReceiveBlocking))
[Stack]

- Max Depth = 160
- Call Chain = HAL_UartReceiveBlocking ⇒ USART_ReadBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> USART_ReadBlocking
- >> __aeabi_assert

[Address Reference Count : 1]

- fsl_debug_console.o(.text.DbgConsole_Init)

HAL_UartSendBlocking (Thumb, 102 bytes, Stack size 8 bytes, fsl_adapter_usart.o(.text.HAL_UartSendBlocking))
[Stack]

- Max Depth = 144
- Call Chain = HAL_UartSendBlocking ⇒ USART_WriteBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> USART_WriteBlocking
- >> __aeabi_assert

[Address Reference Count : 1]

- fsl_debug_console.o(.text.DbgConsole_Init)

INPUTMUX_AttachSignal (Thumb, 14 bytes, Stack size 0 bytes, fsl_inputmux.o(.text.INPUTMUX_AttachSignal))
[Called By]

- >> APP_InitUserKey

INPUTMUX_Deinit (Thumb, 16 bytes, Stack size 0 bytes, fsl_inputmux.o(.text.INPUTMUX_Deinit))
[Called By]

- >> APP_InitUserKey

INPUTMUX_Init (Thumb, 16 bytes, Stack size 0 bytes, fsl_inputmux.o(.text.INPUTMUX_Init))
[Called By]

- >> APP_InitUserKey

LCD_ClearScreen (Thumb, 94 bytes, Stack size 56 bytes, lcd.o(.text.LCD_ClearScreen))
[Stack]

- Max Depth = 304
- Call Chain = LCD_ClearScreen ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_SetCursor
- >> SPI_MasterTransferBlocking

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128
- >> main

LCD_DisplayImage (Thumb, 120 bytes, Stack size 56 bytes, lcd.o(.text.LCD_DisplayImage))
[Stack]

- Max Depth = 312
- Call Chain = LCD_DisplayImage ⇒ LCD_SetAreaAddr ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_SetAreaAddr
- >> SPI_MasterTransferBlocking

[Called By]

- >> task_pq_records
- >> task_pq_mat_mul
- >> task_pq_mat_inv
- >> task_pq_mat_add

LCD_DrawPoint (Thumb, 128 bytes, Stack size 32 bytes, lcd.o(.text.LCD_DrawPoint))
[Stack]

- Max Depth = 280
- Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_SetCursor
- >> __aeabi_assert
- >> SPI_MasterTransferBlocking

[Called By]

- >> LCD_PrintFreqSpec
- >> LCD_PrintWaveformFir
- >> LCD_PrintWaveform

LCD_Hx8347Init (Thumb, 568 bytes, Stack size 16 bytes, lcd_hx8347d.o(.text.LCD_Hx8347Init))
[Stack]

- Max Depth = 160
- Call Chain = LCD_Hx8347Init ⇒ SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> SDK_DelayAtLeastUs

[Called By]

- >> LCD_Init

LCD_Init (Thumb, 262 bytes, Stack size 80 bytes, lcd.o(.text.LCD_Init))
[Stack]

- Max Depth = 264
- Call Chain = LCD_Init ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_Hx8347Init
- >> SPI_MasterInit
- >> CLOCK_GetHsLspiClkFreq
- >> SPI_MasterGetDefaultConfig
- >> SPI8_InitPins
- >> SPI_MasterTransferBlocking
- >> GPIO_PinInit
- >> GPIO_PortInit
- >> CLOCK_AttachClk

[Called By]

- >> main

LCD_PrintFreqSpec (Thumb, 78 bytes, Stack size 32 bytes, task_lcd_display.o(.text.LCD_PrintFreqSpec))
[Stack]

- Max Depth = 312
- Call Chain = LCD_PrintFreqSpec ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_DrawPoint

[Called By]

- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

LCD_PrintFreqSpecText (Thumb, 74 bytes, Stack size 32 bytes, task_lcd_display.o(.text.LCD_PrintFreqSpecText))
[Stack]

- Max Depth = 344
- Call Chain = LCD_PrintFreqSpecText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_WrChar

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

LCD_PrintText (Thumb, 88 bytes, Stack size 40 bytes, task_lcd_display.o(.text.LCD_PrintText))
[Stack]

- Max Depth = 352
- Call Chain = LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_WrChar

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_mat_mul
- >> task_pq_mat_inv
- >> task_pq_mat_add
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

LCD_PrintWaveform (Thumb, 70 bytes, Stack size 24 bytes, task_lcd_display.o(.text.LCD_PrintWaveform))
[Stack]

- Max Depth = 304
- Call Chain = LCD_PrintWaveform ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_DrawPoint

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

LCD_PrintWaveformFir (Thumb, 78 bytes, Stack size 32 bytes, task_lcd_display.o(.text.LCD_PrintWaveformFir))
[Stack]

- Max Depth = 312
- Call Chain = LCD_PrintWaveformFir ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_DrawPoint

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass

LCD_PrintWaveformText (Thumb, 74 bytes, Stack size 32 bytes, task_lcd_display.o(.text.LCD_PrintWaveformText))
[Stack]

- Max Depth = 344
- Call Chain = LCD_PrintWaveformText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_WrChar

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

LCD_SetAreaAddr (Thumb, 820 bytes, Stack size 72 bytes, lcd.o(.text.LCD_SetAreaAddr))
[Stack]

- Max Depth = 256
- Call Chain = LCD_SetAreaAddr ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> SPI_MasterTransferBlocking

[Called By]

- >> LCD_DisplayImage

LCD_SetCursor (Thumb, 456 bytes, Stack size 64 bytes, lcd.o(.text.LCD_SetCursor))
[Stack]

- Max Depth = 248
- Call Chain = LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> SPI_MasterTransferBlocking

[Called By]

- >> main
- >> LCD_WrString
- >> LCD_WrChar
- >> LCD_DrawPoint
- >> LCD_ClearScreen

LCD_WrChar (Thumb, 344 bytes, Stack size 64 bytes, lcd.o(.text.LCD_WrChar))
[Stack]

- Max Depth = 312
- Call Chain = LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> DbgConsole_Printf
- >> LCD_SetCursor
- >> __aeabi_assert
- >> SPI_MasterTransferBlocking

[Called By]

- >> LCD_PrintFreqSpecText
- >> LCD_PrintWaveformText
- >> LCD_PrintText
- >> LCD_WrString

LCD_WrCmd (Thumb, 66 bytes, Stack size 32 bytes, lcd.o(.text.LCD_WrCmd))
[Stack]

- Max Depth = 216
- Call Chain = LCD_WrCmd ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> SPI_MasterTransferBlocking

[Address Reference Count : 1]

- lcd.o(.text.LCD_Init)

LCD_WrData (Thumb, 66 bytes, Stack size 32 bytes, lcd.o(.text.LCD_WrData))
[Stack]

- Max Depth = 216
- Call Chain = LCD_WrData ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> SPI_MasterTransferBlocking

[Address Reference Count : 1]

- lcd.o(.text.LCD_Init)

LCD_WrPixelValue (Thumb, 68 bytes, Stack size 32 bytes, lcd.o(.text.LCD_WrPixelValue))
[Stack]

- Max Depth = 216
- Call Chain = LCD_WrPixelValue ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> SPI_MasterTransferBlocking

[Called By]

- >> main

LCD_WrString (Thumb, 292 bytes, Stack size 80 bytes, lcd.o(.text.LCD_WrString))
[Stack]

- Max Depth = 392
- Call Chain = LCD_WrString ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_WrChar
- >> LCD_SetCursor
- >> __aeabi_assert
- >> SPI_MasterTransferBlocking

[Called By]

- >> task_pq_records

PINT_EnableCallbackByIndex (Thumb, 120 bytes, Stack size 8 bytes, fsl_pint.o(.text.PINT_EnableCallbackByIndex))
[Stack]

- Max Depth = 144
- Call Chain = PINT_EnableCallbackByIndex ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> APP_InitUserKey

PINT_Init (Thumb, 156 bytes, Stack size 16 bytes, fsl_pint.o(.text.PINT_Init))
[Stack]

- Max Depth = 160
- Call Chain = PINT_Init ⇒ RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> RESET_PeripheralReset
- >> __aeabi_assert

[Called By]

- >> APP_InitUserKey

PINT_PinInterruptConfig (Thumb, 116 bytes, Stack size 8 bytes, fsl_pint.o(.text.PINT_PinInterruptConfig))
[Stack]

- Max Depth = 144
- Call Chain = PINT_PinInterruptConfig ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> APP_InitUserKey

PIN_INT0_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT0_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT0_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT1_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT1_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT1_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT2_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT2_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT2_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT3_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT3_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT3_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT4_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT4_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT4_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT5_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT5_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT5_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT6_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT6_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT6_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT7_DriverIRQHandler (Thumb, 72 bytes, Stack size 8 bytes, fsl_pint.o(.text.PIN_INT7_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PIN_INT7_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

POWER_PowerInit (Thumb, 96 bytes, Stack size 0 bytes, fsl_power.o(.text.POWER_PowerInit))
[Called By]

- >> BOARD_BootClockPLL150M

POWER_SetVoltageForFreq (Thumb, 244 bytes, Stack size 24 bytes, fsl_power.o(.text.POWER_SetVoltageForFreq))
[Stack]

- Max Depth = 24
- Call Chain = POWER_SetVoltageForFreq

[Calls]

- >> POWER_SetVoltageForProcess

[Called By]

- >> BOARD_BootClockPLL150M

PQ_FIR (Thumb, 104 bytes, Stack size 8 bytes, fsl_powerquad_filter.o(.text.PQ_FIR))
[Stack]

- Max Depth = 144
- Call Chain = PQ_FIR ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass

PQ_Init (Thumb, 36 bytes, Stack size 8 bytes, fsl_powerquad_basic.o(.text.PQ_Init))
[Stack]

- Max Depth = 152
- Call Chain = PQ_Init ⇒ RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> RESET_PeripheralReset

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> main

PQ_MatrixAddition (Thumb, 100 bytes, Stack size 0 bytes, fsl_powerquad_matrix.o(.text.PQ_MatrixAddition))
[Stack]

- Max Depth = 136
- Call Chain = PQ_MatrixAddition ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> arm_mat_add_f32

PQ_MatrixInversion (Thumb, 104 bytes, Stack size 8 bytes, fsl_powerquad_matrix.o(.text.PQ_MatrixInversion))
[Stack]

- Max Depth = 144
- Call Chain = PQ_MatrixInversion ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> arm_mat_inverse_f32

PQ_MatrixMultiplication (Thumb, 100 bytes, Stack size 0 bytes, fsl_powerquad_matrix.o(.text.PQ_MatrixMultiplication))
[Stack]

- Max Depth = 136
- Call Chain = PQ_MatrixMultiplication ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> arm_mat_mult_f32

PQ_MatrixScale (Thumb, 68 bytes, Stack size 0 bytes, fsl_powerquad_matrix.o(.text.PQ_MatrixScale))
[Stack]

- Max Depth = 136
- Call Chain = PQ_MatrixScale ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass

PQ_SetConfig (Thumb, 92 bytes, Stack size 8 bytes, fsl_powerquad_basic.o(.text.PQ_SetConfig))
[Stack]

- Max Depth = 144
- Call Chain = PQ_SetConfig ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass

PQ_TransformCFFT (Thumb, 64 bytes, Stack size 0 bytes, fsl_powerquad_transform.o(.text.PQ_TransformCFFT))
[Stack]

- Max Depth = 136
- Call Chain = PQ_TransformCFFT ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> arm_cfft_q31

PQ_TransformIFFT (Thumb, 64 bytes, Stack size 0 bytes, fsl_powerquad_transform.o(.text.PQ_TransformIFFT))
[Stack]

- Max Depth = 136
- Call Chain = PQ_TransformIFFT ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> arm_cfft_q31

RESET_ClearPeripheralReset (Thumb, 66 bytes, Stack size 0 bytes, fsl_reset.o(.text.RESET_ClearPeripheralReset))
[Stack]

- Max Depth = 136
- Call Chain = RESET_ClearPeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> BOARD_InitDebugConsole

RESET_PeripheralReset (Thumb, 82 bytes, Stack size 8 bytes, fsl_reset.o(.text.RESET_PeripheralReset))
[Stack]

- Max Depth = 144
- Call Chain = RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> FLEXCOMM_Init
- >> PINT_Init
- >> PQ_Init
- >> GPIO_PortInit

SDK_DelayAtLeastUs (Thumb, 64 bytes, Stack size 8 bytes, fsl_common_arm.o(.text.SDK_DelayAtLeastUs))
[Stack]

- Max Depth = 144
- Call Chain = SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> __aeabi_uldivmod

[Called By]

- >> CLOCK_SetPLL0Freq
- >> LCD_Hx8347Init

SEC_GPIO_INT0_IRQ0_DriverIRQHandler (Thumb, 68 bytes, Stack size 8 bytes, fsl_pint.o(.text.SEC_GPIO_INT0_IRQ0_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = SEC_GPIO_INT0_IRQ0_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_GPIO_INT0_IRQ1_DriverIRQHandler (Thumb, 68 bytes, Stack size 8 bytes, fsl_pint.o(.text.SEC_GPIO_INT0_IRQ1_DriverIRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = SEC_GPIO_INT0_IRQ1_DriverIRQHandler

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SPI8_InitPins (Thumb, 50 bytes, Stack size 0 bytes, pin_mux.o(.text.SPI8_InitPins))
[Called By]

- >> LCD_Init

SPI_MasterGetDefaultConfig (Thumb, 68 bytes, Stack size 16 bytes, fsl_spi.o(.text.SPI_MasterGetDefaultConfig))
[Stack]

- Max Depth = 152
- Call Chain = SPI_MasterGetDefaultConfig ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> memset

[Called By]

- >> LCD_Init

SPI_MasterInit (Thumb, 444 bytes, Stack size 16 bytes, fsl_spi.o(.text.SPI_MasterInit))
[Stack]

- Max Depth = 176
- Call Chain = SPI_MasterInit ⇒ FLEXCOMM_Init ⇒ RESET_PeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> FLEXCOMM_Init
- >> __aeabi_assert

[Called By]

- >> LCD_Init

SPI_MasterTransferBlocking (Thumb, 512 bytes, Stack size 48 bytes, fsl_spi.o(.text.SPI_MasterTransferBlocking))
[Stack]

- Max Depth = 184
- Call Chain = SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> LCD_DisplayImage
- >> LCD_WrString
- >> LCD_WrChar
- >> LCD_DrawPoint
- >> LCD_WrPixelValue
- >> LCD_ClearScreen
- >> LCD_SetAreaAddr
- >> LCD_SetCursor
- >> LCD_Init
- >> LCD_WrData
- >> LCD_WrCmd

SystemInit (Thumb, 114 bytes, Stack size 0 bytes, system_lpc55s36.o(.text.SystemInit))
[Calls]

- >> SystemInitHook

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SystemInitHook (Thumb, 2 bytes, Stack size 0 bytes, system_lpc55s36.o(.text.SystemInitHook))
[Called By]

- >> SystemInit

USART_GetDefaultConfig (Thumb, 68 bytes, Stack size 16 bytes, fsl_usart.o(.text.USART_GetDefaultConfig))
[Stack]

- Max Depth = 152
- Call Chain = USART_GetDefaultConfig ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> memset

[Called By]

- >> HAL_UartInit

USART_Init (Thumb, 372 bytes, Stack size 16 bytes, fsl_usart.o(.text.USART_Init))
[Stack]

- Max Depth = 192
- Call Chain = USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> USART_SetBaudRate
- >> FLEXCOMM_Init
- >> __aeabi_assert

[Called By]

- >> HAL_UartInit

USART_ReadBlocking (Thumb, 166 bytes, Stack size 16 bytes, fsl_usart.o(.text.USART_ReadBlocking))
[Stack]

- Max Depth = 152
- Call Chain = USART_ReadBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartReceiveBlocking

USART_SetBaudRate (Thumb, 242 bytes, Stack size 40 bytes, fsl_usart.o(.text.USART_SetBaudRate))
[Stack]

- Max Depth = 176
- Call Chain = USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> USART_Init

USART_WriteBlocking (Thumb, 74 bytes, Stack size 0 bytes, fsl_usart.o(.text.USART_WriteBlocking))
[Stack]

- Max Depth = 136
- Call Chain = USART_WriteBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartSendBlocking

__aeabi_assert (Thumb, 16 bytes, Stack size 0 bytes, fsl_assert.o(.text.__aeabi_assert))
[Stack]

- Max Depth = 136
- Call Chain = __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> DbgConsole_Printf

[Called By]

- >> FLEXCOMM8_DriverIRQHandler
- >> FLEXCOMM7_DriverIRQHandler
- >> FLEXCOMM6_DriverIRQHandler
- >> FLEXCOMM5_DriverIRQHandler
- >> FLEXCOMM4_DriverIRQHandler
- >> FLEXCOMM3_DriverIRQHandler
- >> FLEXCOMM2_DriverIRQHandler
- >> FLEXCOMM1_DriverIRQHandler
- >> FLEXCOMM0_DriverIRQHandler
- >> USART_ReadBlocking
- >> USART_WriteBlocking
- >> USART_GetDefaultConfig
- >> USART_SetBaudRate
- >> FLEXCOMM_Init
- >> USART_Init
- >> RESET_PeripheralReset
- >> HAL_UartReceiveBlocking
- >> HAL_UartSendBlocking
- >> HAL_UartInit
- >> RESET_ClearPeripheralReset
- >> PINT_EnableCallbackByIndex
- >> PINT_PinInterruptConfig
- >> PINT_Init
- >> arm_mat_mult_f32
- >> arm_mat_inverse_f32
- >> arm_mat_add_f32
- >> PQ_FIR
- >> PQ_MatrixScale
- >> PQ_SetConfig
- >> arm_cfft_q31
- >> SDK_DelayAtLeastUs
- >> LCD_WrString
- >> LCD_WrChar
- >> LCD_DrawPoint
- >> LCD_SetAreaAddr
- >> LCD_SetCursor
- >> SPI_MasterInit
- >> SPI_MasterGetDefaultConfig
- >> SPI_MasterTransferBlocking
- >> GPIO_PinInit
- >> GPIO_PortInit
- >> DMA_IRQHandle
- >> PQ_MatrixInversion
- >> PQ_MatrixMultiplication
- >> PQ_MatrixAddition
- >> PQ_TransformCFFT
- >> PQ_TransformIFFT

arm_cfft_q31 (Thumb, 102 bytes, Stack size 8 bytes, fsl_powerquad_cmsis.o(.text.arm_cfft_q31))
[Stack]

- Max Depth = 144
- Call Chain = arm_cfft_q31 ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> PQ_TransformCFFT
- >> PQ_TransformIFFT

[Called By]

- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

arm_cmplx_mag_f32 (Thumb, 58 bytes, Stack size 24 bytes, complexmathfunctions.o(.text.arm_cmplx_mag_f32))
[Stack]

- Max Depth = 40
- Call Chain = arm_cmplx_mag_f32 ⇒ __hardfp_sqrtf

[Calls]

- >> __hardfp_sqrtf

[Called By]

- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

arm_cos_f32 (Thumb, 18 bytes, Stack size 0 bytes, fsl_powerquad_cmsis.o(.text.arm_cos_f32))
[Called By]

- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

arm_float_to_q31 (Thumb, 48 bytes, Stack size 0 bytes, supportfunctions.o(.text.arm_float_to_q31))
[Called By]

- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

arm_mat_add_f32 (Thumb, 178 bytes, Stack size 24 bytes, fsl_powerquad_cmsis.o(.text.arm_mat_add_f32))
[Stack]

- Max Depth = 160
- Call Chain = arm_mat_add_f32 ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> PQ_MatrixAddition

[Called By]

- >> task_pq_mat_add

arm_mat_inverse_f32 (Thumb, 148 bytes, Stack size 4120 bytes, fsl_powerquad_cmsis.o(.text.arm_mat_inverse_f32))
[Stack]

- Max Depth = 4264
- Call Chain = arm_mat_inverse_f32 ⇒ PQ_MatrixInversion ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> PQ_MatrixInversion

[Called By]

- >> task_pq_mat_inv

arm_mat_mult_f32 (Thumb, 178 bytes, Stack size 24 bytes, fsl_powerquad_cmsis.o(.text.arm_mat_mult_f32))
[Stack]

- Max Depth = 160
- Call Chain = arm_mat_mult_f32 ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_assert
- >> PQ_MatrixMultiplication

[Called By]

- >> task_pq_mat_mul

arm_q31_to_float (Thumb, 52 bytes, Stack size 0 bytes, supportfunctions.o(.text.arm_q31_to_float))
[Called By]

- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

arm_sin_f32 (Thumb, 18 bytes, Stack size 0 bytes, fsl_powerquad_cmsis.o(.text.arm_sin_f32))
[Called By]

- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass

main (Thumb, 260 bytes, Stack size 0 bytes, main.o(.text.main))
[Stack]

- Max Depth = 304
- Call Chain = main ⇒ LCD_ClearScreen ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> PQ_Init
- >> FLEXSPI_NorFlash_Init
- >> FLEXSPI_NorFlash_GetConfig
- >> APP_InitUserKey
- >> DbgConsole_Printf
- >> LCD_WrPixelValue
- >> LCD_ClearScreen
- >> LCD_SetCursor
- >> LCD_Init
- >> BOARD_InitHardware
- >> memset

[Address Reference Count : 1]

- entry9a.o(.ARM.Collect$$$$0000000B)

task_pq_fft_128 (Thumb, 600 bytes, Stack size 104 bytes, task_pq_fft_128.o(.text.task_pq_fft_128))
[Stack]

- Max Depth = 456
- Call Chain = task_pq_fft_128 ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_d2iz
- >> __aeabi_dmul
- >> __aeabi_f2d
- >> arm_cmplx_mag_f32
- >> arm_q31_to_float
- >> arm_cfft_q31
- >> arm_float_to_q31
- >> arm_cos_f32
- >> LCD_PrintFreqSpecText
- >> LCD_PrintWaveformText
- >> LCD_PrintText
- >> LCD_PrintFreqSpec
- >> LCD_PrintWaveform
- >> DbgConsole_Printf
- >> LCD_ClearScreen
- >> memset
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_fft_256 (Thumb, 616 bytes, Stack size 104 bytes, task_pq_fft_256.o(.text.task_pq_fft_256))
[Stack]

- Max Depth = 456
- Call Chain = task_pq_fft_256 ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_d2iz
- >> __aeabi_dmul
- >> __aeabi_f2d
- >> arm_cmplx_mag_f32
- >> arm_q31_to_float
- >> arm_cfft_q31
- >> arm_float_to_q31
- >> arm_cos_f32
- >> LCD_PrintFreqSpecText
- >> LCD_PrintWaveformText
- >> LCD_PrintText
- >> LCD_PrintFreqSpec
- >> LCD_PrintWaveform
- >> DbgConsole_Printf
- >> LCD_ClearScreen
- >> memset
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_fft_512 (Thumb, 616 bytes, Stack size 104 bytes, task_pq_fft_512.o(.text.task_pq_fft_512))
[Stack]

- Max Depth = 456
- Call Chain = task_pq_fft_512 ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> __aeabi_d2iz
- >> __aeabi_dmul
- >> __aeabi_f2d
- >> arm_cmplx_mag_f32
- >> arm_q31_to_float
- >> arm_cfft_q31
- >> arm_float_to_q31
- >> arm_cos_f32
- >> LCD_PrintFreqSpecText
- >> LCD_PrintWaveformText
- >> LCD_PrintText
- >> LCD_PrintFreqSpec
- >> LCD_PrintWaveform
- >> DbgConsole_Printf
- >> LCD_ClearScreen
- >> memset
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_fir_highpass (Thumb, 688 bytes, Stack size 120 bytes, task_pq_fir.o(.text.task_pq_fir_highpass))
[Stack]

- Max Depth = 472
- Call Chain = task_pq_fir_highpass ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> PQ_FIR
- >> PQ_MatrixScale
- >> PQ_SetConfig
- >> __aeabi_d2f
- >> __aeabi_dadd
- >> arm_sin_f32
- >> __aeabi_d2iz
- >> __aeabi_dmul
- >> __aeabi_f2d
- >> LCD_PrintFreqSpecText
- >> LCD_PrintWaveformText
- >> LCD_PrintText
- >> LCD_PrintWaveformFir
- >> LCD_PrintWaveform
- >> PQ_Init
- >> LCD_ClearScreen
- >> memset
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_fir_lowpass (Thumb, 672 bytes, Stack size 112 bytes, task_pq_fir.o(.text.task_pq_fir_lowpass))
[Stack]

- Max Depth = 464
- Call Chain = task_pq_fir_lowpass ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> PQ_FIR
- >> PQ_MatrixScale
- >> PQ_SetConfig
- >> __aeabi_d2f
- >> __aeabi_dadd
- >> arm_sin_f32
- >> __aeabi_d2iz
- >> __aeabi_dmul
- >> __aeabi_f2d
- >> LCD_PrintFreqSpecText
- >> LCD_PrintWaveformText
- >> LCD_PrintText
- >> LCD_PrintWaveformFir
- >> LCD_PrintWaveform
- >> PQ_Init
- >> LCD_ClearScreen
- >> memset
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_mat_add (Thumb, 300 bytes, Stack size 3120 bytes, task_pq_mat_add.o(.text.task_pq_mat_add))
[Stack]

- Max Depth = 3472
- Call Chain = task_pq_mat_add ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> arm_mat_add_f32
- >> LCD_PrintText
- >> LCD_DisplayImage
- >> DbgConsole_Printf
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_mat_inv (Thumb, 236 bytes, Stack size 688 bytes, task_pq_mat_inv.o(.text.task_pq_mat_inv))
[Stack]

- Max Depth = 4952
- Call Chain = task_pq_mat_inv ⇒ arm_mat_inverse_f32 ⇒ PQ_MatrixInversion ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> arm_mat_inverse_f32
- >> LCD_PrintText
- >> LCD_DisplayImage
- >> DbgConsole_Printf
- >> __aeabi_memclr4
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_mat_mul (Thumb, 280 bytes, Stack size 3128 bytes, task_pq_mat_mul.o(.text.task_pq_mat_mul))
[Stack]

- Max Depth = 3480
- Call Chain = task_pq_mat_mul ⇒ LCD_PrintText ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> arm_mat_mult_f32
- >> LCD_PrintText
- >> LCD_DisplayImage
- >> DbgConsole_Printf
- >> __aeabi_memclr4
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

task_pq_records (Thumb, 288 bytes, Stack size 40 bytes, task_pq_recods.o(.text.task_pq_records))
[Stack]

- Max Depth = 432
- Call Chain = task_pq_records ⇒ LCD_WrString ⇒ LCD_WrChar ⇒ LCD_SetCursor ⇒ SPI_MasterTransferBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> LCD_DisplayImage
- >> LCD_WrString
- >> __2sprintf

[Address Reference Count : 1]

- main.o(.data.cAppLcdDisplayPageFunc)

user_button_callback (Thumb, 44 bytes, Stack size 0 bytes, task_user_key.o(.text.user_button_callback))
[Stack]

- Max Depth = 136
- Call Chain = user_button_callback ⇒ DbgConsole_Printf ⇒ DbgConsole_Vprintf ⇒ memcpy

[Calls]

- >> DbgConsole_Printf

[Address Reference Count : 1]

- task_user_key.o(.text.APP_InitUserKey)

__0sprintf$6 (Thumb, 34 bytes, Stack size 24 bytes, printf6.o(i.__0sprintf$6), UNUSED)
[Calls]

- >> _sputc
- >> _printf_core

__1sprintf$6 (Thumb, 0 bytes, Stack size 24 bytes, printf6.o(i.__0sprintf$6), UNUSED)

__2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf6.o(i.__0sprintf$6))
[Stack]

- Max Depth = 24
- Call Chain = __2sprintf

[Called By]

- >> task_pq_records
- >> task_pq_fir_highpass
- >> task_pq_fir_lowpass
- >> task_pq_mat_mul
- >> task_pq_mat_inv
- >> task_pq_mat_add
- >> task_pq_fft_512
- >> task_pq_fft_256
- >> task_pq_fft_128

__hardfp_sqrtf (Thumb, 58 bytes, Stack size 16 bytes, sqrtf.o(i.__hardfp_sqrtf))
[Stack]

- Max Depth = 16
- Call Chain = __hardfp_sqrtf

[Calls]

- >> __set_errno

[Called By]

- >> arm_cmplx_mag_f32

__scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

__scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

__scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

__set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
[Called By]

- >> __hardfp_sqrtf

### Local Symbols

POWER_SetVoltageForProcess (Thumb, 950 bytes, Stack size 0 bytes, fsl_power.o(.text.POWER_SetVoltageForProcess))
[Called By]

- >> POWER_SetVoltageForFreq

_printf_core (Thumb, 748 bytes, Stack size 96 bytes, printf6.o(i._printf_core), UNUSED)
[Calls]

- >> __aeabi_uidivmod
- >> _printf_pre_padding
- >> _printf_post_padding

[Called By]

- >> __0sprintf$6

_printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf6.o(i._printf_post_padding), UNUSED)
[Called By]

- >> _printf_core

_printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf6.o(i._printf_pre_padding), UNUSED)
[Called By]

- >> _printf_core

_sputc (Thumb, 10 bytes, Stack size 0 bytes, printf6.o(i._sputc))
[Called By]

- >> __0sprintf$6

[Address Reference Count : 1]

- printf6.o(i.__0sprintf$6)

### Undefined Global Symbols