<map id="erpc::Transport" name="erpc::Transport">
<area shape="rect" id="node2" href="$classerpc_1_1_framed_transport.html" title="Base class for framed transport layers. " alt="" coords="189,259,343,285"/>
<area shape="rect" id="node13" href="$classerpc_1_1_inter_thread_buffer_transport.html" title="Very basic transport to send/receive messages between threads. " alt="" coords="163,436,369,463"/>
<area shape="rect" id="node14" href="$classerpc_1_1_m_u_transport.html" title="Transport that uses Messaging Unit (MU) for interprocessor messaging. " alt="" coords="201,487,331,513"/>
<area shape="rect" id="node15" href="$classerpc_1_1_r_p_msg_base_transport.html" title="Transport that other RPMsg transports inherits. " alt="" coords="175,537,357,564"/>
<area shape="rect" id="node19" href="$classerpc_1_1_r_p_msg_linux_transport.html" title="RPMSG Linux transport to send/receive messages through RPMSG endpoints based on github.com/NXPmicro/rpmsg&#45;sysfs/tree/0aa1817545a765c200b1b2f9b6680a420dcf9171 implementation. " alt="" coords="175,588,357,615"/>
<area shape="rect" id="node20" href="$classerpc_1_1_transport_arbitrator.html" title="Interposer to share transport between client and server. " alt="" coords="185,639,347,665"/>
<area shape="rect" id="node3" href="$classerpc_1_1_dspi_master_transport.html" title="Very basic transport to send/receive messages via DSPI. " alt="" coords="435,5,610,32"/>
<area shape="rect" id="node4" href="$classerpc_1_1_dspi_slave_transport.html" title="Very basic transport to send/receive messages via DSPI. " alt="" coords="439,56,606,83"/>
<area shape="rect" id="node5" href="$classerpc_1_1_i2c_slave_transport.html" title="Very basic transport to send/receive messages via I2C. " alt="" coords="444,107,601,133"/>
<area shape="rect" id="node6" href="$classerpc_1_1_serial_transport.html" title="Serial transport layer for host PC. " alt="" coords="451,157,594,184"/>
<area shape="rect" id="node7" href="$classerpc_1_1_spidev_master_transport.html" title="Very basic transport to send/receive messages via SPIdev. " alt="" coords="429,208,616,235"/>
<area shape="rect" id="node8" href="$classerpc_1_1_spi_master_transport.html" title="Very basic transport to send/receive messages via SPI. " alt="" coords="439,259,607,285"/>
<area shape="rect" id="node9" href="$classerpc_1_1_spi_slave_transport.html" title="Very basic transport to send/receive messages via SPI. " alt="" coords="443,309,602,336"/>
<area shape="rect" id="node10" href="$classerpc_1_1_t_c_p_transport.html" title="Client side of TCP/IP transport. " alt="" coords="455,360,590,387"/>
<area shape="rect" id="node11" href="$classerpc_1_1_uart_transport.html" title="Very basic transport to send/receive messages via UART. " alt="" coords="456,411,589,437"/>
<area shape="rect" id="node12" href="$classerpc_1_1_usb_cdc_transport.html" title="Very basic transport to send/receive messages via virtual USB CDC port. " alt="" coords="445,461,600,488"/>
<area shape="rect" id="node16" href="$classerpc_1_1_r_p_msg_r_t_o_s_transport.html" title="Transport that uses RPMsg zero copy RTOS API for interprocessor messaging. " alt="" coords="429,512,616,539"/>
<area shape="rect" id="node17" href="$classerpc_1_1_r_p_msg_transport.html" title="Transport that uses RPMsg zero copy API for interprocessor messaging. " alt="" coords="447,563,599,589"/>
<area shape="rect" id="node18" href="$classerpc_1_1_r_p_msg_t_t_y_r_t_o_s_transport.html" title="Transport that uses RPMsg zero copy RTOS API for interprocessor messaging. " alt="" coords="417,613,628,640"/>
</map>
