| Maestro Audio Framework v 1.0 NXP Semiconductors

Data Fields
STREAMER_MSG_T Struct Reference

Streamer Message Type. More...

`#include <streamer_api.h>`

## Data Fields
uint32_t | id
| Message Identifier, relative with STREAMER_MSG_ID.
int | errorcode
| Error Code.
int8_t | pipeline_index
| Pipeline Index.
StreamPipelineType | pipeline_type
| Pipeline Type.
ELEMENT_PROPERTY_T | element_property
| Property Structure.
PipelineState | state
| Pipeline State.
StreamInfoType | query_type
| Query Type.
StreamData | query_data
| Query Return Data.
uint32_t | event_id
| Event Identifier.
int | event_data
| Event Data.
uint32_t | time_ms
| Time.
char * | in_dev_name
| Input Device Name.
char * | out_dev_name
| Output Device Name.
OsaMutex * | mutex
OsaCondition * | cond
| Mutex to protect signal.
bool * | processed
| Signal to unlock wait for streamer response.
int32_t * | ret
| Flag to indicate streamer msg processed.
void * | get_value
| streamer message processing result

## Detailed Description

Structure for messages transmitted and received by the streamer task.

The documentation for this struct was generated from the following file:

- streamer_api.h