# Static Call Graph for image debug\hello_world.out

#<CALLGRAPH># ARM Linker, 6140002: Last Updated: Fri Jan 14 15:14:06 2022

### Maximum Stack Usage = 296 bytes + Unknown(Functions without stacksize, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ HAL_UartInitCommon ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

### Functions with no stack information

- Reset_Handler
- ACMP_DriverIRQHandler
- ADC0_DriverIRQHandler
- ADC1_DriverIRQHandler
- Analog_Glitch_DriverIRQHandler
- BusFault_Handler
- CAN0_IRQ0_DriverIRQHandler
- CAN0_IRQ1_DriverIRQHandler
- CDOG_DriverIRQHandler
- CSSV2_ERR_DriverIRQHandler
- CSS_IRQ1_DriverIRQHandler
- CTIMER0_DriverIRQHandler
- CTIMER1_DriverIRQHandler
- CTIMER2_DriverIRQHandler
- CTIMER3_DriverIRQHandler
- CTIMER4_DriverIRQHandler
- DAC0_DriverIRQHandler
- DAC1_DriverIRQHandler
- DAC2_DriverIRQHandler
- DMA0_DriverIRQHandler
- DMA1_DriverIRQHandler
- DMIC_DriverIRQHandler
- DebugMon_Handler
- DefaultISR
- ENC0_COMPARE_DriverIRQHandler
- ENC0_HOME_DriverIRQHandler
- ENC0_IDX_DriverIRQHandler
- ENC0_WDG_DriverIRQHandler
- ENC1_COMPARE_DriverIRQHandler
- ENC1_HOME_DriverIRQHandler
- ENC1_IDX_DriverIRQHandler
- ENC1_WDG_DriverIRQHandler
- EZH_ARCH_B0_DriverIRQHandler
- FLASH_DriverIRQHandler
- FLEXPWM0_CAPTURE_DriverIRQHandler
- FLEXPWM0_COMPARE0_DriverIRQHandler
- FLEXPWM0_COMPARE1_DriverIRQHandler
- FLEXPWM0_COMPARE2_DriverIRQHandler
- FLEXPWM0_COMPARE3_DriverIRQHandler
- FLEXPWM0_FAULT_DriverIRQHandler
- FLEXPWM0_RELOAD0_DriverIRQHandler
- FLEXPWM0_RELOAD1_DriverIRQHandler
- FLEXPWM0_RELOAD2_DriverIRQHandler
- FLEXPWM0_RELOAD3_DriverIRQHandler
- FLEXPWM0_RELOAD_ERROR_DriverIRQHandler
- FLEXPWM1_CAPTURE_DriverIRQHandler
- FLEXPWM1_COMPARE0_DriverIRQHandler
- FLEXPWM1_COMPARE1_DriverIRQHandler
- FLEXPWM1_COMPARE2_DriverIRQHandler
- FLEXPWM1_COMPARE3_DriverIRQHandler
- FLEXPWM1_FAULT_DriverIRQHandler
- FLEXPWM1_RELOAD0_DriverIRQHandler
- FLEXPWM1_RELOAD1_DriverIRQHandler
- FLEXPWM1_RELOAD2_DriverIRQHandler
- FLEXPWM1_RELOAD3_DriverIRQHandler
- FLEXPWM1_RELOAD_ERROR_DriverIRQHandler
- FlexSPI0_DriverIRQHandler
- Freqme_DriverIRQHandler
- GINT0_DriverIRQHandler
- GINT1_DriverIRQHandler
- HSCMP0_DriverIRQHandler
- HSCMP1_DriverIRQHandler
- HSCMP2_DriverIRQHandler
- HWVAD0_DriverIRQHandler
- I3C0_DriverIRQHandler
- ITRC0_DriverIRQHandler
- MRT0_DriverIRQHandler
- MemManage_Handler
- OS_EVENT_DriverIRQHandler
- PIN_INT0_DriverIRQHandler
- PIN_INT1_DriverIRQHandler
- PIN_INT2_DriverIRQHandler
- PIN_INT3_DriverIRQHandler
- PIN_INT4_DriverIRQHandler
- PIN_INT5_DriverIRQHandler
- PIN_INT6_DriverIRQHandler
- PIN_INT7_DriverIRQHandler
- PKC_DriverIRQHandler
- PKC_ERR_DriverIRQHandler
- POWERQUAD_DriverIRQHandler
- PUF_DriverIRQHandler
- RAM_PARITY_ECC_ERR_DriverIRQHandler
- RTC_DriverIRQHandler
- Reserved127_DriverIRQHandler
- Reserved130_DriverIRQHandler
- Reserved131_DriverIRQHandler
- Reserved132_DriverIRQHandler
- Reserved133_DriverIRQHandler
- Reserved56_DriverIRQHandler
- Reserved57_DriverIRQHandler
- Reserved58_DriverIRQHandler
- Reserved62_DriverIRQHandler
- Reserved63_DriverIRQHandler
- Reserved64_DriverIRQHandler
- Reserved77_DriverIRQHandler
- Reserved79_DriverIRQHandler
- Reserved80_DriverIRQHandler
- Reserved84_DriverIRQHandler
- Reserved85_DriverIRQHandler
- Reserved86_DriverIRQHandler
- Reserved87_DriverIRQHandler
- Reserved88_DriverIRQHandler
- Reserved89_DriverIRQHandler
- SCT0_DriverIRQHandler
- SEC_GPIO_INT0_IRQ0_DriverIRQHandler
- SEC_GPIO_INT0_IRQ1_DriverIRQHandler
- SEC_HYPERVISOR_CALL_DriverIRQHandler
- SEC_VIO_DriverIRQHandler
- SHA_DriverIRQHandler
- SPI_FILTER_DriverIRQHandler
- SecureFault_Handler
- Tamper_DriverIRQHandler
- USB0_DriverIRQHandler
- USB0_NEEDCLK_DriverIRQHandler
- UTICK0_DriverIRQHandler
- UsageFault_Handler
- WAKEUP_DriverIRQHandler
- WDT_BOD_DriverIRQHandler
- NMI_Handler
- HardFault_Handler
- SVC_Handler
- PendSV_Handler
- SysTick_Handler
- WDT_BOD_IRQHandler
- DMA0_IRQHandler
- GINT0_IRQHandler
- GINT1_IRQHandler
- PIN_INT0_IRQHandler
- PIN_INT1_IRQHandler
- PIN_INT2_IRQHandler
- PIN_INT3_IRQHandler
- UTICK0_IRQHandler
- MRT0_IRQHandler
- CTIMER0_IRQHandler
- CTIMER1_IRQHandler
- SCT0_IRQHandler
- CTIMER3_IRQHandler
- FLEXCOMM0_IRQHandler
- FLEXCOMM1_IRQHandler
- FLEXCOMM2_IRQHandler
- FLEXCOMM3_IRQHandler
- FLEXCOMM4_IRQHandler
- FLEXCOMM5_IRQHandler
- FLEXCOMM6_IRQHandler
- FLEXCOMM7_IRQHandler
- ADC0_IRQHandler
- ADC1_IRQHandler
- ACMP_IRQHandler
- DMIC_IRQHandler
- HWVAD0_IRQHandler
- USB0_NEEDCLK_IRQHandler
- USB0_IRQHandler
- RTC_IRQHandler
- EZH_ARCH_B0_IRQHandler
- WAKEUP_IRQHandler
- PIN_INT4_IRQHandler
- PIN_INT5_IRQHandler
- PIN_INT6_IRQHandler
- PIN_INT7_IRQHandler
- CTIMER2_IRQHandler
- CTIMER4_IRQHandler
- OS_EVENT_IRQHandler
- FlexSPI0_IRQHandler
- Reserved56_IRQHandler
- Reserved57_IRQHandler
- Reserved58_IRQHandler
- CAN0_IRQ0_IRQHandler
- CAN0_IRQ1_IRQHandler
- SPI_FILTER_IRQHandler
- Reserved62_IRQHandler
- Reserved63_IRQHandler
- Reserved64_IRQHandler
- SEC_HYPERVISOR_CALL_IRQHandler
- SEC_GPIO_INT0_IRQ0_IRQHandler
- SEC_GPIO_INT0_IRQ1_IRQHandler
- Freqme_IRQHandler
- SEC_VIO_IRQHandler
- SHA_IRQHandler
- PKC_IRQHandler
- PUF_IRQHandler
- POWERQUAD_IRQHandler
- DMA1_IRQHandler
- FLEXCOMM8_IRQHandler
- CDOG_IRQHandler
- Reserved77_IRQHandler
- I3C0_IRQHandler
- Reserved79_IRQHandler
- Reserved80_IRQHandler
- CSS_IRQ1_IRQHandler
- Tamper_IRQHandler
- Analog_Glitch_IRQHandler
- Reserved84_IRQHandler
- Reserved85_IRQHandler
- Reserved86_IRQHandler
- Reserved87_IRQHandler
- Reserved88_IRQHandler
- Reserved89_IRQHandler
- DAC0_IRQHandler
- DAC1_IRQHandler
- DAC2_IRQHandler
- HSCMP0_IRQHandler
- HSCMP1_IRQHandler
- HSCMP2_IRQHandler
- FLEXPWM0_CAPTURE_IRQHandler
- FLEXPWM0_FAULT_IRQHandler
- FLEXPWM0_RELOAD_ERROR_IRQHandler
- FLEXPWM0_COMPARE0_IRQHandler
- FLEXPWM0_RELOAD0_IRQHandler
- FLEXPWM0_COMPARE1_IRQHandler
- FLEXPWM0_RELOAD1_IRQHandler
- FLEXPWM0_COMPARE2_IRQHandler
- FLEXPWM0_RELOAD2_IRQHandler
- FLEXPWM0_COMPARE3_IRQHandler
- FLEXPWM0_RELOAD3_IRQHandler
- FLEXPWM1_CAPTURE_IRQHandler
- FLEXPWM1_FAULT_IRQHandler
- FLEXPWM1_RELOAD_ERROR_IRQHandler
- FLEXPWM1_COMPARE0_IRQHandler
- FLEXPWM1_RELOAD0_IRQHandler
- FLEXPWM1_COMPARE1_IRQHandler
- FLEXPWM1_RELOAD1_IRQHandler
- FLEXPWM1_COMPARE2_IRQHandler
- FLEXPWM1_RELOAD2_IRQHandler
- FLEXPWM1_COMPARE3_IRQHandler
- FLEXPWM1_RELOAD3_IRQHandler
- ENC0_COMPARE_IRQHandler
- ENC0_HOME_IRQHandler
- ENC0_WDG_IRQHandler
- ENC0_IDX_IRQHandler
- ENC1_COMPARE_IRQHandler
- ENC1_HOME_IRQHandler
- ENC1_WDG_IRQHandler
- ENC1_IDX_IRQHandler
- ITRC0_IRQHandler
- Reserved127_IRQHandler
- CSSV2_ERR_IRQHandler
- PKC_ERR_IRQHandler
- Reserved130_IRQHandler
- Reserved131_IRQHandler
- Reserved132_IRQHandler
- Reserved133_IRQHandler
- FLASH_IRQHandler
- RAM_PARITY_ECC_ERR_IRQHandler

### Function Pointers

- ACMP_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ACMP_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ADC0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ADC0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ADC1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ADC1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Analog_Glitch_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Analog_Glitch_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- BusFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CAN0_IRQ0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CAN0_IRQ0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CAN0_IRQ1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CAN0_IRQ1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CDOG_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CDOG_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CSSV2_ERR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CSSV2_ERR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CSS_IRQ1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CSS_IRQ1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- CTIMER4_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- CTIMER4_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DAC0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DAC0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DAC1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DAC1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DAC2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DAC2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DMA0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DMA0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DMA1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DMA1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DMIC_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- DMIC_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- DebugMon_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_COMPARE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_COMPARE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_HOME_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_HOME_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_IDX_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_IDX_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC0_WDG_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC0_WDG_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_COMPARE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_COMPARE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_HOME_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_HOME_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_IDX_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_IDX_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ENC1_WDG_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ENC1_WDG_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- EZH_ARCH_B0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- EZH_ARCH_B0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLASH_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLASH_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM0_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM0_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM1_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM1_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM2_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM2_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM3_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM3_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM4_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM4_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM4_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM5_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM5_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM5_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM6_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM6_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM6_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM7_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM7_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM7_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXCOMM8_DriverIRQHandler from fsl_flexcomm.o(.text.FLEXCOMM8_DriverIRQHandler) referenced from startup_lpc55s36.o(.text)
- FLEXCOMM8_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_CAPTURE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_CAPTURE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_COMPARE3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_COMPARE3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_FAULT_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_FAULT_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM0_RELOAD_ERROR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM0_RELOAD_ERROR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_CAPTURE_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_CAPTURE_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_COMPARE3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_COMPARE3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_FAULT_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_FAULT_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FLEXPWM1_RELOAD_ERROR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FLEXPWM1_RELOAD_ERROR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- FlexSPI0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- FlexSPI0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Freqme_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Freqme_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- GINT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- GINT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- GINT1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- GINT1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HAL_UartReceiveBlocking from fsl_adapter_usart.o(.text.HAL_UartReceiveBlocking) referenced 2 times from fsl_debug_console.o(.text.DbgConsole_Init)
- HAL_UartSendBlocking from fsl_adapter_usart.o(.text.HAL_UartSendBlocking) referenced 2 times from fsl_debug_console.o(.text.DbgConsole_Init)
- HSCMP0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HSCMP0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HSCMP1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HSCMP1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HSCMP2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HSCMP2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HWVAD0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- HWVAD0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HardFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- HardFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- I3C0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- I3C0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- ITRC0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- ITRC0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- MRT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- MRT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- MemManage_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- NMI_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- NMI_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- OS_EVENT_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- OS_EVENT_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT2_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT2_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT3_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT3_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT4_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT4_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT5_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT5_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT6_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT6_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PIN_INT7_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PIN_INT7_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PKC_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PKC_ERR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PKC_ERR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PKC_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- POWERQUAD_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- POWERQUAD_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PUF_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- PUF_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PendSV_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- PendSV_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- RAM_PARITY_ECC_ERR_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- RAM_PARITY_ECC_ERR_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- RTC_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- RTC_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved127_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved127_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved130_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved130_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved131_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved131_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved132_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved132_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved133_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved133_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved56_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved56_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved57_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved57_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved58_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved58_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved62_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved62_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved63_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved63_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved64_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved64_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved77_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved77_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved79_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved79_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved80_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved80_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved84_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved84_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved85_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved85_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved86_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved86_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved87_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved87_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved88_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved88_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reserved89_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Reserved89_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- Reset_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SCT0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SCT0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_GPIO_INT0_IRQ0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SEC_GPIO_INT0_IRQ0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_GPIO_INT0_IRQ1_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SEC_GPIO_INT0_IRQ1_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_HYPERVISOR_CALL_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SEC_HYPERVISOR_CALL_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SEC_VIO_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SEC_VIO_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SHA_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SHA_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SPI_FILTER_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SPI_FILTER_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SVC_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SVC_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SecureFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SysTick_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- SysTick_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- SystemInit from system_lpc55s36.o(.text.SystemInit) referenced from startup_lpc55s36.o(.text)
- Tamper_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- Tamper_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- USB0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- USB0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- USB0_NEEDCLK_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- USB0_NEEDCLK_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- UTICK0_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- UTICK0_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- UsageFault_Handler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- WAKEUP_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- WAKEUP_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- WDT_BOD_DriverIRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.text)
- WDT_BOD_IRQHandler from startup_lpc55s36.o(.text) referenced from startup_lpc55s36.o(.isr_vector)
- __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc55s36.o(.text)
- main from hello_world.o(.text.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

### Global Symbols

__main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

_main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry4.o(.ARM.Collect$$$$00000003))

_main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Calls]

- >> __scatterload

__main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Called By]

- >> __scatterload

_main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

_main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

_main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

__rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

__rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

Reset_Handler (Thumb, 52 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ACMP_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ADC0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ADC1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Analog_Glitch_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

BusFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CAN0_IRQ0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CAN0_IRQ1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CDOG_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CSSV2_ERR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CSS_IRQ1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

CTIMER4_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DAC0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DAC1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DAC2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DMA0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DMA1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DMIC_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

DebugMon_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DefaultISR (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Called By]

- >> ACMP_DriverIRQHandler

ENC0_COMPARE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_HOME_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_IDX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC0_WDG_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_COMPARE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_HOME_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_IDX_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ENC1_WDG_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

EZH_ARCH_B0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLASH_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_CAPTURE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_COMPARE3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_FAULT_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM0_RELOAD_ERROR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_CAPTURE_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_COMPARE3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_FAULT_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXPWM1_RELOAD_ERROR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FlexSPI0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Freqme_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

GINT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

GINT1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HSCMP0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HSCMP1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HSCMP2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

HWVAD0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

I3C0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

ITRC0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

MRT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

MemManage_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

OS_EVENT_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT2_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT3_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT4_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT5_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT6_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PIN_INT7_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PKC_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PKC_ERR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

POWERQUAD_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

PUF_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

RAM_PARITY_ECC_ERR_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

RTC_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved127_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved130_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved131_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved132_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved133_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved56_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved57_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved58_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved62_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved63_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved64_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved77_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved79_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved80_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved84_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved85_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved86_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved87_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved88_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

Reserved89_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SCT0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_GPIO_INT0_IRQ0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_GPIO_INT0_IRQ1_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_HYPERVISOR_CALL_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SEC_VIO_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SHA_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SPI_FILTER_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SecureFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Tamper_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

USB0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

USB0_NEEDCLK_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

UTICK0_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

UsageFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

WAKEUP_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

WDT_BOD_DriverIRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

NMI_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

HardFault_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

SVC_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

PendSV_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

SysTick_Handler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 2]

- startup_lpc55s36.o(.text)
- startup_lpc55s36.o(.isr_vector)

WDT_BOD_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DMA0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

GINT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

GINT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

UTICK0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

MRT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SCT0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ADC0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ADC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ACMP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DMIC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HWVAD0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

USB0_NEEDCLK_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

USB0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

RTC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

EZH_ARCH_B0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

WAKEUP_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT5_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT6_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PIN_INT7_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CTIMER4_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

OS_EVENT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FlexSPI0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved56_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved57_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved58_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CAN0_IRQ0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CAN0_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SPI_FILTER_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved62_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved63_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved64_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_HYPERVISOR_CALL_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_GPIO_INT0_IRQ0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_GPIO_INT0_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Freqme_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SEC_VIO_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

SHA_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PKC_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PUF_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

POWERQUAD_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DMA1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXCOMM8_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CDOG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved77_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

I3C0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved79_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved80_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CSS_IRQ1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Tamper_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Analog_Glitch_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved84_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved85_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved86_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved87_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved88_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved89_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DAC0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DAC1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

DAC2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HSCMP0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HSCMP1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

HSCMP2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_CAPTURE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_COMPARE3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM0_RELOAD3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_CAPTURE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_FAULT_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD_ERROR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD1_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD2_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_COMPARE3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLEXPWM1_RELOAD3_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_COMPARE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_HOME_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_WDG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC0_IDX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_COMPARE_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_HOME_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_WDG_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ENC1_IDX_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

ITRC0_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved127_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

CSSV2_ERR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

PKC_ERR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved130_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved131_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved132_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

Reserved133_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

FLASH_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

RAM_PARITY_ECC_ERR_IRQHandler (Thumb, 4 bytes, Stack size unknown bytes, startup_lpc55s36.o(.text))
[Address Reference Count : 1]

- startup_lpc55s36.o(.isr_vector)

__aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
[Stack]

- Max Depth = 40
- Call Chain = __aeabi_uldivmod

[Calls]

- >> __aeabi_llsr
- >> __aeabi_llsl

[Called By]

- >> SDK_DelayAtLeastUs

memset (Thumb, 18 bytes, Stack size 8 bytes, memset.o(.text))
[Stack]

- Max Depth = 8
- Call Chain = memset

[Called By]

- >> USART_GetDefaultConfig

strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
[Called By]

- >> DbgConsole_PrintfFormattedData

__aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
[Called By]

- >> __aeabi_uldivmod

_ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

__aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
[Called By]

- >> __aeabi_uldivmod

_ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

__scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
[Calls]

- >> __main_after_scatterload

[Called By]

- >> _main_scatterload

__scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

BOARD_BootClockPLL150M (Thumb, 184 bytes, Stack size 64 bytes, clock_config.o(.text.BOARD_BootClockPLL150M))
[Stack]

- Max Depth = 232
- Call Chain = BOARD_BootClockPLL150M ⇒ CLOCK_SetPLL0Freq ⇒ SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> CLOCK_SetClkDiv
- >> CLOCK_AttachClk
- >> POWER_SetVoltageForFreq
- >> POWER_PowerInit
- >> CLOCK_SetupFROClocking
- >> CLOCK_SetupExtClocking
- >> CLOCK_SetPLL0Freq
- >> CLOCK_SetFLASHAccessCyclesForFreq
- >> POWER_DisablePD

[Called By]

- >> main

BOARD_InitDebugConsole (Thumb, 42 bytes, Stack size 8 bytes, board.o(.text.BOARD_InitDebugConsole))
[Stack]

- Max Depth = 296
- Call Chain = BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ HAL_UartInitCommon ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> DbgConsole_Init
- >> CLOCK_AttachClk
- >> RESET_ClearPeripheralReset

[Called By]

- >> main

BOARD_InitPins (Thumb, 38 bytes, Stack size 8 bytes, pin_mux.o(.text.BOARD_InitPins))
[Stack]

- Max Depth = 8
- Call Chain = BOARD_InitPins

[Calls]

- >> IOCON_PinMuxSet
- >> CLOCK_EnableClock

[Called By]

- >> main

CLOCK_AttachClk (Thumb, 112 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_AttachClk))
[Stack]

- Max Depth = 8
- Call Chain = CLOCK_AttachClk

[Called By]

- >> main
- >> BOARD_InitDebugConsole
- >> BOARD_BootClockPLL150M

CLOCK_FroHfTrim (Thumb, 38 bytes, Stack size 4 bytes, fsl_clock.o(.text.CLOCK_FroHfTrim))
[Stack]

- Max Depth = 4
- Call Chain = CLOCK_FroHfTrim

[Called By]

- >> CLOCK_SetupFROClocking

CLOCK_GetExtClkFreq (Thumb, 28 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetExtClkFreq))
[Called By]

- >> CLOCK_GetPLL0InClockRate

CLOCK_GetFro1MFreq (Thumb, 26 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetFro1MFreq))
[Called By]

- >> CLOCK_GetPLL0InClockRate

CLOCK_GetOsc32KFreq (Thumb, 40 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_GetOsc32KFreq))
[Called By]

- >> CLOCK_GetPLL0InClockRate

CLOCK_GetPLL0InClockRate (Thumb, 58 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_GetPLL0InClockRate))
[Stack]

- Max Depth = 8
- Call Chain = CLOCK_GetPLL0InClockRate

[Calls]

- >> CLOCK_GetOsc32KFreq
- >> CLOCK_GetFro1MFreq
- >> CLOCK_GetExtClkFreq

[Called By]

- >> CLOCK_SetPLL0Freq

CLOCK_SetClkDiv (Thumb, 56 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_SetClkDiv))
[Called By]

- >> main
- >> BOARD_BootClockPLL150M

CLOCK_SetFLASHAccessCyclesForFreq (Thumb, 106 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_SetFLASHAccessCyclesForFreq))
[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetPLL0Freq (Thumb, 212 bytes, Stack size 16 bytes, fsl_clock.o(.text.CLOCK_SetPLL0Freq))
[Stack]

- Max Depth = 168
- Call Chain = CLOCK_SetPLL0Freq ⇒ SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> SDK_DelayAtLeastUs
- >> CLOCK_GetPLL0InClockRate
- >> findPll0PreDiv
- >> POWER_EnablePD
- >> POWER_DisablePD
- >> CLOCK_IsPLL0Locked

[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetupExtClocking (Thumb, 66 bytes, Stack size 8 bytes, fsl_clock.o(.text.CLOCK_SetupExtClocking))
[Stack]

- Max Depth = 8
- Call Chain = CLOCK_SetupExtClocking

[Calls]

- >> POWER_DisablePD

[Called By]

- >> BOARD_BootClockPLL150M

CLOCK_SetupFROClocking (Thumb, 90 bytes, Stack size 16 bytes, fsl_clock.o(.text.CLOCK_SetupFROClocking))
[Stack]

- Max Depth = 20
- Call Chain = CLOCK_SetupFROClocking ⇒ CLOCK_FroHfTrim

[Calls]

- >> CLOCK_FroHfTrim
- >> POWER_DisablePD

[Called By]

- >> BOARD_BootClockPLL150M

DbgConsole_Getchar (Thumb, 44 bytes, Stack size 16 bytes, fsl_debug_console.o(.text.DbgConsole_Getchar))
[Stack]

- Max Depth = 16
- Call Chain = DbgConsole_Getchar

[Called By]

- >> main

DbgConsole_Init (Thumb, 78 bytes, Stack size 32 bytes, fsl_debug_console.o(.text.DbgConsole_Init))
[Stack]

- Max Depth = 288
- Call Chain = DbgConsole_Init ⇒ HAL_UartInit ⇒ HAL_UartInitCommon ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> HAL_UartInit

[Called By]

- >> BOARD_InitDebugConsole

DbgConsole_Printf (Thumb, 50 bytes, Stack size 24 bytes, fsl_debug_console.o(.text.DbgConsole_Printf))
[Stack]

- Max Depth = 144
- Call Chain = DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> DbgConsole_PrintfFormattedData

[Called By]

- >> main
- >> __aeabi_assert

DbgConsole_Putchar (Thumb, 42 bytes, Stack size 16 bytes, fsl_debug_console.o(.text.DbgConsole_Putchar))
[Stack]

- Max Depth = 16
- Call Chain = DbgConsole_Putchar

[Called By]

- >> main
- >> DbgConsole_PrintfPaddingCharacter
- >> DbgConsole_PrintfFormattedData

FLEXCOMM0_DriverIRQHandler (Thumb, 80 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM0_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM0_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM1_DriverIRQHandler (Thumb, 80 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM1_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM1_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM2_DriverIRQHandler (Thumb, 80 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM2_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM2_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM3_DriverIRQHandler (Thumb, 80 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM3_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM3_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM4_DriverIRQHandler (Thumb, 80 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM4_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM4_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM5_DriverIRQHandler (Thumb, 80 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM5_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM5_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM6_DriverIRQHandler (Thumb, 82 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM6_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM6_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM7_DriverIRQHandler (Thumb, 82 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM7_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM7_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM8_DriverIRQHandler (Thumb, 82 bytes, Stack size 8 bytes, fsl_flexcomm.o(.text.FLEXCOMM8_DriverIRQHandler))
[Stack]

- Max Depth = 152
- Call Chain = FLEXCOMM8_DriverIRQHandler ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> FLEXCOMM_GetInstance

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

FLEXCOMM_GetInstance (Thumb, 92 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM_GetInstance))
[Stack]

- Max Depth = 144
- Call Chain = FLEXCOMM_GetInstance ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert

[Called By]

- >> FLEXCOMM_Init
- >> FLEXCOMM8_DriverIRQHandler
- >> FLEXCOMM7_DriverIRQHandler
- >> FLEXCOMM6_DriverIRQHandler
- >> FLEXCOMM5_DriverIRQHandler
- >> FLEXCOMM4_DriverIRQHandler
- >> FLEXCOMM3_DriverIRQHandler
- >> FLEXCOMM2_DriverIRQHandler
- >> FLEXCOMM1_DriverIRQHandler
- >> FLEXCOMM0_DriverIRQHandler

FLEXCOMM_Init (Thumb, 84 bytes, Stack size 16 bytes, fsl_flexcomm.o(.text.FLEXCOMM_Init))
[Stack]

- Max Depth = 168
- Call Chain = FLEXCOMM_Init ⇒ RESET_PeripheralReset ⇒ RESET_ClearPeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> RESET_PeripheralReset
- >> FLEXCOMM_GetInstance
- >> FLEXCOMM_SetPeriph
- >> CLOCK_EnableClock

[Called By]

- >> USART_Init

HAL_UartInit (Thumb, 24 bytes, Stack size 16 bytes, fsl_adapter_usart.o(.text.HAL_UartInit))
[Stack]

- Max Depth = 256
- Call Chain = HAL_UartInit ⇒ HAL_UartInitCommon ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> HAL_UartInitCommon

[Called By]

- >> DbgConsole_Init

HAL_UartReceiveBlocking (Thumb, 104 bytes, Stack size 8 bytes, fsl_adapter_usart.o(.text.HAL_UartReceiveBlocking))
[Stack]

- Max Depth = 168
- Call Chain = HAL_UartReceiveBlocking ⇒ USART_ReadBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> USART_ReadBlocking
- >> HAL_UartGetStatus

[Address Reference Count : 1]

- fsl_debug_console.o(.text.DbgConsole_Init)

HAL_UartSendBlocking (Thumb, 102 bytes, Stack size 8 bytes, fsl_adapter_usart.o(.text.HAL_UartSendBlocking))
[Stack]

- Max Depth = 152
- Call Chain = HAL_UartSendBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> USART_WriteBlocking

[Address Reference Count : 1]

- fsl_debug_console.o(.text.DbgConsole_Init)

POWER_PowerInit (Thumb, 96 bytes, Stack size 0 bytes, fsl_power.o(.text.POWER_PowerInit))
[Called By]

- >> BOARD_BootClockPLL150M

POWER_SetVoltageForFreq (Thumb, 46 bytes, Stack size 8 bytes, fsl_power.o(.text.POWER_SetVoltageForFreq))
[Stack]

- Max Depth = 32
- Call Chain = POWER_SetVoltageForFreq ⇒ POWER_SetVoltageForProcess ⇒ POWER_SetSystemVoltage

[Calls]

- >> POWER_SetVoltageForProcess
- >> POWER_SetSystemPowerProfile

[Called By]

- >> BOARD_BootClockPLL150M

RESET_ClearPeripheralReset (Thumb, 66 bytes, Stack size 0 bytes, fsl_reset.o(.text.RESET_ClearPeripheralReset))
[Stack]

- Max Depth = 144
- Call Chain = RESET_ClearPeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert

[Called By]

- >> BOARD_InitDebugConsole
- >> RESET_PeripheralReset

RESET_PeripheralReset (Thumb, 16 bytes, Stack size 8 bytes, fsl_reset.o(.text.RESET_PeripheralReset))
[Stack]

- Max Depth = 152
- Call Chain = RESET_PeripheralReset ⇒ RESET_ClearPeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> RESET_ClearPeripheralReset
- >> RESET_SetPeripheralReset

[Called By]

- >> FLEXCOMM_Init

RESET_SetPeripheralReset (Thumb, 64 bytes, Stack size 0 bytes, fsl_reset.o(.text.RESET_SetPeripheralReset))
[Stack]

- Max Depth = 144
- Call Chain = RESET_SetPeripheralReset ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert

[Called By]

- >> RESET_PeripheralReset

SDK_DelayAtLeastUs (Thumb, 136 bytes, Stack size 8 bytes, fsl_common_arm.o(.text.SDK_DelayAtLeastUs))
[Stack]

- Max Depth = 152
- Call Chain = SDK_DelayAtLeastUs ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> DelayLoop
- >> __aeabi_uldivmod

[Called By]

- >> CLOCK_SetPLL0Freq

SystemInit (Thumb, 88 bytes, Stack size 8 bytes, system_lpc55s36.o(.text.SystemInit))
[Stack]

- Max Depth = 8
- Call Chain = SystemInit

[Calls]

- >> SystemInitHook

[Address Reference Count : 1]

- startup_lpc55s36.o(.text)

SystemInitHook (Thumb, 2 bytes, Stack size 0 bytes, system_lpc55s36.o(.text.SystemInitHook))
[Called By]

- >> SystemInit

USART_GetDefaultConfig (Thumb, 68 bytes, Stack size 16 bytes, fsl_usart.o(.text.USART_GetDefaultConfig))
[Stack]

- Max Depth = 160
- Call Chain = USART_GetDefaultConfig ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> memset

[Called By]

- >> HAL_UartInitCommon

USART_Init (Thumb, 368 bytes, Stack size 24 bytes, fsl_usart.o(.text.USART_Init))
[Stack]

- Max Depth = 200
- Call Chain = USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> USART_SetBaudRate
- >> FLEXCOMM_Init
- >> USART_EnableContinuousSCLK

[Called By]

- >> HAL_UartInitCommon

USART_ReadBlocking (Thumb, 166 bytes, Stack size 16 bytes, fsl_usart.o(.text.USART_ReadBlocking))
[Stack]

- Max Depth = 160
- Call Chain = USART_ReadBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartReceiveBlocking

USART_SetBaudRate (Thumb, 238 bytes, Stack size 32 bytes, fsl_usart.o(.text.USART_SetBaudRate))
[Stack]

- Max Depth = 176
- Call Chain = USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert

[Called By]

- >> USART_Init

USART_WriteBlocking (Thumb, 78 bytes, Stack size 0 bytes, fsl_usart.o(.text.USART_WriteBlocking))
[Stack]

- Max Depth = 144
- Call Chain = USART_WriteBlocking ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert

[Called By]

- >> HAL_UartSendBlocking

__aeabi_assert (Thumb, 60 bytes, Stack size 0 bytes, fsl_assert.o(.text.__aeabi_assert))
[Stack]

- Max Depth = 144
- Call Chain = __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> DbgConsole_Printf

[Called By]

- >> HAL_UartSendBlocking
- >> HAL_UartReceiveBlocking
- >> RESET_ClearPeripheralReset
- >> SDK_DelayAtLeastUs
- >> USART_WriteBlocking
- >> USART_SetBaudRate
- >> USART_ReadBlocking
- >> USART_Init
- >> USART_GetDefaultConfig
- >> RESET_SetPeripheralReset
- >> FLEXCOMM_GetInstance
- >> FLEXCOMM8_DriverIRQHandler
- >> FLEXCOMM7_DriverIRQHandler
- >> FLEXCOMM6_DriverIRQHandler
- >> FLEXCOMM5_DriverIRQHandler
- >> FLEXCOMM4_DriverIRQHandler
- >> FLEXCOMM3_DriverIRQHandler
- >> FLEXCOMM2_DriverIRQHandler
- >> FLEXCOMM1_DriverIRQHandler
- >> FLEXCOMM0_DriverIRQHandler
- >> HAL_UartInitCommon

main (Thumb, 80 bytes, Stack size 0 bytes, hello_world.o(.text.main))
[Stack]

- Max Depth = 296
- Call Chain = main ⇒ BOARD_InitDebugConsole ⇒ DbgConsole_Init ⇒ HAL_UartInit ⇒ HAL_UartInitCommon ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> DbgConsole_Putchar
- >> DbgConsole_Printf
- >> DbgConsole_Getchar
- >> CLOCK_SetClkDiv
- >> CLOCK_AttachClk
- >> BOARD_InitPins
- >> BOARD_InitDebugConsole
- >> BOARD_BootClockPLL150M

[Address Reference Count : 1]

- entry9a.o(.ARM.Collect$$$$0000000B)

__scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

__scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

__scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

### Local Symbols

CLOCK_EnableClock (Thumb, 16 bytes, Stack size 0 bytes, pin_mux.o(.text.CLOCK_EnableClock))
[Called By]

- >> BOARD_InitPins

IOCON_PinMuxSet (Thumb, 14 bytes, Stack size 0 bytes, pin_mux.o(.text.IOCON_PinMuxSet))
[Called By]

- >> BOARD_InitPins

POWER_DisablePD (Thumb, 22 bytes, Stack size 0 bytes, clock_config.o(.text.POWER_DisablePD))
[Called By]

- >> BOARD_BootClockPLL150M

DbgConsole_ConvertRadixNumToString (Thumb, 74 bytes, Stack size 16 bytes, fsl_debug_console.o(.text.DbgConsole_ConvertRadixNumToString))
[Stack]

- Max Depth = 16
- Call Chain = DbgConsole_ConvertRadixNumToString

[Called By]

- >> DbgConsole_PrintfFormattedData

DbgConsole_PrintfFormattedData (Thumb, 622 bytes, Stack size 88 bytes, fsl_debug_console.o(.text.DbgConsole_PrintfFormattedData))
[Stack]

- Max Depth = 120
- Call Chain = DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> DbgConsole_Putchar
- >> DbgConsole_PrintfPaddingCharacter
- >> DbgConsole_ConvertRadixNumToString
- >> strlen

[Called By]

- >> DbgConsole_Printf

DbgConsole_PrintfPaddingCharacter (Thumb, 32 bytes, Stack size 16 bytes, fsl_debug_console.o(.text.DbgConsole_PrintfPaddingCharacter))
[Stack]

- Max Depth = 32
- Call Chain = DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> DbgConsole_Putchar

[Called By]

- >> DbgConsole_PrintfFormattedData

DelayLoop (Thumb, 10 bytes, Stack size 0 bytes, fsl_common_arm.o(.text.DelayLoop))
[Called By]

- >> SDK_DelayAtLeastUs

CLOCK_IsPLL0Locked (Thumb, 16 bytes, Stack size 0 bytes, fsl_clock.o(.text.CLOCK_IsPLL0Locked))
[Called By]

- >> CLOCK_SetPLL0Freq

POWER_DisablePD (Thumb, 22 bytes, Stack size 0 bytes, fsl_clock.o(.text.POWER_DisablePD))
[Called By]

- >> CLOCK_SetupFROClocking
- >> CLOCK_SetupExtClocking
- >> CLOCK_SetPLL0Freq

POWER_EnablePD (Thumb, 22 bytes, Stack size 0 bytes, fsl_clock.o(.text.POWER_EnablePD))
[Called By]

- >> CLOCK_SetPLL0Freq

findPll0PreDiv (Thumb, 30 bytes, Stack size 0 bytes, fsl_clock.o(.text.findPll0PreDiv))
[Called By]

- >> CLOCK_SetPLL0Freq

POWER_GetPartProcessCorner (Thumb, 78 bytes, Stack size 0 bytes, fsl_power.o(.text.POWER_GetPartProcessCorner))
[Called By]

- >> POWER_SetVoltageForProcess

POWER_SetSystemPowerProfile (Thumb, 150 bytes, Stack size 0 bytes, fsl_power.o(.text.POWER_SetSystemPowerProfile))
[Called By]

- >> POWER_SetVoltageForFreq

POWER_SetSystemVoltage (Thumb, 336 bytes, Stack size 16 bytes, fsl_power.o(.text.POWER_SetSystemVoltage))
[Stack]

- Max Depth = 16
- Call Chain = POWER_SetSystemVoltage

[Called By]

- >> POWER_SetVoltageForProcess

POWER_SetVoltageForProcess (Thumb, 78 bytes, Stack size 8 bytes, fsl_power.o(.text.POWER_SetVoltageForProcess))
[Stack]

- Max Depth = 24
- Call Chain = POWER_SetVoltageForProcess ⇒ POWER_SetSystemVoltage

[Calls]

- >> POWER_SetSystemVoltage
- >> POWER_GetPartProcessCorner

[Called By]

- >> POWER_SetVoltageForFreq

USART_EnableContinuousSCLK (Thumb, 18 bytes, Stack size 0 bytes, fsl_usart.o(.text.USART_EnableContinuousSCLK))
[Called By]

- >> USART_Init

CLOCK_EnableClock (Thumb, 24 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.CLOCK_EnableClock))
[Called By]

- >> FLEXCOMM_Init

FLEXCOMM_PeripheralIsPresent (Thumb, 40 bytes, Stack size 0 bytes, fsl_flexcomm.o(.text.FLEXCOMM_PeripheralIsPresent))
[Called By]

- >> FLEXCOMM_SetPeriph

FLEXCOMM_SetPeriph (Thumb, 50 bytes, Stack size 16 bytes, fsl_flexcomm.o(.text.FLEXCOMM_SetPeriph))
[Stack]

- Max Depth = 16
- Call Chain = FLEXCOMM_SetPeriph

[Calls]

- >> FLEXCOMM_PeripheralIsPresent

[Called By]

- >> FLEXCOMM_Init

HAL_UartGetStatus (Thumb, 10 bytes, Stack size 0 bytes, fsl_adapter_usart.o(.text.HAL_UartGetStatus))
[Called By]

- >> HAL_UartReceiveBlocking
- >> HAL_UartInitCommon

HAL_UartInitCommon (Thumb, 220 bytes, Stack size 40 bytes, fsl_adapter_usart.o(.text.HAL_UartInitCommon))
[Stack]

- Max Depth = 240
- Call Chain = HAL_UartInitCommon ⇒ USART_Init ⇒ USART_SetBaudRate ⇒ __aeabi_assert ⇒ DbgConsole_Printf ⇒ DbgConsole_PrintfFormattedData ⇒ DbgConsole_PrintfPaddingCharacter ⇒ DbgConsole_Putchar

[Calls]

- >> __aeabi_assert
- >> USART_Init
- >> USART_GetDefaultConfig
- >> HAL_UartGetStatus

[Called By]

- >> HAL_UartInit

### Undefined Global Symbols