Status of the operation: SUCCESS: New workspace created: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash
Status of the operation: SUCCESS: New workspace created: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash
Status of the operation: CANCELLED: Manufacturing Tool cancelled by the user
Status of the operation: CANCELLED: Manufacturing Tool cancelled by the user
ERROR: Uncaught exception: ValueError: invalid literal for int() with base 16: ''
ERROR: Uncaught exception: ValueError: invalid literal for int() with base 16: ''
ERROR: Traceback (most recent call last):
  File "src\gui\main\main_win_ctrl.py", line 632, in on_sb_editor_menu_item
  File "src\gui\manufacturing\sb_file_editor_dlg_ctrl.py", line 119, in __init__
  File "src\logic\app_config\sb_model.py", line 517, in __init__
  File "src\logic\app_config\sb_utils.py", line 1199, in create_sb_model_variables
  File "src\logic\app_config\sb_utils.py", line 1141, in _create_method_variables
ValueError: invalid literal for int() with base 16: ''

ERROR: Traceback (most recent call last):
  File "src\gui\main\main_win_ctrl.py", line 632, in on_sb_editor_menu_item
  File "src\gui\manufacturing\sb_file_editor_dlg_ctrl.py", line 119, in __init__
  File "src\logic\app_config\sb_model.py", line 517, in __init__
  File "src\logic\app_config\sb_utils.py", line 1199, in create_sb_model_variables
  File "src\logic\app_config\sb_utils.py", line 1141, in _create_method_variables
ValueError: invalid literal for int() with base 16: ''

Status of the operation: CANCELLED: Cancelled by the user: Manufacturing package imported into new workspace
Status of the operation: CANCELLED: Cancelled by the user: Manufacturing package imported into new workspace
Write script created: (workspace)/gen_scripts\write_cmpa_win.bat
Write script created: (workspace)/gen_scripts\write_cmpa_win.bat
Executing script "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat"
Executing script "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat"
### SCRIPT: Write user configuration to processor: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat
### SCRIPT: Write user configuration to processor: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (455ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
### Check connection ###
blhost -t 2000 -p COM7,115200 -j -- get-property 1 0
{
   "command": "get-property",
   "response": [
      1258488065
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded
### Write Customer Manufacturing/Factory Programmable Area [CMPA] ###
blhost -t 5000 -p COM7,115200 -j -- write-memory 0x0003E200 "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin"
{
   "command": "write-memory",
   "response": [
      512
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded

### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (455ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
### Check connection ###
blhost -t 2000 -p COM7,115200 -j -- get-property 1 0
{
   "command": "get-property",
   "response": [
      1258488065
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded
### Write Customer Manufacturing/Factory Programmable Area [CMPA] ###
blhost -t 5000 -p COM7,115200 -j -- write-memory 0x0003E200 "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin"
{
   "command": "write-memory",
   "response": [
      512
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded

### RESULT of the script `Write user configuration to processor`: SUCCESS (return code = [0]SUCCESS)
### RESULT of the script `Write user configuration to processor`: SUCCESS (return code = [0]SUCCESS)
Status of the operation: SUCCESS: Write user configuration to processor
Status of the operation: SUCCESS: Write user configuration to processor
##########################################################################################################
##########################################################################################################
Build image - operation started at 2023-11-01 14:45:28
Build image - operation started at 2023-11-01 14:45:28
##########################################################################################################
##########################################################################################################
Build script generated: build_image_lnx.sh
Build script generated: build_image_lnx.sh
Build script generated: build_image_win.bat
Build script generated: build_image_win.bat
Build script generated: build_image_mac.sh
Build script generated: build_image_mac.sh
Executing script "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat"
Executing script "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat"
### SCRIPT: Building image: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat
### SCRIPT: Building image: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat
### Create bootable image ###
nxpimage mbi export -c "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\mbi_config.json"
Success. (Master Boot Image: C:/Sandeep Work/Recovery Boot 1-bit SPI Flash/bootable_images/lpcxpresso55s36_led_blinky.bin created.)
nxpimage succeeded
### Create CFPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c \"C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.json\" -o \"C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin\"
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (455ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (425ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin

### Create bootable image ###
nxpimage mbi export -c "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\mbi_config.json"
Success. (Master Boot Image: C:/Sandeep Work/Recovery Boot 1-bit SPI Flash/bootable_images/lpcxpresso55s36_led_blinky.bin created.)
nxpimage succeeded
### Create CFPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c \"C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.json\" -o \"C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin\"
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (455ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (425ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin

### RESULT of the script `Building image`: SUCCESS (return code = [0]SUCCESS)
### RESULT of the script `Building image`: SUCCESS (return code = [0]SUCCESS)
Status of the operation: SUCCESS: Building image
Status of the operation: SUCCESS: Building image
Write script created: (workspace)/gen_scripts\write_cmpa_win.bat
Write script created: (workspace)/gen_scripts\write_cmpa_win.bat
Executing script "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat"
Executing script "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat"
### SCRIPT: Write user configuration to processor: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat
### SCRIPT: Write user configuration to processor: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (380ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
### Check connection ###
blhost -t 2000 -p COM7,115200 -j -- get-property 1 0
{
   "command": "get-property",
   "response": [
      1258488065
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded
### Write Customer Manufacturing/Factory Programmable Area [CMPA] ###
blhost -t 5000 -p COM7,115200 -j -- write-memory 0x0003E200 "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin"
{
   "command": "write-memory",
   "response": [
      512
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded

### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (380ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
### Check connection ###
blhost -t 2000 -p COM7,115200 -j -- get-property 1 0
{
   "command": "get-property",
   "response": [
      1258488065
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded
### Write Customer Manufacturing/Factory Programmable Area [CMPA] ###
blhost -t 5000 -p COM7,115200 -j -- write-memory 0x0003E200 "C:\Sandeep Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin"
{
   "command": "write-memory",
   "response": [
      512
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded

### RESULT of the script `Write user configuration to processor`: SUCCESS (return code = [0]SUCCESS)
### RESULT of the script `Write user configuration to processor`: SUCCESS (return code = [0]SUCCESS)
Status of the operation: SUCCESS: Write user configuration to processor
Status of the operation: SUCCESS: Write user configuration to processor
Status of the operation: SUCCESS: Settings loaded successfully; workspace: `C:\Work\Recovery Boot 1-bit SPI Flash`
Status of the operation: SUCCESS: Settings loaded successfully; workspace: `C:\Work\Recovery Boot 1-bit SPI Flash`
Write script created: (workspace)/gen_scripts\write_cmpa_win.bat
Write script created: (workspace)/gen_scripts\write_cmpa_win.bat
Executing script "C:\Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat"
Executing script "C:\Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat"
### SCRIPT: Write user configuration to processor: C:\Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat
### SCRIPT: Write user configuration to processor: C:\Work\Recovery Boot 1-bit SPI Flash\gen_scripts\write_cmpa_win.bat
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (502ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
### Check connection ###
blhost -t 2000 -p COM7,115200 -j -- get-property 1 0
{
   "command": "get-property",
   "response": [
      1258488065
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded
### Write Customer Manufacturing/Factory Programmable Area [CMPA] ###
blhost -t 5000 -p COM7,115200 -j -- write-memory 0x0003E200 "C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin"
{
   "command": "write-memory",
   "response": [
      512
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded

### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (502ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
### Check connection ###
blhost -t 2000 -p COM7,115200 -j -- get-property 1 0
{
   "command": "get-property",
   "response": [
      1258488065
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded
### Write Customer Manufacturing/Factory Programmable Area [CMPA] ###
blhost -t 5000 -p COM7,115200 -j -- write-memory 0x0003E200 "C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin"
{
   "command": "write-memory",
   "response": [
      512
   ],
   "status": {
      "description": "0 (0x0) Success.",
      "value": 0
   }
}
blhost succeeded

### RESULT of the script `Write user configuration to processor`: SUCCESS (return code = [0]SUCCESS)
### RESULT of the script `Write user configuration to processor`: SUCCESS (return code = [0]SUCCESS)
Status of the operation: SUCCESS: Write user configuration to processor
Status of the operation: SUCCESS: Write user configuration to processor


##########################################################################################################
##########################################################################################################
Open workspace - operation started at 2023-11-24 14:47:42
Open workspace - operation started at 2023-11-24 14:47:42
##########################################################################################################
##########################################################################################################
Status of the operation: SUCCESS: Settings loaded successfully; workspace: `C:\Work\Recovery Boot 1-bit SPI Flash`
Status of the operation: SUCCESS: Settings loaded successfully; workspace: `C:\Work\Recovery Boot 1-bit SPI Flash`


##########################################################################################################
##########################################################################################################
Build image - operation started at 2023-11-24 14:47:47
Build image - operation started at 2023-11-24 14:47:47
##########################################################################################################
##########################################################################################################
Build script generated: build_image_lnx.sh
Build script generated: build_image_lnx.sh
Build script generated: build_image_win.bat
Build script generated: build_image_win.bat
Build script generated: build_image_mac.sh
Build script generated: build_image_mac.sh
Executing script "C:\Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat"
Executing script "C:\Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat"
### SCRIPT: Building image: C:\Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat
### SCRIPT: Building image: C:\Work\Recovery Boot 1-bit SPI Flash\build_image_win.bat
### Create bootable image ###
nxpimage mbi export -c "C:\Work\Recovery Boot 1-bit SPI Flash\configs\mbi_config.json"
Success. (Master Boot Image: C:/Work/Recovery Boot 1-bit SPI Flash/bootable_images/lpcxpresso55s36_led_blinky.bin created.)
nxpimage succeeded
### Create CFPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c \"C:\Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.json\" -o \"C:\Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin\"
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (394ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (356ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin

### Create bootable image ###
nxpimage mbi export -c "C:\Work\Recovery Boot 1-bit SPI Flash\configs\mbi_config.json"
Success. (Master Boot Image: C:/Work/Recovery Boot 1-bit SPI Flash/bootable_images/lpcxpresso55s36_led_blinky.bin created.)
nxpimage succeeded
### Create CFPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c \"C:\Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.json\" -o \"C:\Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin\"
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (394ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Work\Recovery Boot 1-bit SPI Flash\configs\cfpa.bin
### Create CMPA page - binary ###
C:\nxp\MCUX_Provi_v8\bin\tools\spsdk\pfr.exe generate-binary -c C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.json -o C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin
WARNING:spsdk.pfr.pfr:The configuration file doesn't contain silicon revision, the latest: '1a' has been used. (356ms since start, pfr.py:379)
Success. (PFR binary has been generated)
Result has been stored in: C:\Work\Recovery Boot 1-bit SPI Flash\configs\cmpa.bin

### RESULT of the script `Building image`: SUCCESS (return code = [0]SUCCESS)
### RESULT of the script `Building image`: SUCCESS (return code = [0]SUCCESS)
Status of the operation: SUCCESS: Building image
Status of the operation: SUCCESS: Building image


##########################################################################################################
##########################################################################################################
Save settings - operation started at 2023-11-24 14:48:36
Save settings - operation started at 2023-11-24 14:48:36
##########################################################################################################
##########################################################################################################
Status of the operation: SUCCESS: Configuration saved to workspace: C:\Work\Recovery Boot 1-bit SPI Flash
Status of the operation: SUCCESS: Configuration saved to workspace: C:\Work\Recovery Boot 1-bit SPI Flash
